# tracer: nop
#
# entries-in-buffer/entries-written: 471/471   #P:8
#
#                                _-----=> irqs-off
#                               / _----=> need-resched
#                              | / _---=> hardirq/softirq
#                              || / _--=> preempt-depth
#                              ||| /     delay
#           TASK-PID     CPU#  ||||   TIMESTAMP  FUNCTION
#              | |         |   ||||      |         |
           <...>-1       [005] ....     0.264926: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] found dsi host node.
           <...>-180     [007] ....     0.295953: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] found dsi host node.
           <...>-180     [007] ....     0.302053: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] found dsi host node.
           <...>-180     [007] ....     0.302062: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] get panel node.
           <...>-180     [007] ....     0.302176: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] init gpio
           <...>-180     [007] ....     0.302239: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] low power mode, pon 365, reset 393.
           <...>-180     [007] ....     0.302430: drm_trace_printf: 4-0058 [drm:anx7625_i2c_probe] probe done
           <...>-190     [001] ....     0.326811: drm_trace_printf: 3-005c [drm:it6505_i2c_probe] using afe_setting: 0           <...>-190     [001] ....     0.327341: drm_trace_printf: 3-005c [drm:it6505_i2c_probe] bound to hdmi-audio-codec           <...>-190     [001] ....     0.329135: drm_trace_printf: 4-0058 [drm:anx7625_bridge_attach] drm attach
           <...>-190     [001] ....     0.329139: drm_trace_printf: 4-0058 [drm:anx7625_bridge_attach] attach dsi
           <...>-190     [001] ....     0.329201: drm_trace_printf: 4-0058 [drm:anx7625_bridge_attach] attach dsi succeeded.
           <...>-316     [001] ....     0.330499: drm_trace_printf: 3-005c [drm:it6505_extcon_work] EXTCON_DISP_DP = 0x00           <...>-316     [001] ....     0.330503: drm_trace_printf: 3-005c [drm:it6505_extcon_work] start to power off           <...>-316     [001] ....     0.330508: drm_trace_printf: 3-005c [drm:it6505_poweroff] power had been already off           <...>-316     [001] ....     0.330513: drm_trace_printf: 3-005c [drm:it6505_extcon_work] power off it6505 success!           <...>-595     [000] ....     1.848682: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [000] ....     1.848698: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] status updated from unknown to connected
           <...>-595     [000] ....     1.849585: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [001] ....     1.890756: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] power on !
           <...>-595     [001] ....     1.893444: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] disable PD feature succeeded.
           <...>-595     [001] ....     1.894379: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] Firmware ver 1300,           <...>-595     [001] ....     1.894384: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] Driver version 0.1.04
           <...>-595     [001] ....     1.917601: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] system status: 0x91. HPD raise up.
           <...>-595     [001] ....     1.922251: drm_trace_printf: 4-0058 [drm:anx7625_start_dp_work] Secure OCM version=00
           <...>-595     [001] ....     1.939768: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid]  EDID Block = 1
           <...>-595     [004] ....     2.077176: drm_trace_printf: 4-0058 [drm:anx7625_power_standby] power down
           <...>-595     [004] ....     2.077196: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077204: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077209: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077213: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077226: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077235: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077238: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077241: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077275: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [004] ....     2.077278: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [004] ....     2.077301: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [004] ....     2.077310: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [004] ....     2.077443: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [004] ....     2.077449: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [004] ....     2.077455: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077458: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077461: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077464: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077472: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077474: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077477: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077480: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077498: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [004] ....     2.077500: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [004] ....     2.077516: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [004] ....     2.077522: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [004] ....     2.077536: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [004] ....     2.077539: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [004] ....     2.077544: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077547: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077550: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077553: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077558: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.077561: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.077567: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.077570: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.077585: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [004] ....     2.077587: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [004] ....     2.077602: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [004] ....     2.077608: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [004] ....     2.080478: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 000000008e2716c9 dma_addr = 0x00000000ff800000 size = 4196352
           <...>-595     [004] ....     2.080517: drm_trace_printf: [drm:drm_mode_addfb2] [FB:63]
           <...>-595     [004] ....     2.082719: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [004] ....     2.082725: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [004] ....     2.082734: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.082738: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.082741: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.082744: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.082754: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [004] ....     2.082757: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [004] ....     2.082759: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [004] ....     2.082762: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [004] ....     2.082787: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [004] ....     2.082790: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [004] ....     2.082807: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [004] ....     2.082815: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [003] ....     2.087841: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000087230f65 dma_addr = 0x00000000ff000000 size = 4196352
           <...>-595     [003] ....     2.087896: drm_trace_printf: [drm:drm_mode_addfb2] [FB:62]
           <...>-595     [006] ....     2.095632: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000097ba6628 dma_addr = 0x00000000fe800000 size = 4196352
           <...>-595     [006] ....     2.095688: drm_trace_printf: [drm:drm_mode_addfb2] [FB:65]
           <...>-595     [005] ....     2.102513: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000a8e7e98a dma_addr = 0x00000000fe000000 size = 4196352
           <...>-595     [005] ....     2.102570: drm_trace_printf: [drm:drm_mode_addfb2] [FB:66]
           <...>-595     [000] ....     2.153108: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [000] ....     2.153129: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [000] ....     2.153149: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [000] ....     2.153161: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [000] ....     2.153169: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [000] ....     2.153175: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [000] ....     2.153198: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [000] ....     2.153204: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [000] ....     2.153209: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [000] ....     2.153214: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [000] ....     2.153275: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [000] ....     2.153279: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [000] ....     2.153309: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [000] ....     2.153322: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [000] ....     2.153367: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [000] ....     2.153372: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [000] ....     2.153380: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [000] ....     2.153386: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [000] ....     2.153391: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [000] ....     2.153396: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [000] ....     2.153406: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [000] ....     2.153412: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [000] ....     2.153417: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [000] ....     2.153422: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [000] ....     2.153445: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [000] ....     2.153449: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [000] ....     2.153474: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [000] ....     2.153483: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [000] ....     2.153596: drm_trace_printf: [drm:drm_mode_setcrtc] [CRTC:54:crtc-0]
           <...>-595     [000] ....     2.153613: drm_trace_printf: [drm:drm_mode_setcrtc] [CONNECTOR:32:eDP-1]
           <...>-595     [000] ....     2.153662: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [000] ....     2.153666: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [000] ....     2.153675: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] drm mode fixup set
           <...>-595     [000] ....     2.153679: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] before mode fixup
           <...>-595     [000] ....     2.153684: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-595     [000] ....     2.153693: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-595     [000] ....     2.153698: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] after mode fixup
           <...>-595     [000] ....     2.153703: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-595     [000] ....     2.153707: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-595     [000] ....     2.153748: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] drm mode set
           <...>-595     [000] ....     2.153752: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] pixelclock(72300).
           <...>-595     [000] ....     2.153757: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] hactive(1366), hsync(32), hfp(40), hbp(88)
           <...>-595     [000] ....     2.153762: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] vactive(768), vsync(5), vfp(5), vbp(12)
           <...>-595     [000] ....     2.153767: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] hdisplay(1366),hsync_start(1406).
           <...>-595     [000] ....     2.153771: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] hsync_end(1438),htotal(1526).
           <...>-595     [000] ....     2.153776: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] vdisplay(768),vsync_start(773).
           <...>-595     [000] ....     2.153780: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_set] vsync_end(778),vtotal(790).
           <...>-595     [000] ....     2.153790: drm_trace_printf: [drm:mtk_drm_crtc_atomic_enable] mtk_drm_crtc_atomic_enable 54
           <...>-595     [000] ....     2.157303: drm_trace_printf: 4-0058 [drm:anx7625_bridge_enable] drm enable
           <...>-595     [005] ....     2.197902: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] power on !
           <...>-595     [005] ....     2.201257: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] disable PD feature succeeded.
           <...>-595     [005] ....     2.202376: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] Firmware ver 1300,           <...>-595     [005] ....     2.202379: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] Driver version 0.1.04
           <...>-595     [005] ....     2.220598: drm_trace_printf: 4-0058 [drm:anx7625_runtime_pm_resume] system status: 0x91. HPD raise up.
           <...>-595     [001] ....     2.226868: drm_trace_printf: 4-0058 [drm:anx7625_start_dp_work] Secure OCM version=00
           <...>-595     [001] ....     2.234797: drm_trace_printf: 4-0058 [drm:anx7625_bridge_enable] config dsi.
           <...>-595     [001] ....     2.239153: drm_trace_printf: 4-0058 [drm:anx7625_bridge_enable] compute M(15794176), N(737280), divider(8).
           <...>-595     [001] ....     2.267484: drm_trace_printf: 4-0058 [drm:anx7625_bridge_enable] success to config DSI
           <...>-595     [001] ....     2.690732: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-595     [001] ....     2.690750: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-595     [001] ....     2.690758: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] status updated from unknown to disconnected
           <...>-595     [001] ....     2.690774: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-595     [001] ....     2.692565: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [001] ....     2.692582: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [001] ....     2.692600: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.692612: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.692620: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.692626: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.692647: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.692652: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.692657: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.692662: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.692709: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [001] ....     2.692713: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [001] ....     2.692742: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [001] ....     2.692754: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [001] ....     2.692856: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [001] ....     2.692861: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [001] ....     2.692869: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.692875: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.692884: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.692889: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.692899: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.692905: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.692910: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.692915: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.692938: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [001] ....     2.692942: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [001] ....     2.692967: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [001] ....     2.692975: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [001] ....     2.722903: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [001] ....     2.722923: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [001] ....     2.722942: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.722954: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.722961: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.722968: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.722991: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.722997: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.723002: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.723007: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.723055: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [001] ....     2.723060: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [001] ....     2.723089: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [001] ....     2.723102: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-595     [001] ....     2.723215: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-595     [001] ....     2.723220: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-595     [001] ....     2.723239: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.723245: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.723250: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.723255: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.723266: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-595     [001] ....     2.723271: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-595     [001] ....     2.723276: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-595     [001] ....     2.723281: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-595     [001] ....     2.723304: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-595     [001] ....     2.723308: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-595     [001] ....     2.723337: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-595     [001] ....     2.723346: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1361    [004] ....     4.403624: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-1361    [004] ....     4.403641: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-1361    [004] ....     4.403654: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1361    [004] ....     4.403662: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1361    [004] ....     4.403668: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1361    [004] ....     4.403672: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1361    [004] ....     4.403687: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1361    [004] ....     4.403690: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1361    [004] ....     4.403692: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1361    [004] ....     4.403695: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1361    [004] ....     4.403730: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-1361    [004] ....     4.403733: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-1361    [004] ....     4.403753: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-1361    [004] ....     4.403762: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1361    [004] ....     4.403811: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-1361    [004] ....     4.403820: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-1361    [004] ....     4.403826: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-1507    [005] ....     5.192213: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-1507    [005] ....     5.192243: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-1507    [005] ....     5.192259: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [005] ....     5.192267: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [005] ....     5.192272: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [005] ....     5.192276: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [005] ....     5.192292: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [005] ....     5.192295: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [005] ....     5.192298: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [005] ....     5.192301: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [005] ....     5.192336: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-1507    [005] ....     5.192339: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-1507    [005] ....     5.192360: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-1507    [005] ....     5.192369: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1507    [005] ....     5.192400: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-1507    [005] ....     5.192406: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-1507    [005] ....     5.192411: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-1507    [005] ....     5.192447: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-1507    [005] ....     5.192450: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-1507    [005] ....     5.192456: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [005] ....     5.192459: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [005] ....     5.192462: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [005] ....     5.192465: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [005] ....     5.192472: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [005] ....     5.192475: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [005] ....     5.192478: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [005] ....     5.192481: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [005] ....     5.192498: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-1507    [005] ....     5.192500: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-1507    [005] ....     5.192516: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-1507    [005] ....     5.192525: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1507    [005] ....     5.192656: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-1507    [005] ....     5.192660: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-1507    [005] ....     5.192664: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-1507    [007] ....     6.408611: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-1507    [007] ....     6.408631: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-1507    [007] ....     6.408648: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [007] ....     6.408657: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [007] ....     6.408662: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [007] ....     6.408667: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [007] ....     6.408688: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [007] ....     6.408691: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [007] ....     6.408694: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [007] ....     6.408697: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [007] ....     6.408734: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-1507    [007] ....     6.408737: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-1507    [007] ....     6.408757: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-1507    [007] ....     6.408767: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1507    [007] ....     6.408897: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-1507    [007] ....     6.408903: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-1507    [007] ....     6.408908: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-1507    [007] ....     6.408997: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1]
           <...>-1507    [007] ....     6.409001: drm_trace_printf: 4-0058 [drm:anx7625_bridge_get_edid] drm bridge get edid
           <...>-1507    [007] ....     6.409009: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [007] ....     6.409014: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [007] ....     6.409017: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [007] ....     6.409020: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [007] ....     6.409027: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Supported Monitor Refresh rate range is 0 Hz - 0 Hz
           <...>-1507    [007] ....     6.409031: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] Assigning EDID-1.4 digital sink color depth as 6 bpc.
           <...>-1507    [007] ....     6.409034: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD monitor 
           <...>-1507    [007] ....     6.409037: drm_trace_printf: mediatek-drm.3.auto [drm:update_display_info] [CONNECTOR:32:eDP-1] ELD size 20, SAD count 0
           <...>-1507    [007] ....     6.409057: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode checking
           <...>-1507    [007] ....     6.409059: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_valid] drm mode valid.
           <...>-1507    [007] ....     6.409075: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:32:eDP-1] probed modes :
           <...>-1507    [007] ....     6.409082: drm_trace_printf: [drm:drm_mode_debug_printmodeline] Modeline "1366x768": 60 72300 1366 1406 1438 1526 768 773 778 790 0x48 0xa
           <...>-1507    [007] ....     6.409115: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1]
           <...>-1507    [007] ....     6.409119: drm_trace_printf: 3-005c [drm:it6505_bridge_detect] it6505->sink_count:0 powered:0           <...>-1507    [007] ....     6.409138: drm_trace_printf: [drm:drm_helper_probe_single_connector_modes] [CONNECTOR:35:DP-1] disconnected
           <...>-1507    [007] ....     6.415936: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000f2fd03f6 dma_addr = 0x00000000fdffc000 size = 16384
           <...>-1507    [007] ....     6.416090: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000f7814b31 dma_addr = 0x00000000fdff8000 size = 16384
           <...>-1507    [006] ....     6.885492: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000735cc124 dma_addr = 0x00000000fd800000 size = 4227072
           <...>-1507    [006] ....     6.885685: drm_trace_printf: [drm:drm_mode_addfb2] [FB:64]
           <...>-1507    [006] ....     6.885905: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] drm mode fixup set
           <...>-1507    [006] ....     6.885909: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] before mode fixup
           <...>-1507    [006] ....     6.885913: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-1507    [006] ....     6.885916: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-1507    [006] ....     6.885920: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] after mode fixup
           <...>-1507    [006] ....     6.885923: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-1507    [006] ....     6.885925: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-1507    [007] ....     7.008605: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000e0f83c99 dma_addr = 0x00000000fc800000 size = 4227072
           <...>-1507    [007] ....     7.008795: drm_trace_printf: [drm:drm_mode_addfb2] [FB:64]
           <...>-1507    [007] ....     7.061175: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000e0f83c99 dma_addr = 0x00000000fc800000 size = 4227072
           <...>-1507    [007] ....     7.061372: drm_trace_printf: [drm:drm_mode_addfb2] [FB:64]
           <...>-2312    [001] ....     7.111696: drm_trace_printf: mediatek-drm.3.auto [drm:drm_mode_getconnector] User-space requested a forced probe on [CONNECTOR:32:eDP-1] but is not the DRM master, demoting to read-only probe           <...>-2312    [001] ....     7.111754: drm_trace_printf: mediatek-drm.3.auto [drm:drm_mode_getconnector] User-space requested a forced probe on [CONNECTOR:35:DP-1] but is not the DRM master, demoting to read-only probe           <...>-1507    [002] ....     7.263656: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] drm mode fixup set
           <...>-1507    [002] ....     7.263665: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] before mode fixup
           <...>-1507    [002] ....     7.263674: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-1507    [002] ....     7.263679: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-1507    [002] ....     7.263684: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] after mode fixup
           <...>-1507    [002] ....     7.263689: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync(32), hfp(40), hbp(88), clock(72300)
           <...>-1507    [002] ....     7.263694: drm_trace_printf: 4-0058 [drm:anx7625_bridge_mode_fixup] hsync_start(1406), hsync_end(1438), htot(1526)
           <...>-1507    [006] ....     8.279819: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000cac196af dma_addr = 0x00000000fc000000 size = 4227072
           <...>-1507    [006] ....     8.279981: drm_trace_printf: [drm:drm_mode_addfb2] [FB:67]
           <...>-1507    [006] ....     8.279987: drm_trace_printf: [drm:drm_mode_addfb2] [FB:71]
           <...>-1507    [006] ....     8.281668: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000049bb197d dma_addr = 0x00000000fb800000 size = 4227072
           <...>-1507    [006] ....     8.281838: drm_trace_printf: [drm:drm_mode_addfb2] [FB:72]
           <...>-1507    [006] ....     8.281844: drm_trace_printf: [drm:drm_mode_addfb2] [FB:73]
           <...>-1507    [006] ....     8.283466: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000023960d87 dma_addr = 0x00000000fb000000 size = 4227072
           <...>-1507    [006] ....     8.283585: drm_trace_printf: [drm:drm_mode_addfb2] [FB:74]
           <...>-1507    [006] ....     8.283592: drm_trace_printf: [drm:drm_mode_addfb2] [FB:75]
           <...>-1507    [006] ....     8.521747: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000fb5abc06 dma_addr = 0x00000000fc800000 size = 4227072
           <...>-1507    [006] ....     8.522153: drm_trace_printf: [drm:drm_mode_addfb2] [FB:64]
           <...>-1507    [006] ....     8.522163: drm_trace_printf: [drm:drm_mode_addfb2] [FB:67]
           <...>-1507    [006] ....     8.532982: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 00000000cac196af dma_addr = 0x00000000fc000000 size = 4227072
           <...>-1507    [006] ....     8.533261: drm_trace_printf: [drm:drm_mode_addfb2] [FB:71]
           <...>-1507    [006] ....     8.533435: drm_trace_printf: [drm:drm_mode_addfb2] [FB:74]
           <...>-1507    [006] ....     8.541646: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000023960d87 dma_addr = 0x00000000fb000000 size = 4227072
           <...>-1507    [006] ....     8.541791: drm_trace_printf: [drm:drm_mode_addfb2] [FB:75]
           <...>-1507    [006] ....     8.541798: drm_trace_printf: [drm:drm_mode_addfb2] [FB:76]
           <...>-3369    [004] ....     9.333547: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.334402: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.335243: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [007] ....     9.336097: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.336966: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.337819: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.338665: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.339456: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [007] ....     9.340300: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.341136: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.341982: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.342833: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.343683: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.344460: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.345393: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.346251: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.347102: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.347954: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.348803: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.349652: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.350462: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.351305: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.352134: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.352957: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.353799: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.354646: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.355464: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.356304: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.357133: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.357959: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.358785: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.359607: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....     9.359624: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_access] DP-AUX: Too many retries, giving up. First error: -5
           <...>-3369    [004] ....     9.359628: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_probe] DP-AUX: 0x00000 AUX -> (ret= -5)
           <...>-1507    [004] ....    11.198666: drm_trace_printf: [drm:mtk_drm_gem_create] cookie = 0000000034f6b6f8 dma_addr = 0x00000000fbff8000 size = 30720
           <...>-3369    [004] ....    15.010315: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....    15.011224: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [004] ....    15.012322: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [002] ....    15.013477: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [002] ....    15.014561: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.015679: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.016672: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.017503: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.018387: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.019268: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.020139: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.021011: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.021880: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.022750: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.023638: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.024520: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.025404: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.026286: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.027168: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.028051: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.028934: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.029815: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.030695: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.031511: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.032397: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.033281: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.034165: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.035047: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.035929: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.036813: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.037696: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.038512: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [001] ....    15.038543: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_access] DP-AUX: Too many retries, giving up. First error: -5
           <...>-3369    [001] ....    15.038554: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_probe] DP-AUX: 0x00000 AUX -> (ret= -5)
           <...>-3369    [003] ....    66.009976: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.011363: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.013349: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.014559: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.015551: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.016556: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.017558: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.018556: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.019857: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.020944: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.021951: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.023007: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.023903: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.024795: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.025749: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.026747: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.027795: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.028748: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.029746: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.030747: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.031747: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.032758: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.033804: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.034745: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.035752: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.036764: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.037757: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.038763: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.039899: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.040749: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.041618: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.042600: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [003] ....    66.042620: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_access] DP-AUX: Too many retries, giving up. First error: -5
           <...>-3369    [003] ....    66.042627: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_probe] DP-AUX: 0x00000 AUX -> (ret= -5)
           <...>-3369    [000] ....    72.008956: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [000] ....    72.009850: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [000] ....    72.010710: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [000] ....    72.011568: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [000] ....    72.012425: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [000] ....    72.013284: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [005] ....    72.014144: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [005] ....    72.014985: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [005] ....    72.015814: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [005] ....    72.016640: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.017454: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.018275: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.019094: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.019908: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.020721: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.021436: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.022247: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.023058: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.023869: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.024680: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.025434: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.026245: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.027055: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.027868: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.028680: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.029435: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.030248: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.031084: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.031906: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.032741: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.033577: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.034397: drm_trace_printf: 3-005c [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6           <...>-3369    [006] ....    72.034412: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_access] DP-AUX: Too many retries, giving up. First error: -5
           <...>-3369    [006] ....    72.034415: drm_trace_printf: mediatek-drm.3.auto [drm:drm_dp_dpcd_probe] DP-AUX: 0x00000 AUX -> (ret= -5)
