/sys/fs/pstore/console-ramoops-0:
[    0.000000] Booting Linux on physical CPU 0x0000000000 [0x410fd034]
[    0.000000] Linux version 5.10.230-25844-gdc65f732bf53 (cros-kernel@chromium.org) (Chromium OS 19.0_pre530567 clang version 19.0.0git (/mnt/host/source/src/third_party/llvm-project 3b5e7c83a6e226d5bd7ed2e9b67449b64812074c), LLD 19.0.0) #1 SMP PREEMPT Thu, 2 Jan 2025 01:16:47 -0800
[    0.000000] random: crng init done
[    0.000000] Machine model: Google kenzo sku17 board
[    0.000000] Reserved memory: created DMA memory pool at 0x0000000050000000, size 41 MiB
[    0.000000] OF: reserved mem: initialized node memory@50000000, compatible id shared-dma-pool
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000040000000-0x00000000ffffffff]
[    0.000000]   DMA32    empty
[    0.000000]   Normal   [mem 0x0000000100000000-0x000000013fffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000040000000-0x000000004fffffff]
[    0.000000]   node   0: [mem 0x0000000050000000-0x00000000528fffff]
[    0.000000]   node   0: [mem 0x0000000052900000-0x00000000545fffff]
[    0.000000]   node   0: [mem 0x0000000054700000-0x00000000ffdfffff]
[    0.000000]   node   0: [mem 0x0000000100000000-0x000000013fffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000013fffffff]
[    0.000000] On node 0, zone DMA: 256 pages in unavailable ranges
[    0.000000] On node 0, zone Normal: 512 pages in unavailable ranges
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.2
[    0.000000] percpu: Embedded 32 pages/cpu s93592 r8192 d29288 u131072
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: detected: ARM erratum 845719
[    0.000000] CPU features: detected: GIC system register CPU interface
[    0.000000] CPU features: kernel page table isolation forced ON by KASLR
[    0.000000] CPU features: detected: Kernel page table isolation (KPTI)
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031424
[    0.000000] Kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes, linear)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes, linear)
[    0.000000] mem auto-init: stack:all(zero), heap alloc:on, heap free:off
[    0.000000] software IO TLB: mapped [mem 0x00000000fbe00000-0x00000000ffe00000] (64MB)
[    0.000000] Memory: 3971572K/4191232K available (13758K kernel code, 2436K rwdata, 9280K rodata, 1408K init, 1075K bss, 219660K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=8, Nodes=1
[    0.000000] ftrace: allocating 40629 entries in 159 pages
[    0.000000] ftrace: allocated 159 pages with 6 groups
[    0.000000] rcu: Preemptible hierarchical RCU implementation.
[    0.000000] 	Trampoline variant of Tasks RCU enabled.
[    0.000000] 	Rude variant of Tasks RCU enabled.
[    0.000000] 	Tracing variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 100 jiffies.
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] GIC: enabling workaround for GICv3: Mediatek Chromebook GICR save problem
[    0.000000] GICv3: GIC: Using split EOI/Deactivate mode
[    0.000000] GICv3: 640 SPIs implemented
[    0.000000] GICv3: 0 Extended SPIs implemented
[    0.000000] GICv3: Distributor has no Range Selector support
[    0.000000] GICv3: 16 PPIs implemented
[    0.000000] GICv3: CPU0: found redistributor 0 region 0:0x000000000c100000
[    0.000000] GICv3: GIC: PPI partition interrupt-partition-0[0] { /cpus/cpu@0[0] /cpus/cpu@1[1] /cpus/cpu@2[2] /cpus/cpu@3[3] }
[    0.000000] GICv3: GIC: PPI partition interrupt-partition-1[1] { /cpus/cpu@100[4] /cpus/cpu@101[5] /cpus/cpu@102[6] /cpus/cpu@103[7] }
[    0.000000] rcu: 	Offload RCU callbacks from CPUs: 0-7.
[    0.000000] kfence: initialized - using 2097152 bytes for 255 objects at 0x(____ptrval____)-0x(____ptrval____)
[    0.000000] arch_timer: cp15 timer(s) running at 13.00MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x2ff89eacb, max_idle_ns: 440795202429 ns
[    0.000002] sched_clock: 56 bits at 13MHz, resolution 76ns, wraps every 4398046511101ns
[    0.000353] Calibrating delay loop (skipped), value calculated using timer frequency.. 26.00 BogoMIPS (lpj=13000)
[    0.000360] pid_max: default: 32768 minimum: 301
[    0.000443] LSM: Security Framework initializing
[    0.000476] landlock: Up and running.
[    0.000479] Yama: becoming mindful.
[    0.000489] LoadPin: ready to pin (currently enforcing)
[    0.000505] Chromium OS LSM: enabled
[    0.000508] SELinux:  Initializing.
[    0.000553] LSM support for eBPF active
[    0.000588] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.000602] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.001967] rcu: Hierarchical SRCU implementation.
[    0.002634] smp: Bringing up secondary CPUs ...
[    0.003198] Detected VIPT I-cache on CPU1
[    0.003222] GICv3: CPU1: found redistributor 1 region 0:0x000000000c120000
[    0.003251] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
[    0.003873] Detected VIPT I-cache on CPU2
[    0.003883] GICv3: CPU2: found redistributor 2 region 0:0x000000000c140000
[    0.003895] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
[    0.004471] Detected VIPT I-cache on CPU3
[    0.004480] GICv3: CPU3: found redistributor 3 region 0:0x000000000c160000
[    0.004492] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
[    0.005179] CPU features: detected: ARM erratum 858921
[    0.005186] CPU features: detected: Spectre-v2
[    0.005192] CPU features: detected: Spectre-BHB
[    0.005196] Detected VIPT I-cache on CPU4
[    0.005211] GICv3: CPU4: found redistributor 100 region 0:0x000000000c180000
[    0.005218] arch_timer: Enabling local workaround for ARM erratum 858921
[    0.005226] arch_timer: CPU4: Trapping CNTVCT access
[    0.005235] CPU4: Booted secondary processor 0x0000000100 [0x410fd092]
[    0.005779] Detected VIPT I-cache on CPU5
[    0.005791] GICv3: CPU5: found redistributor 101 region 0:0x000000000c1a0000
[    0.005796] arch_timer: Enabling local workaround for ARM erratum 858921
[    0.005801] arch_timer: CPU5: Trapping CNTVCT access
[    0.005808] CPU5: Booted secondary processor 0x0000000101 [0x410fd092]
[    0.006379] Detected VIPT I-cache on CPU6
[    0.006391] GICv3: CPU6: found redistributor 102 region 0:0x000000000c1c0000
[    0.006397] arch_timer: Enabling local workaround for ARM erratum 858921
[    0.006402] arch_timer: CPU6: Trapping CNTVCT access
[    0.006408] CPU6: Booted secondary processor 0x0000000102 [0x410fd092]
[    0.006979] Detected VIPT I-cache on CPU7
[    0.006991] GICv3: CPU7: found redistributor 103 region 0:0x000000000c1e0000
[    0.006996] arch_timer: Enabling local workaround for ARM erratum 858921
[    0.007001] arch_timer: CPU7: Trapping CNTVCT access
[    0.007008] CPU7: Booted secondary processor 0x0000000103 [0x410fd092]
[    0.007080] smp: Brought up 1 node, 8 CPUs
[    0.007118] SMP: Total of 8 processors activated.
[    0.007122] CPU features: detected: 32-bit EL0 Support
[    0.007126] CPU features: detected: CRC32 instructions
[    0.007129] CPU features: detected: 32-bit EL1 Support
[    0.007262] CPU features: emulated: Privileged Access Never (PAN) using TTBR0_EL1 switching
[    0.020637] CPU: All CPU(s) started at EL2
[    0.020668] alternatives: patching kernel code
[    0.021873] devtmpfs: initialized
[    0.029592] KASLR enabled
[    0.029719] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
[    0.029746] futex hash table entries: 2048 (order: 5, 131072 bytes, linear)
[    0.029960] pinctrl core: initialized pinctrl subsystem
[    0.030420] NET: Registered protocol family 16
[    0.031141] DMA: preallocated 512 KiB GFP_KERNEL pool for atomic allocations
[    0.031351] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
[    0.031554] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
[    0.031602] audit: initializing netlink subsys (disabled)
[    0.031774] audit: type=2000 audit(0.031:1): state=initialized audit_enabled=0 res=1
[    0.031978] thermal_sys: Registered thermal governor 'step_wise'
[    0.031981] thermal_sys: Registered thermal governor 'user_space'
[    0.031985] thermal_sys: Registered thermal governor 'power_allocator'
[    0.032450] thermal thermal_zone7: power_allocator: sustainable_power will be estimated
[    0.032488] thermal thermal_zone8: power_allocator: sustainable_power will be estimated
[    0.032582] cpuidle: using governor ladder
[    0.032693] cpuidle: using governor menu
[    0.032707] cpuidle: using governor teo
[    0.032883] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.032987] ASID allocator initialised with 32768 entries
[    0.034465] printk: console [ramoops-1] enabled
[    0.034583] pstore: Registered ramoops as persistent store backend
[    0.034589] ramoops: using 0x100000@0xffedb000, ecc: 0
[    0.100524] cryptd: max_cpu_qlen set to 1000
[    0.103076] pp1200_mipibrdg: supplied by pp1800_alw
[    0.103400] pp1800_mipibrdg: supplied by pp1800_alw
[    0.103640] pp3300_panel: supplied by pp3300_alw
[    0.103881] vddio_mipibrdg: supplied by pp3300_alw
[    0.104265] iommu: Default domain type: Translated 
[    0.104376] vgaarb: loaded
[    0.104645] SCSI subsystem initialized
[    0.104733] usbcore: registered new interface driver usbfs
[    0.104755] usbcore: registered new interface driver hub
[    0.104776] usbcore: registered new device driver usb
[    0.104807] mc: Linux media interface: v0.10
[    0.104821] videodev: Linux video capture interface: v2.00
[    0.106268] Advanced Linux Sound Architecture Driver Initialized.
[    0.106923] clocksource: Switched to clocksource arch_sys_counter
[    0.126145] VFS: Disk quotas dquot_6.6.0
[    0.126195] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.126823] NET: Registered protocol family 2
[    0.126954] IP idents hash table entries: 65536 (order: 7, 524288 bytes, linear)
[    0.128776] tcp_listen_portaddr_hash hash table entries: 2048 (order: 3, 32768 bytes, linear)
[    0.128879] TCP established hash table entries: 32768 (order: 6, 262144 bytes, linear)
[    0.129072] TCP bind hash table entries: 32768 (order: 7, 524288 bytes, linear)
[    0.129325] TCP: Hash tables configured (established 32768 bind 32768)
[    0.129421] UDP hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.129492] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.129647] NET: Registered protocol family 1
[    0.129668] PCI: CLS 0 bytes, default 64
[    0.130471] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
[    0.130658] hw perfevents: enabled with armv8_cortex_a73 PMU driver, 7 counters available
[    0.131084] kvm [1]: IPA Size Limit: 40 bits
[    0.131772] kvm [1]: vgic-v2@c420000
[    0.131789] kvm [1]: GIC system register CPU interface enabled
[    0.131904] kvm [1]: vgic interrupt IRQ18
[    0.132043] kvm [1]: Hyp mode initialized successfully
[    0.135497] Initialise system trusted keyrings
[    0.135593] workingset: timestamp_bits=62 max_order=20 bucket_order=0
[    0.138551] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.138762] Registering esdfs 0.2
[    0.138904] alt_syscall: table 'read_write_test' available.
[    0.138940] alt_syscall: table 'android' available.
[    0.138962] alt_syscall: table 'android_permissive' available.
[    0.138986] alt_syscall: table 'third_party' available.
[    0.139004] alt_syscall: table 'third_party_permissive' available.
[    0.139021] alt_syscall: table 'complete' available.
[    0.139037] alt_syscall: table 'complete_permissive' available.
[    0.165444] Key type asymmetric registered
[    0.165453] Asymmetric key parser 'x509' registered
[    0.165483] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 246)
[    0.165556] io scheduler mq-deadline registered
[    0.165562] io scheduler kyber registered
[    0.165618] io scheduler bfq registered
[    0.167959] of_fixed_factor_clk: probe of fixed-factor-clock-13m failed with error -17
[    0.178548] mtk-socinfo mtk-socinfo.0.auto: error -ENOENT: Failed to get socinfo data
[    0.178562] mtk-socinfo: probe of mtk-socinfo.0.auto failed with error -2
[    0.178623] mtk-socinfo mtk-socinfo.1.auto: SoC detected, family: MediaTek, soc_id: MT8183, machine: Kompanio 500
[    0.179271] Serial: 8250/16550 driver, 4 ports, IRQ sharing disabled
[    0.200492] 11002000.serial: ttyS0 at MMIO 0x11002000 (irq = 33, base_baud = 1625000) is a ST16650V2
[    0.221259] 11003000.serial: ttyS1 at MMIO 0x11003000 (irq = 34, base_baud = 1625000) is a ST16650V2
[    0.221367] serial serial0: tty port ttyS1 registered
[    0.225880] usbcore: registered new interface driver udl
[    0.228537] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14008000
[    0.228571] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14009000
[    0.228598] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@1400a000
[    0.228625] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400b000
[    0.228652] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400c000
[    0.228686] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/color@1400e000
[    0.228713] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ccorr@1400f000
[    0.228739] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/aal@14010000
[    0.228766] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/gamma@14011000
[    0.228841] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dsi@14014000
[    0.228869] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dpi@14015000
[    0.232649] mali 13040000.mali: Kernel DDK version r44p1-01eac0
[    0.232664] mali 13040000.mali: IRQ JOB not found
[    0.232709] mali 13040000.mali: IRQ MMU not found
[    0.232720] mali 13040000.mali: IRQ GPU not found
[    0.232745] mali 13040000.mali: GPU metrics tracepoint support enabled
[    0.232862] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.235216] loop: module loaded
[    0.235391] lkdtm: No crash points registered, enable through debugfs
[    0.244142] vsim1: Bringing 1800000uV into 2700000-2700000uV
[    0.255865] spi-nor spi1.0: found w25q64jwm, expected w25q64dw
[    0.256386] spi-nor spi1.0: w25q64jwm (8192 Kbytes)
[    0.258385] PPP generic driver version 2.4.2
[    0.258488] PPP MPPE Compression module registered
[    0.259172] mtu3 11201000.usb: uwk - reg:0x420, version:101
[    0.259217] mtu3 11201000.usb: supply vbus not found, using dummy regulator
[    0.259276] mtu3 11201000.usb: dr_mode: 1, is_u3_dr: 0, u3p_dis_msk: 0, drd: auto
[    0.259970] mtu3 11201000.usb: xHCI platform device register success...
[    0.260220] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    0.260227] ehci-pci: EHCI PCI platform driver
[    0.260263] ehci-platform: EHCI generic platform driver
[    0.260407] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    0.260419] ohci-pci: OHCI PCI platform driver
[    0.260438] ohci-platform: OHCI generic platform driver
[    0.261025] xhci-mtk 11200000.xhci: supply vbus not found, using dummy regulator
[    0.261284] xhci-mtk 11200000.xhci: xHCI Host Controller
[    0.261361] tpm_tis_spi spi0.0: TPM ready IRQ confirmed on attempt 2
[    0.261375] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 1
[    0.261452] xhci-mtk 11200000.xhci: hcc params 0x01400f99 hci version 0x110 quirks 0x0000000000210010
[    0.261488] xhci-mtk 11200000.xhci: irq 290, io mem 0x11200000
[    0.261567] xhci-mtk 11200000.xhci: xHCI Host Controller
[    0.261637] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 2
[    0.261647] xhci-mtk 11200000.xhci: Host supports USB 3.0 SuperSpeed
[    0.261731] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.10
[    0.261738] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.261744] usb usb1: Product: xHCI Host Controller
[    0.261750] usb usb1: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
[    0.261755] usb usb1: SerialNumber: 11200000.xhci
[    0.262006] hub 1-0:1.0: USB hub found
[    0.262028] hub 1-0:1.0: 1 port detected
[    0.262208] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
[    0.262259] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.10
[    0.262266] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.262272] usb usb2: Product: xHCI Host Controller
[    0.262277] usb usb2: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
[    0.262282] usb usb2: SerialNumber: 11200000.xhci
[    0.262471] hub 2-0:1.0: USB hub found
[    0.262492] hub 2-0:1.0: config failed, hub doesn't have any ports! (err -19)
[    0.262722] usbcore: registered new interface driver cdc_acm
[    0.262728] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
[    0.262760] usbcore: registered new interface driver usb-storage
[    0.263929] mt6397-rtc mt6358-rtc: registered as rtc0
[    0.264101] mt6397-rtc mt6358-rtc: setting system clock to 2025-02-28T18:52:53 UTC (1740768773)
[    0.264135] i2c /dev entries driver
[    0.267517] elan_i2c 2-0015: supply vcc not found, using dummy regulator
[    0.270598] tpm_tis_spi spi0.0: 2.0 TPM (device-id 0x28, rev-id 0)
[    0.271154] mtk-wdt 10007000.watchdog: Watchdog enabled (timeout=31 sec, nowayout=0)
[    0.271507] device-mapper: ioctl: 4.43.0-ioctl (2020-10-01) initialised: dm-devel@redhat.com
[    0.271611] device-mapper: verity-chromeos: dm-verity-chromeos registered
[    0.271952] cpu cpu0: dummy supplies not allowed for exclusive requests
[    0.272734] cpu cpu4: dummy supplies not allowed for exclusive requests
[    0.273584] cpu cpu0: EM: created perf domain
[    0.273928] cpu cpu4: EM: created perf domain
[    0.274279] cpufreq: cpufreq_online: CPU4: Running at unlisted initial frequency: 1199999 KHz, changing to: 1248000 KHz
[    0.275613] sdhci: Secure Digital Host Controller Interface driver
[    0.275617] sdhci: Copyright(c) Pierre Ossman
[    0.275866] sdhci-pltfm: SDHCI platform and OF driver helper
[    0.276354] mtk-msdc 11240000.mmc: allocated mmc-pwrseq
[    0.276650] SMCCC: SOC_ID: ARCH_SOC_ID(0) returned error: ffffffffffffffff
[    0.276672] hid: raw HID events driver (C) Jiri Kosina
[    0.276874] usbcore: registered new interface driver usbhid
[    0.276878] usbhid: USB HID core driver
[    0.277107] i2c_hid_of 0-0040: supply vdd not found, using dummy regulator
[    0.277172] i2c_hid_of 0-0040: supply vddl not found, using dummy regulator
[    0.277470] ashmem: initialized
[    0.277574] i2c_hid_of 2-002c: supply vdd not found, using dummy regulator
[    0.277604] spi_master spi2: will run message pump with realtime priority
[    0.277632] i2c_hid_of 2-002c: supply vddl not found, using dummy regulator
[    0.282500] GACT probability NOT on
[    0.282930] xt_time: kernel timezone is -0000
[    0.283123] Initializing XFRM netlink socket
[    0.283310] NET: Registered protocol family 10
[    0.283683] Segment Routing with IPv6
[    0.283811] NET: Registered protocol family 17
[    0.283822] NET: Registered protocol family 15
[    0.283901] NET: Registered protocol family 40
[    0.284138] registered taskstats version 1
[    0.284145] Loading compiled-in X.509 certificates
[    0.284231] Key type .fscrypt registered
[    0.284235] Key type fscrypt-provisioning registered
[    0.284439] pstore: Using crash dump compression: deflate
[    0.285080] Key type encrypted registered
[    0.298402] mali 13040000.mali: Kernel DDK version r44p1-01eac0
[    0.298420] mali 13040000.mali: IRQ JOB not found
[    0.298440] mali 13040000.mali: IRQ MMU not found
[    0.298451] mali 13040000.mali: IRQ GPU not found
[    0.298474] mali 13040000.mali: GPU metrics tracepoint support enabled
[    0.302543] mtk-iommu 10205000.iommu: bound 14017000.larb (ops 0xffffffda1f2c6448)
[    0.302556] mtk-iommu 10205000.iommu: bound 16010000.larb (ops 0xffffffda1f2c6448)
[    0.302562] mtk-iommu 10205000.iommu: bound 1502f000.larb (ops 0xffffffda1f2c6448)
[    0.302567] mtk-iommu 10205000.iommu: bound 1a002000.larb (ops 0xffffffda1f2c6448)
[    0.302572] mtk-iommu 10205000.iommu: bound 17010000.larb (ops 0xffffffda1f2c6448)
[    0.302577] mtk-iommu 10205000.iommu: bound 15021000.larb (ops 0xffffffda1f2c6448)
[    0.302582] mtk-iommu 10205000.iommu: bound 1a001000.larb (ops 0xffffffda1f2c6448)
[    0.302711] mediatek-disp-ovl 14008000.ovl: Adding to iommu group 0
[    0.303133] mediatek-disp-ovl 14009000.ovl: Adding to iommu group 0
[    0.303318] mediatek-disp-ovl 1400a000.ovl: Adding to iommu group 0
[    0.303491] mediatek-disp-rdma 1400b000.rdma: Adding to iommu group 0
[    0.303655] mediatek-disp-rdma 1400c000.rdma: Adding to iommu group 0
[    0.306025] mali 13040000.mali: Kernel DDK version r44p1-01eac0
[    0.306043] mali 13040000.mali: IRQ JOB not found
[    0.306062] mali 13040000.mali: IRQ MMU not found
[    0.306073] mali 13040000.mali: IRQ GPU not found
[    0.306105] mali 13040000.mali: GPU metrics tracepoint support enabled
[    0.308631] cros-ec-pchg cros-ec-pchg.15.auto: Unable to get number or ports (err:-95)
[    0.308643] cros-ec-pchg cros-ec-pchg.15.auto: No peripheral charge ports (err:-95)
[    0.309095] mali 13040000.mali: GPU identified as 0x1 arch 6.2.2 r0p3 status 0
[    0.309587] mali 13040000.mali: No priority control manager is configured
[    0.309842] mali 13040000.mali: No memory group manager is configured
[    0.310579] input: wifi-wakeup as /devices/platform/wifi-wakeup/input/input0
[    0.311001] input: volume-buttons as /devices/platform/volume-buttons/input/input1
[    0.311157] device-mapper: init: waiting for all devices to be available before creating mapped devices
[    0.311164] mali 13040000.mali: Using configured power model mali-g72-power-model, and fallback mali-simple-power-model
[    0.311173] mali 13040000.mali: No volt-bin detected, using default OPP table
[    0.311186] mali 13040000.mali: OPP 0 : opp_freq=300000000 core_mask=f
[    0.311191] mali 13040000.mali: OPP 1 : opp_freq=320000000 core_mask=f
[    0.311197] mali 13040000.mali: OPP 2 : opp_freq=340000000 core_mask=f
[    0.311202] mali 13040000.mali: OPP 3 : opp_freq=360000000 core_mask=f
[    0.311207] mali 13040000.mali: OPP 4 : opp_freq=380000000 core_mask=f
[    0.311212] mali 13040000.mali: OPP 5 : opp_freq=400000000 core_mask=f
[    0.311217] mali 13040000.mali: OPP 6 : opp_freq=420000000 core_mask=f
[    0.311222] mali 13040000.mali: OPP 7 : opp_freq=460000000 core_mask=f
[    0.311227] mali 13040000.mali: OPP 8 : opp_freq=500000000 core_mask=f
[    0.311231] mali 13040000.mali: OPP 9 : opp_freq=540000000 core_mask=f
[    0.311236] mali 13040000.mali: OPP 10 : opp_freq=580000000 core_mask=f
[    0.311240] mali 13040000.mali: OPP 11 : opp_freq=620000000 core_mask=f
[    0.311245] mali 13040000.mali: OPP 12 : opp_freq=653000000 core_mask=f
[    0.311249] mali 13040000.mali: OPP 13 : opp_freq=698000000 core_mask=f
[    0.311253] mali 13040000.mali: OPP 14 : opp_freq=743000000 core_mask=f
[    0.311257] mali 13040000.mali: OPP 15 : opp_freq=800000000 core_mask=f
[    0.311740] mali 13040000.mali: Probed as mali0
[    0.312207] thermal thermal_zone9: power_allocator: sustainable_power will be estimated
[    0.312329] sbs-battery 12-000b: sbs-battery: battery gas gauge device registered
[    0.314923] mtk-svs 1100b000.svs: M_HW_RES0: 0x00120090
[    0.314930] mtk-svs 1100b000.svs: M_HW_RES1: 0xe7fcbb1b
[    0.314934] mtk-svs 1100b000.svs: M_HW_RES2: 0x478b47c7
[    0.314937] mtk-svs 1100b000.svs: M_HW_RES3: 0xabfbf757
[    0.314941] mtk-svs 1100b000.svs: M_HW_RES4: 0xe6fca5ed
[    0.314944] mtk-svs 1100b000.svs: M_HW_RES5: 0x47bb4bc0
[    0.314947] mtk-svs 1100b000.svs: M_HW_RES6: 0xe6fcc7e6
[    0.314951] mtk-svs 1100b000.svs: M_HW_RES7: 0xe7fc980f
[    0.314954] mtk-svs 1100b000.svs: M_HW_RES8: 0x4bbb4bef
[    0.314957] mtk-svs 1100b000.svs: M_HW_RES9: 0xabfb366c
[    0.314960] mtk-svs 1100b000.svs: M_HW_RES14: 0x9e862dbb
[    0.314963] mtk-svs 1100b000.svs: M_HW_RES15: 0x015a0010
[    0.314966] mtk-svs 1100b000.svs: M_HW_RES16: 0xe7fc8e1c
[    0.314970] mtk-svs 1100b000.svs: M_HW_RES17: 0x47bb47ef
[    0.314973] mtk-svs 1100b000.svs: M_HW_RES18: 0xabfbc84d
[    0.317096] devfreq 13040000.mali: Couldn't update frequency transition information.
[    0.317830]  SVSB_CPU_LITTLE: svs_init01_isr_handler: VDN74~30:0x141c242b~0x2f33373d, DC:0x031601c6
[    0.318102]  SVSB_CPU_BIG: svs_init01_isr_handler: VDN74~30:0x151e262d~0x32373c41, DC:0x031a016a
[    0.318371]  SVSB_CCI: svs_init01_isr_handler: VDN74~30:0x13192229~0x2d32383d, DC:0x0319fec8
[    0.318639]  SVSB_GPU: svs_init01_isr_handler: VDN74~30:0x1416181a~0x1d202428, DC:0x031ffef8
[    0.320183] input: cros_ec as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input2
[    0.321134]  SVSB_CPU_LITTLE: svs_init02_isr_handler: VOP74~30:0x1b232b32~0x363a3e44, DC:0x03160000
[    0.321323]  SVSB_CPU_BIG: svs_init02_isr_handler: VOP74~30:0x1c252d34~0x393e4348, DC:0x031a0000
[    0.321385]  SVSB_CCI: svs_init02_isr_handler: VOP74~30:0x1d232b32~0x373b4247, DC:0x03190138
[    0.321424] input: cros_ec_buttons as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input3
[    0.321508]  SVSB_GPU: svs_init02_isr_handler: VOP74~30:0x181a1c1e~0x2125282c, DC:0x031f0108
[    0.322442] mediatek-dpi 14015000.dpi: Found bridge node: /soc/i2c@1100f000/it6505dptx@5c
[    0.322594] cros-ec-spi spi2.0: Chrome EC device registered
[    0.322890] mediatek-drm mediatek-drm.3.auto: bound 14008000.ovl (ops 0xffffffda1f258738)
[    0.322901] mediatek-drm mediatek-drm.3.auto: bound 14009000.ovl (ops 0xffffffda1f258738)
[    0.322909] mediatek-drm mediatek-drm.3.auto: bound 1400a000.ovl (ops 0xffffffda1f258738)
[    0.322923] mediatek-drm mediatek-drm.3.auto: bound 1400b000.rdma (ops 0xffffffda1f2590f8)
[    0.322931] mediatek-drm mediatek-drm.3.auto: bound 1400c000.rdma (ops 0xffffffda1f2590f8)
[    0.322938] mediatek-drm mediatek-drm.3.auto: bound 1400e000.color (ops 0xffffffda1f257bf0)
[    0.322946] mediatek-drm mediatek-drm.3.auto: bound 1400f000.ccorr (ops 0xffffffda1f2578b8)
[    0.322954] mediatek-drm mediatek-drm.3.auto: bound 14010000.aal (ops 0xffffffda1f257648)
[    0.322961] mediatek-drm mediatek-drm.3.auto: bound 14011000.gamma (ops 0xffffffda1f257f30)
[    0.324207] mediatek-drm mediatek-drm.3.auto: bound 14014000.dsi (ops 0xffffffda1f25e8c0)
[    0.324420] mediatek-drm mediatek-drm.3.auto: bound 14015000.dpi (ops 0xffffffda1f25e2f0)
[    0.325156] [drm] Initialized mediatek 1.0.0 20150513 for mediatek-drm.3.auto on minor 0
[    0.325890] tpm_tis_spi spi0.0: Cr50 firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d
[    0.332206] sbs-battery 12-000b: I2C adapter does not support I2C_FUNC_SMBUS_READ_BLOCK_DATA.
[    0.332206] Fallback method does not support PEC.
[    0.339651] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
[    0.346954] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
[    0.350140] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
[    0.350774] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
[    0.353436] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
[    0.354457] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
[    0.355306] mmc1: queuing unknown CIS tuple 0x80 (1 bytes)
[    0.355354] mmc1: queuing unknown CIS tuple 0x81 (1 bytes)
[    0.355402] mmc1: queuing unknown CIS tuple 0x82 (1 bytes)
[    0.355431] mmc1: new ultra high speed SDR104 SDIO card at address 0001
[    0.371984] mtk-msdc 11230000.mmc: phase: [map:ffffff3f] [maxlen:24] [final:20]
[    0.374306] mmc0: new HS400 MMC card at address 0001
[    0.375941] mmcblk0: mmc0:0001 DA4032 29.1 GiB 
[    0.377194] mmcblk0boot0: mmc0:0001 DA4032 partition 1 4.00 MiB
[    0.378445] mmcblk0boot1: mmc0:0001 DA4032 partition 2 4.00 MiB
[    0.378652] mmcblk0rpmb: mmc0:0001 DA4032 partition 3 16.0 MiB, chardev (241:0)
[    0.384142]  mmcblk0: p1 p2 p3 p4 p5 p6 p7 p8 p9 p10 p11 p12
[    0.409070] input: hid-over-i2c 06CB:CDB5 Mouse as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input4
[    0.409495] hid-generic 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
[    0.410208] device-mapper: verity: sha256 using implementation "sha256-ce"
[    0.410567] device-mapper: ioctl: dm-0 (vroot) is ready
[    0.410797] clk: Disabling unused clocks
[    0.411246] ALSA device list:
[    0.411254]   No soundcards found.
[    0.411301] Warning: unable to open an initial console. Fallback to ttynull.
[    0.411315] printk: console [ttynull0] enabled
[    0.421529] EXT4-fs (dm-0): mounting ext2 file system using the ext4 subsystem
[    0.424562] EXT4-fs (dm-0): mounted filesystem without journal. Opts: (null)
[    0.424608] VFS: Mounted root (ext2 filesystem) readonly on device 254:0.
[    0.427625] devtmpfs: mounted
[    0.429473] Freeing unused kernel memory: 1408K
[    0.431021] Run /sbin/init as init process
[    0.507082] audit: type=1404 audit(1740768773.742:2): enforcing=1 old_enforcing=0 auid=4294967295 ses=4294967295 enabled=1 old-enabled=1 lsm=selinux res=1
[    0.550417] SELinux:  Permission bpf in class capability2 not defined in policy.
[    0.550438] SELinux:  Permission checkpoint_restore in class capability2 not defined in policy.
[    0.550459] SELinux:  Permission bpf in class cap2_userns not defined in policy.
[    0.550464] SELinux:  Permission checkpoint_restore in class cap2_userns not defined in policy.
[    0.550553] SELinux: the above unknown classes and permissions will be denied
[    0.554964] SELinux:  policy capability network_peer_controls=1
[    0.554980] SELinux:  policy capability open_perms=1
[    0.554986] SELinux:  policy capability extended_socket_class=1
[    0.554991] SELinux:  policy capability always_check_network=0
[    0.554996] SELinux:  policy capability cgroup_seclabel=0
[    0.555001] SELinux:  policy capability nnp_nosuid_transition=1
[    0.555006] SELinux:  policy capability genfs_seclabel_symlinks=0
[    0.555011] SELinux:  policy capability ioctl_skip_cloexec=0
[    0.595798] audit: type=1403 audit(1740768773.830:3): auid=4294967295 ses=4294967295 lsm=selinux res=1
[    0.658067] usb 1-1: new high-speed USB device number 2 using xhci-mtk
[    0.786261] usb 1-1: New USB device found, idVendor=05e3, idProduct=0608, bcdDevice=60.90
[    0.786279] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    0.786287] usb 1-1: Product: USB2.0 Hub
[    0.787228] hub 1-1:1.0: USB hub found
[    0.787520] hub 1-1:1.0: 3 ports detected
[    0.887315] audit: type=1400 audit(1740768774.122:4): avc:  granted  { execute } for  pid=347 comm="sh" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:cros_init_scripts:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
[    1.065968] usb 1-1.3: new high-speed USB device number 3 using xhci-mtk
[    1.085410] udevd[360]: Starting version 249
[    1.155466] usb 1-1.3: New USB device found, idVendor=0408, idProduct=a064, bcdDevice= 0.04
[    1.155485] usb 1-1.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    1.155492] usb 1-1.3: Product: HD User Facing
[    1.155499] usb 1-1.3: Manufacturer: Quanta
[    1.241714] EXT4-fs (mmcblk0p1): mounted filesystem with ordered data mode. Opts: commit=600,discard
[    1.245221] EXT4-fs (mmcblk0p8): mounted filesystem with ordered data mode. Opts: 
[    1.260687] LoadPin: dm-0 (254:0): read-only
[    1.260707] LoadPin: load pinning engaged.
[    1.260743] LoadPin: kernel-module pinned obj="/lib/modules/5.10.230-25844-gdc65f732bf53/kernel/drivers/input/serio/serio.ko.gz" pid=384 cmdline="udevd --daemon"
[    1.349202] rmi4_f01 rmi4-00.fn01: found RMI device, manufacturer: Synaptics, product: TM3509-001, fw id: 3010219
[    1.378975] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
[    1.391998] INFO chromeos_startup: [tpm.cc(323)] TPM ready
[    1.392194] INFO chromeos_startup: [tpm2.cc(121)] Getting key from TPM2 NVRAM index 8388613
[    1.405477] INFO chromeos_startup: [tpm.cc(440)] Found encstateful NVRAM area.
[    1.424878] INFO chromeos_startup: [encryption_key.cc(181)] Using NVRAM as system key; already populated.
[    1.425867] input: Synaptics TM3509-001 as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input6
[    1.426131] hid-rmi 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
[    1.515752] INFO chromeos_startup: [tpm_setup.cc(98)] There is no bio_crypto_init binary, so skip sending TPM seed.
[    1.544582] INFO chromeos_startup: [tpm.cc(421)] Version 2 Lockbox NVRAM area found.
[    1.544613] INFO chromeos_startup: [tpm_setup.cc(245)] Lockbox is valid, exporting.
[    1.546146] INFO chromeos_startup: [dmcrypt_container.cc(112)] Setting up backing device
[    1.589535] usb 1-1.3: Found UVC 1.00 device HD User Facing (0408:a064)
[    1.614366] usbcore: registered new interface driver uvcvideo
[    1.670313] INFO chromeos_startup: [dmcrypt_container.cc(177)] Waiting for dm-crypt device to appear
[    1.679723] INFO chromeos_startup: [dmcrypt_container.cc(143)] Removing provisioned dmcrypt key from kernel keyring.
[    1.697801] INFO chromeos_startup: [encrypted_fs.cc(275)] Mounting /dev/mapper/encstateful onto /mnt/stateful_partition/encrypted
[    1.698426] INFO chromeos_startup: [encrypted_fs.cc(89)] Using vm.dirty_expire_centisecs/100 as the commit interval
[    1.703592] EXT4-fs (dm-1): mounted filesystem with ordered data mode. Opts: discard,commit=600
[    1.703696] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/var onto /var
[    1.707264] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/chronos onto /home/chronos
[    1.790909] fscrypt: AES-256-CTS-CBC using implementation "cts-cbc-aes-ce"
[    1.802014] audit: type=1400 audit(1740768775.036:5): avc:  granted  { execute } for  pid=624 comm="chromeos_startu" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:chromeos_startup:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
[    1.808735] WARNING chromeos_startup: [stateful_mount.cc(470)] Failed to read from /mnt/stateful_partition/.update_available: No such file or directory (2)
[    1.808990] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
[    1.918286] frecon[598]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
[    2.120520] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/var)
[    2.300597] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/user)
[    2.301570] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/root)
[    2.302555] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/chronos)
[    2.539640] frecon[598]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
[    2.550815] frecon[598]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
[    2.700432] init: bluetoothd pre-start process (782) terminated with status 1
[    2.763077] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.763520] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.763533] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764737] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764758] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764766] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764777] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764785] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764793] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764855] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    2.764863] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
[    3.292785] Bluetooth: bt_init() Core ver 2.22
[    3.293003] NET: Registered protocol family 31
[    3.293010] Bluetooth: bt_init() HCI device and connection manager initialized
[    3.293029] Bluetooth: hci_sock_init() HCI socket layer initialized
[    3.293039] Bluetooth: l2cap_init_sockets() L2CAP socket layer initialized
[    3.293072] Bluetooth: sco_init() SCO socket layer initialized
[    7.509404] init: failsafe-delay main process (766) killed by TERM signal
[    7.646183] fuse: init (API version 7.32)
[    7.785550] init: secagentd post-start process (1684) terminated with status 2
[    8.026745] memfd_create() without MFD_EXEC nor MFD_NOEXEC_SEAL, pid=1825 'patchpaneld'
[    8.165584] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.364745] mtk-scp 10500000.scp: invalid resource
[    8.364843] mtk-scp 10500000.scp: assigned reserved memory node memory@50000000
[    8.377202] remoteproc remoteproc0: scp is available
[    8.386094] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.387575] remoteproc remoteproc0: powering up scp
[    8.387607] remoteproc remoteproc0: Booting fw image mediatek/mt8183/scp_legacy.img, size 1032064
[    8.387640] mtk-scp 10500000.scp: IPI buf addr 0x0007bdb0
[    8.472228] mt6358-sound mt6358-sound: mt6358_platform_driver_probe(), dev name mt6358-sound
[    8.474241] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.484402] Bluetooth: hci_uart_init() HCI UART driver ver 2.3
[    8.484425] Bluetooth: hci_uart_register_proto() HCI UART protocol H4 registered
[    8.484505] Bluetooth: hci_uart_register_proto() HCI UART protocol Three-wire (H5) registered
[    8.485452] Bluetooth: qca_setup() hci0: setting up ROME/QCA6390
[    8.486612] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.493294] Bluetooth: hci_uart_register_proto() HCI UART protocol QCA registered
[    8.495389] elants_i2c 0-0010: supply vcc33 not found, using dummy regulator
[    8.495707] elants_i2c 0-0010: supply vccio not found, using dummy regulator
[    8.521260] elants_i2c 0-0010: nothing at this address
[    8.560386] mtk-scp 10500000.scp: creating channel cros-ec-rpmsg addr 0xd
[    8.560390] mtk-scp 10500000.scp: SCP is ready. FW version kukui_scp_v2.0.2796-7246101293
[    8.560403] remoteproc remoteproc0: remote processor scp is now up
[    8.707377] Bluetooth: qca_recv() hci0: Frame reassembly failed (-84)
[    8.778739] mtk-mdp3 14001000.mdp3_rdma0: Adding to iommu group 0
[    8.778831] mtk-mdp3 14001000.mdp3_rdma0: can't get node mediatek,mmsys2
[    8.778839] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mmsys2
[    8.778874] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mm-mutex2
[    8.779294] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:3 alias:0 id:11 base:0x14001000 regs:00000000b4e1833e
[    8.779349] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:23 alias:0 id:9 base:0x14000000 regs:000000009232c3ac
[    8.779389] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:24 alias:1 id:10 base:0x14000000 regs:00000000687c1018
[    8.779425] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:7 alias:0 id:18 base:0x14005000 regs:000000001d3270b8
[    8.779458] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:8 alias:1 id:19 base:0x14006000 regs:0000000041db81b9
[    8.779490] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:1 alias:0 id:4 base:0x15020000 regs:000000008d103653
[    8.779523] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:22 alias:1 id:6 base:0x15020000 regs:00000000ffc6c9cd
[    8.779570] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:0 id:14 base:0x14003000 regs:00000000695d0cb1
[    8.779612] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:1 id:15 base:0x14004000 regs:000000007822e8c5
[    8.779653] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:5 alias:0 id:20 base:0x14005000 regs:00000000c81cf7df
[    8.779696] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:6 alias:0 id:21 base:0x14006000 regs:00000000dab70d40
[    8.779816] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:18 alias:0 id:13 base:0x1401c000 regs:00000000d58dddf5
[    8.779995] mdp_debug_init:start
[    8.780194] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-tdshp0
[    8.780204] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-color0
[    8.780211] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-aal0
[    8.780227] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mediatek,larb
[    8.780242] mdp_debug_init:end
[    8.785123] mtk-mdp3 14001000.mdp3_rdma0: Driver registered as /dev/video2
[    8.786715] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.796407] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: No cache defaults, reading back from HW
[    8.797121] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mtk_afe_combine_sub_dai(), num of dai 20
[    8.798691] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
[    8.799678] debugfs: Directory '11220000.audio-controller:mt8183-afe-pcm' with parent 'mt8183_mt6358_ts3a227_max98357' already present!
[    8.804708] hdmi-audio-codec hdmi-audio-codec.17.auto: ASoC: sink widget TX overwritten
[    8.819654] debugfs: File 'Playback' in directory 'dapm' already present!
[    8.819680] debugfs: File 'Capture' in directory 'dapm' already present!
[    8.821709] input: mt8183_mt6358_ts3a227_max98357 Headset Jack as /devices/platform/mt8183-sound/sound/card0/input7
[    8.822434] input: mt8183_mt6358_ts3a227_max98357 HDMI Jack as /devices/platform/mt8183-sound/sound/card0/input8
[    8.857362] mtk-cam-dip 15022000.dip: Adding to iommu group 0
[    8.883520] mtk-fd-4.0 1502b000.fd: Adding to iommu group 0
[    8.884147] mtk-fd-4.0 1502b000.fd: scp addr:0x0000000050c00000 va:ffffffc018c00000
[    8.884181] mtk-fd-4.0 1502b000.fd: scp iova addr:0x00000000fd300000
[    8.901325] IPv6: ADDRCONF(NETDEV_CHANGE): veth0: link becomes ready
[    8.912323] mtk-vcodec-enc 17020000.vcodec: Adding to iommu group 0
[    8.916391] mtk-jpeg 17030000.venc_jpg: Adding to iommu group 0
[    8.917987] mtk-jpeg 17030000.venc_jpg: mtk-jpeg-enc device registered as /dev/video28 (81,31)
[    8.924805] mtk-vcodec-dec 16000000.vcodec: Adding to iommu group 0
[    8.941671] mtk-cam-p1 1a000000.camisp: Adding to iommu group 0
[    8.942754] mtk-cam-p1 1a000000.camisp: Registered media3
[    8.942772] mtk-cam-p1 1a000000.camisp: Registered mtk-cam-p1 1a000000.camisp
[    8.960412] Bluetooth: qca_read_soc_version() hci0: QCA Product ID   :0x00000008
[    8.960439] Bluetooth: qca_read_soc_version() hci0: QCA SOC Version  :0x00000044
[    8.960446] Bluetooth: qca_read_soc_version() hci0: QCA ROM Version  :0x00000302
[    8.960454] Bluetooth: qca_read_soc_version() hci0: QCA Patch Version:0x00000111
[    8.960464] Bluetooth: qca_uart_setup() hci0: QCA controller version 0x00440302
[    8.960474] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/rampatch_00440302.bin
[    9.354002] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/nvm_00440302_i2s.bin
[    9.447766] Bluetooth: qca_uart_setup() hci0: QCA setup on UART is completed
[    9.501160] IPv6: ADDRCONF(NETDEV_CHANGE): veth1: link becomes ready
[    9.539189] udevd[438]: Using default interface naming scheme 'v249'.
[    9.552026] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
[    9.552067] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
[    9.552075] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
[    9.552090] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
[    9.567869] mtk-scp 10500000.scp: No such ipi id = 13
[    9.579392] cros-ec-dev cros-ec-dev.18.auto: CrOS System Control Processor MCU detected
[    9.651639] cros-ec-pchg cros-ec-pchg.25.auto: Unable to get number or ports (err:-95)
[    9.651661] cros-ec-pchg cros-ec-pchg.25.auto: No peripheral charge ports (err:-95)
[    9.655774] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: Chrome EC device registered
[    9.659726] ath10k_sdio mmc1:0001:1: qca6174 hw3.2 sdio target 0x05030000 chip_id 0x00000000 sub 0000:0000
[    9.659748] ath10k_sdio mmc1:0001:1: kconfig debug 1 debugfs 1 tracing 1 dfs 0 testmode 1
[    9.659997] ath10k_sdio mmc1:0001:1: firmware ver WLAN.RMH.4.4.1-00189 api 6 features wowlan,ignore-otp,mfp crc32 595e0108
[    9.810556] IPv6: ADDRCONF(NETDEV_CHANGE): arc_ns0: link becomes ready
[    9.824900] ath10k_sdio mmc1:0001:1: board_file api 2 bmi_id 0:4 crc32 e57aadc7
[   10.049651] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mt8183_adda_dmic_set(), kcontrol name MTKAIF_DMIC, mtkaif_dmic 1
[   10.106352] init: send-boot-elog-metrics main process (3107) terminated with status 1
[   10.194428] ath10k_sdio mmc1:0001:1: htt-ver 3.87 wmi-op 4 htt-op 3 cal otp max-sta 32 raw 0 hwcrypto 1
[   10.262735] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
[   10.271818] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
[   10.275914] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
[   10.280015] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
[   10.285673] mtk-msdc 11240000.mmc: phase: [map:ff80003f] [maxlen:9] [final:27]
[   10.287038] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
[   10.313367] udevd[388]: Using default interface naming scheme 'v249'.
[   10.436083] zram: Added device: zram0
[   10.513664] zram0: detected capacity change from 0 to 8136663040
[   10.538558] Adding 7945956k swap on /dev/zram0.  Priority:-2 extents:1 across:7945956k SS
[   10.634444] async_tx: api initialized (async)
[   10.638147] xor: measuring software checksum speed
[   10.639539]    8regs           :  7290 MB/sec
[   10.640645]    32regs          :  9307 MB/sec
[   10.642221]    arm64_neon      :  6379 MB/sec
[   10.642227] xor: using function: 32regs (9307 MB/sec)
[   10.870750] zram: setup backing device /dev/mapper/zram-writeback
[   11.457279] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.458288] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.459257] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.460350] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.461353] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.462151] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.462988] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.463809] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.464637] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.465456] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.466274] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.467091] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.467908] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.468734] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.469730] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.470625] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.471442] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.472257] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.473072] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.473884] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.474698] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.475511] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.476324] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.477122] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.477935] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.478770] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.479881] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.480710] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.481532] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.482353] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.483130] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   11.483949] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   13.969711] wlan0: authenticate with 84:17:ef:e4:dc:b6
[   14.026542] wlan0: send auth to 84:17:ef:e4:dc:b6 (try 1/3)
[   14.027747] wlan0: authenticated
[   14.029973] wlan0: associate with 84:17:ef:e4:dc:b6 (try 1/3)
[   14.033480] wlan0: RX AssocResp from 84:17:ef:e4:dc:b6 (capab=0x1511 status=0 aid=7)
[   14.040181] wlan0: associated
[   14.070497] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
[   14.073115] wlan0: dropped frame to 84:17:ef:e4:dc:b6 (unauthorized port)
[   14.128351] 8021q: 802.1Q VLAN Support v1.8
[   17.008609] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.009686] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.010729] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.011635] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.012541] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.013382] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.014205] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.015180] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.016107] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.017117] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.018107] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.019105] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.020103] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.021109] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.022106] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.023106] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.024106] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.025111] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.026109] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.027109] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.028108] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.029109] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.030109] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.031106] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.032103] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.033111] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.034090] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.035069] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.036055] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.037054] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.038057] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   17.039058] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   22.830200] device-mapper: verity: sha256 using implementation "sha256-ce"
[   25.844636] device-mapper: verity: sha256 using implementation "sha256-ce"
[   26.738321] fscrypt: AES-256-XTS using implementation "xts-aes-ce"
[   30.688227] vaux18: disabling
[   30.688336] vio28: disabling
[   31.007255] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.008211] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.009247] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.010229] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.011067] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.011897] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.012727] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.013558] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.014385] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.015173] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.016131] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.017028] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.017909] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.018775] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.019609] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.020440] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.021630] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.022473] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.023327] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.024308] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.025277] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.026165] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.027028] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.027862] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.028770] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.029770] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.030753] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.031704] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.034198] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.035163] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.036363] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   31.037253] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   60.612952] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
[   60.612970] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
[   60.612975] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
[   60.612979] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
[   60.724814] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
[   60.724832] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
[   60.724837] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
[   60.724842] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
[   60.786005] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
[   60.786037] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
[   60.786047] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
[   60.786057] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
[   60.846394] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
[   60.846417] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
[   60.846425] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
[   60.846433] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
[   62.433114] PDLOG 2025/02/28 18:52:50.085 P0 Disconnected
[   68.004351] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.005180] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.006030] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.006876] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.007720] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.008560] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.009419] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.010252] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.011079] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.011909] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.012768] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.013657] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.014580] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.015476] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.016351] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.017167] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.017989] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.018806] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.019625] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.020444] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.021259] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.022075] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.022889] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.023703] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.024517] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.025331] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.026124] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.026977] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.027813] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.028655] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.029638] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   68.030565] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.010610] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.011581] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.012533] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.013518] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.014366] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.015166] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.016010] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.016852] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.017694] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.018535] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.019418] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.020304] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.021209] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.022095] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.022981] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.023865] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.024749] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.025637] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.026529] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.027419] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.028303] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.029208] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.030103] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.030998] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.031883] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.032768] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.033650] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.034531] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.035435] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.036315] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.037208] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[   73.038091] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
[  287.409468] perf: interrupt took too long (2544 > 2500), lowering kernel.perf_event_max_sample_rate to 78000
[  287.429368] perf: interrupt took too long (3184 > 3180), lowering kernel.perf_event_max_sample_rate to 62000
[  287.455700] perf: interrupt took too long (4012 > 3980), lowering kernel.perf_event_max_sample_rate to 49000
[  287.485923] perf: interrupt took too long (5061 > 5015), lowering kernel.perf_event_max_sample_rate to 39000
[  287.530705] perf: interrupt took too long (6383 > 6326), lowering kernel.perf_event_max_sample_rate to 31000
[  287.600987] perf: interrupt took too long (8032 > 7978), lowering kernel.perf_event_max_sample_rate to 24000
[  287.704753] perf: interrupt took too long (10096 > 10040), lowering kernel.perf_event_max_sample_rate to 19000
[  289.240485] perf: interrupt took too long (12628 > 12620), lowering kernel.perf_event_max_sample_rate to 15000
[  348.435394] init: cupsd main process ended, respawning
[  855.788105] PM: suspend entry (deep)
[  855.800859] Filesystems sync: 0.012 seconds
[  855.803400] Freezing user space processes ... (elapsed 0.003 seconds) done.
[  855.806546] OOM killer disabled.
[  855.806551] Freezing remaining freezable tasks ... (elapsed 0.003 seconds) done.
[  855.811645] rfkill rfkill1: PM: calling rfkill_suspend+0x0/0x34 @ 10509, parent: phy0
[  855.811658] rfkill rfkill1: PM: rfkill_suspend+0x0/0x34 returned 0 after 1 usecs
[  855.811701] platform cros-ec-throttler.26.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811711] platform cros-ec-throttler.26.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811722] platform cros-ec-pchg.25.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811731] platform cros-ec-pchg.25.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811742] cros-ec-pd-update cros-ec-pd-update.24.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811753] cros-ec-pd-update cros-ec-pd-update.24.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 2 usecs
[  855.811765] cros-ec-sysfs cros-ec-sysfs.23.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811773] cros-ec-sysfs cros-ec-sysfs.23.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811785] cros-ec-pd-sysfs cros-ec-pd-sysfs.22.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811793] cros-ec-pd-sysfs cros-ec-pd-sysfs.22.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811805] platform cros-ec-lightbar.21.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811813] platform cros-ec-lightbar.21.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811824] cros-ec-debugfs cros-ec-debugfs.20.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811835] cros-ec-debugfs cros-ec-debugfs.20.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 3 usecs
[  855.811849] cros-ec-chardev cros-ec-chardev.19.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.18.auto
[  855.811955] ieee80211 phy0: PM: calling wiphy_suspend+0x0/0x11c [cfg80211] @ 9, parent: mmc1:0001:1
[  855.811973] cros-ec-chardev cros-ec-chardev.19.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.811993] wlan0: deauthenticating from 84:17:ef:e4:dc:b6 by local choice (Reason: 3=DEAUTH_LEAVING)
[  855.811997] cros-ec-dev cros-ec-dev.18.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 10500000.scp.cros-ec-rpmsg.13.-1
[  855.812003] cros-ec-dev cros-ec-dev.18.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.812041] mtk-cam-p1 1a000000.camisp: PM: calling mtk_isp_pm_suspend+0x0/0x1e0 [mtk_cam_isp] @ 10509, parent: soc
[  855.812053] mtk-cam-p1 1a000000.camisp: PM: mtk_isp_pm_suspend+0x0/0x1e0 [mtk_cam_isp] returned 0 after 0 usecs
[  855.812077] mtk-jpeg 17030000.venc_jpg: PM: calling mtk_jpeg_suspend+0x0/0x40 [mtk_jpeg] @ 10509, parent: soc
[  855.812095] mtk-jpeg 17030000.venc_jpg: PM: mtk_jpeg_suspend+0x0/0x40 [mtk_jpeg] returned 0 after 3 usecs
[  855.812183] mtk-fd-4.0 1502b000.fd: PM: calling mtk_fd_suspend+0x0/0x88 [mtk_fd] @ 10509, parent: soc
[  855.812193] mtk-fd-4.0 1502b000.fd: PM: mtk_fd_suspend+0x0/0x88 [mtk_fd] returned 0 after 0 usecs
[  855.812260] mtk-cam-dip 15022000.dip: PM: calling mtk_dip_pm_suspend+0x0/0x1ec [mtk_dip] @ 10509, parent: soc
[  855.812272] mtk-cam-dip 15022000.dip: PM: mtk_dip_pm_suspend+0x0/0x1ec [mtk_dip] returned 0 after 0 usecs
[  855.812294] input input8: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: card0
[  855.812304] input input8: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 1 usecs
[  855.812318] input input7: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: card0
[  855.812328] input input7: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 1 usecs
[  855.812344] sound pcmC0D7p: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812353] sound pcmC0D7p: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812365] sound pcmC0D6c: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812373] sound pcmC0D6c: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812384] sound pcmC0D5c: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812392] sound pcmC0D5c: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812405] sound pcmC0D4c: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812413] sound pcmC0D4c: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812425] sound pcmC0D3c: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812572] sound pcmC0D3c: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812585] sound pcmC0D2p: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812593] sound pcmC0D2p: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812604] sound pcmC0D1p: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812613] sound pcmC0D1p: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812625] sound pcmC0D0p: PM: calling do_pcm_suspend+0x0/0x3c @ 10509, parent: card0
[  855.812633] sound pcmC0D0p: PM: do_pcm_suspend+0x0/0x3c returned 0 after 0 usecs
[  855.812655] mt6358-sound mt6358-sound: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 1000d000.pwrap:mt6358
[  855.812663] mt6358-sound mt6358-sound: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.812732] mt8183_mt6358_ts3a227 mt8183-sound: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.812741] mt8183_mt6358_ts3a227 mt8183-sound: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.812767] mtk-mdp3 14001000.mdp3_rdma0: PM: calling mdp_suspend+0x0/0x17c [mtk_mdp3] @ 10509, parent: soc
[  855.812774] mtk-mdp3 14001000.mdp3_rdma0: suspend enter : stage flag 1st 0, 2nd 0
[  855.812780] mtk-mdp3 14001000.mdp3_rdma0: suspend check job : stage flag 1st 0, 2nd 0
[  855.812787] mtk-mdp3 14001000.mdp3_rdma0: suspend done : stage flag 1st 0, 2nd 0
[  855.812801] mtk-mdp3 14001000.mdp3_rdma0: PM: mdp_suspend+0x0/0x17c [mtk_mdp3] returned 0 after 19 usecs
[  855.812819] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: PM: calling cros_ec_rpmsg_suspend+0x0/0x28 [cros_ec_rpmsg] @ 10509, parent: 10500000.scp
[  855.812981] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: PM: cros_ec_rpmsg_suspend+0x0/0x28 [cros_ec_rpmsg] returned 0 after 146 usecs
[  855.813026] rfkill rfkill0: PM: calling rfkill_suspend+0x0/0x34 @ 10509, parent: hci0
[  855.813037] rfkill rfkill0: PM: rfkill_suspend+0x0/0x34 returned 0 after 1 usecs
[  855.813070] platform regulatory.0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.813078] platform regulatory.0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.813116] input input6: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: 0018:06CB:CDB5.0001
[  855.813126] input input6: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 1 usecs
[  855.813235] usb 1-1.3: PM: calling usb_dev_suspend+0x0/0x28 @ 9528, parent: 1-1
[  855.813246] usb 1-1.3: PM: usb_dev_suspend+0x0/0x28 returned 0 after 2 usecs
[  855.813346] usb 1-1: PM: calling usb_dev_suspend+0x0/0x28 @ 7, parent: usb1
[  855.813404] mediatek-drm mediatek-drm.3.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 14000000.syscon
[  855.813469] mmcblk mmc0:0001: PM: calling mmc_bus_suspend+0x0/0x5c @ 199, parent: mmc0
[  855.813526] mediatek-drm mediatek-drm.3.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 96 usecs
[  855.813562] mipi-dsi 14014000.dsi.0: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: 14014000.dsi
[  855.813571] mipi-dsi 14014000.dsi.0: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.813591] input input3: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: 11012000.spi:cros-ec@0:keyboard-controller
[  855.813601] input input3: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 0 usecs
[  855.813616] input input2: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: 11012000.spi:cros-ec@0:keyboard-controller
[  855.813626] input input2: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 1 usecs
[  855.813641] cros-ec-keyb 11012000.spi:cros-ec@0:keyboard-controller: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: spi2.0
[  855.813650] cros-ec-keyb 11012000.spi:cros-ec@0:keyboard-controller: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.813663] cros-ec-typec 11012000.spi:cros-ec@0:typec: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: spi2.0
[  855.813673] cros-ec-typec 11012000.spi:cros-ec@0:typec: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1 usecs
[  855.813689] mtk-svs 1100b000.svs: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.814013] mtk-svs 1100b000.svs: PM: platform_pm_suspend+0x0/0x64 returned 0 after 306 usecs
[  855.814030] hdmi-audio-codec hdmi-audio-codec.17.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 3-005c
[  855.814039] hdmi-audio-codec hdmi-audio-codec.17.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814064] extcon-usbc-cros-ec 11012000.spi:cros-ec@0:extcon0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: spi2.0
[  855.814073] extcon-usbc-cros-ec 11012000.spi:cros-ec@0:extcon0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814107] input input1: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: volume-buttons
[  855.814117] input input1: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 0 usecs
[  855.814131] input input0: PM: calling input_dev_suspend+0x0/0x1c4 @ 10509, parent: wifi-wakeup
[  855.814141] input input0: PM: input_dev_suspend+0x0/0x1c4 returned 0 after 0 usecs
[  855.814177] it6505 3-005c: PM: calling it6505_bridge_suspend+0x0/0x28 @ 9529, parent: i2c-3
[  855.814203] sbs-battery 12-000b: PM: calling sbs_suspend+0x0/0x94 @ 201, parent: i2c-12
[  855.814207] it6505 3-005c: PM: it6505_bridge_suspend+0x0/0x28 returned 0 after 16 usecs
[  855.814220] sbs-battery 12-000b: PM: sbs_suspend+0x0/0x94 returned 0 after 0 usecs
[  855.814262] cros-ec-i2c-tunnel 11012000.spi:cros-ec@0:i2c-tunnel: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: spi2.0
[  855.814271] cros-ec-i2c-tunnel 11012000.spi:cros-ec@0:i2c-tunnel: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814285] platform cros-ec-throttler.16.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.814293] platform cros-ec-throttler.16.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814322] mali 13040000.mali: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.814376] mali 13040000.mali: PM: platform_pm_suspend+0x0/0x64 returned 0 after 44 usecs
[  855.814390] platform cros-ec-pchg.15.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.814399] platform cros-ec-pchg.15.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814533] anx7625 4-0058: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 201, parent: i2c-4
[  855.814544] anx7625 4-0058: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.814562] panel-edp panel: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.814590] panel-edp panel: PM: platform_pm_suspend+0x0/0x64 returned 0 after 18 usecs
[  855.814657] mtk-iommu 10205000.iommu: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.814665] mtk-iommu 10205000.iommu: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814684] backlight backlight_lcd0: PM: calling backlight_suspend+0x0/0x94 @ 10509, parent: backlight_lcd0
[  855.814693] backlight backlight_lcd0: PM: backlight_suspend+0x0/0x94 returned 0 after 1 usecs
[  855.814706] pwm-backlight backlight_lcd0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.814716] pwm-backlight backlight_lcd0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1 usecs
[  855.814733] pwm pwmchip0: PM: calling pwm_class_suspend+0x0/0x200 @ 10509, parent: 1100e000.pwm
[  855.814742] pwm pwmchip0: PM: pwm_class_suspend+0x0/0x200 returned 0 after 0 usecs
[  855.814759] generic-adc-thermal thermal-sensor2: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.814767] generic-adc-thermal thermal-sensor2: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814779] generic-adc-thermal thermal-sensor1: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.814788] generic-adc-thermal thermal-sensor1: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814818] mtk-power-controller 10006000.syscon:power-controller: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 10006000.syscon
[  855.814827] mtk-power-controller 10006000.syscon:power-controller: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814841] amba db10000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.814848] amba db10000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.814861] amba da10000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.814869] amba da10000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.814881] amba d910000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.814889] amba d910000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.814902] amba d810000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.814910] amba d810000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.814931] cros-ec-pd-update cros-ec-pd-update.14.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.814942] cros-ec-pd-update cros-ec-pd-update.14.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1 usecs
[  855.814954] amba d710000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.814962] amba d710000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.814974] cros-ec-sysfs cros-ec-sysfs.13.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.814982] cros-ec-sysfs cros-ec-sysfs.13.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.814994] amba d610000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.815002] amba d610000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.815013] amba d510000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.815021] amba d510000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.815033] amba d410000.cpu-debug: PM: calling pm_generic_suspend+0x0/0x44 @ 10509, parent: soc
[  855.815041] amba d410000.cpu-debug: PM: pm_generic_suspend+0x0/0x44 returned 0 after 0 usecs
[  855.815054] cros-ec-pd-sysfs cros-ec-pd-sysfs.12.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815062] cros-ec-pd-sysfs cros-ec-pd-sysfs.12.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815075] platform cros-ec-lightbar.11.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815083] platform cros-ec-lightbar.11.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815095] cros-ec-debugfs cros-ec-debugfs.10.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815105] cros-ec-debugfs cros-ec-debugfs.10.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 2 usecs
[  855.815120] cros-ec-chardev cros-ec-chardev.9.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815128] cros-ec-chardev cros-ec-chardev.9.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815140] cros-usbpd-notify cros-usbpd-notify.8.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815148] cros-usbpd-notify cros-usbpd-notify.8.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815160] cros-usbpd-logger cros-usbpd-logger.7.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815171] cros-usbpd-logger cros-usbpd-logger.7.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 2 usecs
[  855.815194] cros-usbpd-charger cros-usbpd-charger.6.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: cros-ec-dev.5.auto
[  855.815203] cros-usbpd-charger cros-usbpd-charger.6.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815222] snd-soc-dummy snd-soc-dummy: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.815230] snd-soc-dummy snd-soc-dummy: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815251] cros-ec-dev cros-ec-dev.5.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: spi2.0
[  855.815259] cros-ec-dev cros-ec-dev.5.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815283] mediatek-cci-devfreq cci: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.815291] mediatek-cci-devfreq cci: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.815324] i2c_hid_of 2-002c: PM: calling i2c_hid_core_suspend+0x0/0x144 @ 201, parent: i2c-2
[  855.816178] i2c_hid_of 2-002c: PM: i2c_hid_core_suspend+0x0/0x144 returned 0 after 822 usecs
[  855.819254] mmcblk mmc0:0001: PM: mmc_bus_suspend+0x0/0x5c returned 0 after 5626 usecs
[  855.819311] mtk-msdc 11230000.mmc: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.819344] mtk-msdc 11230000.mmc: PM: platform_pm_suspend+0x0/0x64 returned 0 after 21 usecs
[  855.910819] usb 1-1: PM: usb_dev_suspend+0x0/0x28 returned 0 after 95173 usecs
[  855.923903] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
[  855.931207] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
[  855.934385] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
[  855.935023] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
[  855.937709] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
[  855.938746] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
[  855.938878] ieee80211 phy0: PM: wiphy_suspend+0x0/0x11c [cfg80211] returned 0 after 123827 usecs
[  855.939027] ath10k_sdio mmc1:0001:1: PM: calling pm_generic_suspend+0x0/0x44 @ 9528, parent: mmc1:0001
[  855.939038] ath10k_sdio mmc1:0001:1: PM: pm_generic_suspend+0x0/0x44 returned 0 after 1 usecs
[  855.939150] mmc mmc1:0001: PM: calling mmc_bus_suspend+0x0/0x5c @ 198, parent: mmc1
[  855.940441] mmc mmc1:0001: PM: mmc_bus_suspend+0x0/0x5c returned 0 after 1249 usecs
[  855.940594] mtk-msdc 11240000.mmc: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.940628] mtk-msdc 11240000.mmc: PM: platform_pm_suspend+0x0/0x64 returned 0 after 24 usecs
[  855.940708] psci-cpuidle psci-cpuidle: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.940717] psci-cpuidle psci-cpuidle: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.940739] mtk-cpufreq mtk-cpufreq: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.940747] mtk-cpufreq mtk-cpufreq: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.940811] alarmtimer alarmtimer.4.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: rtc0
[  855.940895] ts3a227e 5-003b: PM: calling ts3a227e_suspend+0x0/0x30 [snd_soc_ts3a227e] @ 9529, parent: i2c-5
[  855.940909] ts3a227e 5-003b: PM: ts3a227e_suspend+0x0/0x30 [snd_soc_ts3a227e] returned 0 after 3 usecs
[  855.942021] alarmtimer alarmtimer.4.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1171 usecs
[  855.942040] rtc rtc0: PM: calling rtc_suspend+0x0/0x14c @ 10509, parent: mt6358-rtc
[  855.942255] rtc rtc0: PM: rtc_suspend+0x0/0x14c returned 0 after 200 usecs
[  855.942308] platform Fixed MDIO bus.0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.942317] platform Fixed MDIO bus.0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.942341] cros-ec-spi spi2.0: PM: calling cros_ec_spi_suspend+0x0/0x28 @ 10509, parent: spi2
[  855.942429] usb usb2: PM: calling usb_dev_suspend+0x0/0x28 @ 9528, parent: 11200000.xhci
[  855.942434] usb usb1: PM: calling usb_dev_suspend+0x0/0x28 @ 198, parent: 11200000.xhci
[  855.942447] usb usb2: PM: usb_dev_suspend+0x0/0x28 returned 0 after 1 usecs
[  855.943505] cros-ec-spi spi2.0: PM: cros_ec_spi_suspend+0x0/0x28 returned 0 after 1127 usecs
[  855.943527] mtd mtd0ro: PM: calling mtd_cls_suspend+0x0/0x78 @ 10509, parent: spi1.0
[  855.943536] mtd mtd0ro: PM: mtd_cls_suspend+0x0/0x78 returned 0 after 0 usecs
[  855.943552] mtd mtd0: PM: calling mtd_cls_suspend+0x0/0x78 @ 10509, parent: spi1.0
[  855.943561] mtd mtd0: PM: mtd_cls_suspend+0x0/0x78 returned 0 after 0 usecs
[  855.943590] tpm_tis_spi spi0.0: PM: calling tpm_pm_suspend+0x0/0xac @ 10509, parent: spi0
[  855.943599] tpm_tis_spi spi0.0: PM: tpm_pm_suspend+0x0/0xac returned 0 after 0 usecs
[  855.943629] mt6397-rtc mt6358-rtc: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 1000d000.pwrap:mt6358
[  855.943642] mt6397-rtc mt6358-rtc: PM: platform_pm_suspend+0x0/0x64 returned 0 after 4 usecs
[  855.943660] regulator regulator.52: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943670] regulator regulator.52: PM: regulator_suspend+0x0/0x128 returned 0 after 1 usecs
[  855.943684] regulator regulator.51: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943694] regulator regulator.51: PM: regulator_suspend+0x0/0x128 returned 0 after 1 usecs
[  855.943706] regulator regulator.50: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943716] regulator regulator.50: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943728] regulator regulator.49: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943738] regulator regulator.49: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943750] regulator regulator.48: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943760] regulator regulator.48: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943772] regulator regulator.47: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943781] regulator regulator.47: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943794] regulator regulator.46: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943803] regulator regulator.46: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943816] regulator regulator.45: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943826] regulator regulator.45: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943838] regulator regulator.44: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943847] regulator regulator.44: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943860] regulator regulator.43: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943869] regulator regulator.43: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943883] regulator regulator.42: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943892] regulator regulator.42: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943905] regulator regulator.41: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943914] regulator regulator.41: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943935] regulator regulator.40: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943945] regulator regulator.40: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943958] regulator regulator.39: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943967] regulator regulator.39: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.943980] regulator regulator.38: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.943989] regulator regulator.38: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944002] regulator regulator.37: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944011] regulator regulator.37: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944024] regulator regulator.36: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944033] regulator regulator.36: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944045] regulator regulator.35: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944054] regulator regulator.35: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944068] regulator regulator.34: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944077] regulator regulator.34: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944090] regulator regulator.33: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944099] regulator regulator.33: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944112] regulator regulator.32: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944121] regulator regulator.32: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944134] regulator regulator.31: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944143] regulator regulator.31: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944156] regulator regulator.30: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944165] regulator regulator.30: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944178] regulator regulator.29: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944187] regulator regulator.29: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944200] regulator regulator.28: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944209] regulator regulator.28: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.944222] regulator regulator.27: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.944231] regulator regulator.27: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.952521] usb usb1: PM: usb_dev_suspend+0x0/0x28 returned 0 after 9843 usecs
[  855.952651] xhci-mtk 11200000.xhci: PM: calling platform_pm_suspend+0x0/0x64 @ 9528, parent: 11201000.usb
[  855.952666] xhci-mtk 11200000.xhci: PM: platform_pm_suspend+0x0/0x64 returned 0 after 6 usecs
[  855.952803] mtu3 11201000.usb: PM: calling platform_pm_suspend+0x0/0x64 @ 9529, parent: soc
[  855.953224] mtu3 11201000.usb: PM: platform_pm_suspend+0x0/0x64 returned 0 after 401 usecs
[  855.953361] regulator regulator.26: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953371] regulator regulator.26: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953386] regulator regulator.25: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953395] regulator regulator.25: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953409] regulator regulator.24: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953418] regulator regulator.24: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953431] regulator regulator.23: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953440] regulator regulator.23: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953453] regulator regulator.22: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953462] regulator regulator.22: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953475] regulator regulator.21: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953485] regulator regulator.21: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953497] regulator regulator.20: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953506] regulator regulator.20: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953520] regulator regulator.19: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953529] regulator regulator.19: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953541] regulator regulator.18: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953550] regulator regulator.18: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953564] regulator regulator.17: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953573] regulator regulator.17: PM: regulator_suspend+0x0/0x128 returned 0 after 1 usecs
[  855.953587] regulator regulator.16: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953596] regulator regulator.16: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953610] regulator regulator.15: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953619] regulator regulator.15: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953632] regulator regulator.14: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953641] regulator regulator.14: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953654] regulator regulator.13: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953663] regulator regulator.13: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953676] regulator regulator.12: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: mt6358-regulator
[  855.953685] regulator regulator.12: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.953721] mt6358-regulator mt6358-regulator: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 1000d000.pwrap:mt6358
[  855.953729] mt6358-regulator mt6358-regulator: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.953798] hci_uart_qca serial0-0: PM: calling qca_suspend+0x0/0x3a8 [hci_uart] @ 10509, parent: serial0
[  855.953856] hci_uart_qca serial0-0: PM: qca_suspend+0x0/0x3a8 [hci_uart] returned 0 after 40 usecs
[  855.953883] serial8250 serial8250: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.953892] serial8250 serial8250: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1 usecs
[  855.953912] clk-mt8183-mm clk-mt8183-mm.2.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 14000000.syscon
[  855.953930] clk-mt8183-mm clk-mt8183-mm.2.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.953946] mt6397 1000d000.pwrap:mt6358: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 1000d000.pwrap
[  855.953954] mt6397 1000d000.pwrap:mt6358: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954052] mtk-socinfo mtk-socinfo.1.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 11f10000.efuse
[  855.954061] mtk-socinfo mtk-socinfo.1.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954076] platform mtk-socinfo.0.auto: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: 8000000.soc_data
[  855.954085] platform mtk-socinfo.0.auto: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954104] regulator regulator.11: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: vddio-mipibrdg
[  855.954113] regulator regulator.11: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954128] regulator regulator.10: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: pp3300-panel
[  855.954137] regulator regulator.10: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954152] regulator regulator.9: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: pp1800-mipibrdg
[  855.954161] regulator regulator.9: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954175] regulator regulator.8: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: pp1200-mipibrdg
[  855.954184] regulator regulator.8: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954198] regulator regulator.7: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator6
[  855.954207] regulator regulator.7: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954221] regulator regulator.6: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator5
[  855.954230] regulator regulator.6: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954244] regulator regulator.5: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator4
[  855.954253] regulator regulator.5: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954266] regulator regulator.4: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator3
[  855.954275] regulator regulator.4: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954289] regulator regulator.3: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator2
[  855.954298] regulator regulator.3: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954312] regulator regulator.2: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator1
[  855.954321] regulator regulator.2: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954335] regulator regulator.1: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: regulator0
[  855.954344] regulator regulator.1: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.954378] max98357a max98357a: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954386] max98357a max98357a: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954400] gpio-keys volume-buttons: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954411] gpio-keys volume-buttons: PM: platform_pm_suspend+0x0/0x64 returned 0 after 2 usecs
[  855.954424] reg-fixed-voltage vddio-mipibrdg: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954432] reg-fixed-voltage vddio-mipibrdg: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954445] reg-fixed-voltage pp3300-panel: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954453] reg-fixed-voltage pp3300-panel: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954465] reg-fixed-voltage pp1800-mipibrdg: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954473] reg-fixed-voltage pp1800-mipibrdg: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954485] reg-fixed-voltage pp1200-mipibrdg: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954493] reg-fixed-voltage pp1200-mipibrdg: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954508] gpio-keys wifi-wakeup: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954518] gpio-keys wifi-wakeup: PM: platform_pm_suspend+0x0/0x64 returned 0 after 2 usecs
[  855.954531] pwrseq_simple wifi-pwrseq: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954539] pwrseq_simple wifi-pwrseq: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954552] bt-sco bt-sco: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954560] bt-sco bt-sco: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954572] reg-fixed-voltage regulator6: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954580] reg-fixed-voltage regulator6: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954592] reg-fixed-voltage regulator5: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954600] reg-fixed-voltage regulator5: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954612] reg-fixed-voltage regulator4: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954620] reg-fixed-voltage regulator4: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954633] reg-fixed-voltage regulator3: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954640] reg-fixed-voltage regulator3: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954653] reg-fixed-voltage regulator2: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954660] reg-fixed-voltage regulator2: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954673] reg-fixed-voltage regulator1: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954681] reg-fixed-voltage regulator1: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954694] reg-fixed-voltage regulator0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.954702] reg-fixed-voltage regulator0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954715] clk-mt8183-cam 1a000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954723] clk-mt8183-cam 1a000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954736] clk-mt8183-ipu_core1 19280000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954744] clk-mt8183-ipu_core1 19280000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954757] clk-mt8183-ipu_core0 19180000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954765] clk-mt8183-ipu_core0 19180000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954777] clk-mt8183-ipu_adl 19010000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954785] clk-mt8183-ipu_adl 19010000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954798] clk-mt8183-ipu_conn 19000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954806] clk-mt8183-ipu_conn 19000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954818] clk-mt8183-venc 17000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954827] clk-mt8183-venc 17000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954839] clk-mt8183-vdec 16000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954848] clk-mt8183-vdec 16000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954860] clk-mt8183-img 15020000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954868] clk-mt8183-img 15020000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954881] platform 1401c000.mdp3_ccorr: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954889] platform 1401c000.mdp3_ccorr: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954901] platform 14012000.dither: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954909] platform 14012000.dither: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954929] platform 14006000.mdp3_wdma: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954938] platform 14006000.mdp3_wdma: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954951] platform 14005000.mdp3_wrot0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954959] platform 14005000.mdp3_wrot0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954971] platform 14004000.mdp3_rsz1: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954979] platform 14004000.mdp3_rsz1: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.954991] platform 14003000.mdp3_rsz0: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.954999] platform 14003000.mdp3_rsz0: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955015] mtk-mmsys 14000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955023] mtk-mmsys 14000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955038] mtk-tphy soc:usb-phy@11f40000: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955046] mtk-tphy soc:usb-phy@11f40000: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955059] mediatek,efuse 11f10000.efuse: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955067] mediatek,efuse 11f10000.efuse: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955080] mediatek-mipi-tx 11e50000.mipi-dphy: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955088] mediatek-mipi-tx 11e50000.mipi-dphy: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955102] clk-mt8183-audio 11220000.audio-controller: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955110] clk-mt8183-audio 11220000.audio-controller: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955123] i2c-mt65xx 11016000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955131] i2c-mt65xx 11016000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955144] mtk-spi 11012000.spi: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955159] mtk-spi 11012000.spi: PM: platform_pm_suspend+0x0/0x64 returned 0 after 6 usecs
[  855.955172] i2c-mt65xx 11011000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955180] i2c-mt65xx 11011000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955193] mtk-spi 11010000.spi: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955201] mtk-spi 11010000.spi: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955214] i2c-mt65xx 1100f000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955221] i2c-mt65xx 1100f000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955233] platform 11006000.pwm: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955241] platform 11006000.pwm: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955255] mtk-thermal 1100b000.thermal: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955269] mtk-thermal 1100b000.thermal: PM: platform_pm_suspend+0x0/0x64 returned 0 after 5 usecs
[  855.955282] mtk-spi 1100a000.spi: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955291] mtk-spi 1100a000.spi: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955303] i2c-mt65xx 11009000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955311] i2c-mt65xx 11009000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955324] i2c-mt65xx 11008000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955332] i2c-mt65xx 11008000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955344] i2c-mt65xx 11007000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955352] i2c-mt65xx 11007000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955365] i2c-mt65xx 11005000.i2c: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955373] i2c-mt65xx 11005000.i2c: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955386] mt6577-uart 11003000.serial: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955473] mt6577-uart 11003000.serial: PM: platform_pm_suspend+0x0/0x64 returned 0 after 76 usecs
[  855.955487] mt6577-uart 11002000.serial: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955518] mt6577-uart 11002000.serial: PM: platform_pm_suspend+0x0/0x64 returned 0 after 21 usecs
[  855.955532] mt6577-auxadc 11001000.auxadc: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955543] mt6577-auxadc 11001000.auxadc: PM: platform_pm_suspend+0x0/0x64 returned 0 after 3 usecs
[  855.955557] mtk_cmdq 10238000.mailbox: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955569] mtk_cmdq 10238000.mailbox: PM: platform_pm_suspend+0x0/0x64 returned 0 after 3 usecs
[  855.955581] platform 10017000.timer: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955589] platform 10017000.timer: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955604] mtk-scp 10500000.scp: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955612] mtk-scp 10500000.scp: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955624] mt-pmic-pwrap 1000d000.pwrap: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955633] mt-pmic-pwrap 1000d000.pwrap: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955646] clk-mt8183 1000c000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955654] clk-mt8183 1000c000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955668] mtk-wdt 10007000.watchdog: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955677] mtk-wdt 10007000.watchdog: PM: platform_pm_suspend+0x0/0x64 returned 0 after 1 usecs
[  855.955690] platform 10006000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955698] platform 10006000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955713] mt8183-pinctrl 10005000.pinctrl: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955722] mt8183-pinctrl 10005000.pinctrl: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955734] clk-mt8183 10003000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955742] clk-mt8183 10003000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955757] clk-mt8183 10001000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955765] clk-mt8183 10001000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955777] clk-mt8183 10000000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955785] clk-mt8183 10000000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955797] clk-mt8183 c530000.syscon: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955805] clk-mt8183 c530000.syscon: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955818] mediatek,efuse 8000000.soc_data: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: soc
[  855.955826] mediatek,efuse 8000000.soc_data: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955895] platform soc: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.955903] platform soc: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955923] platform timer: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.955931] platform timer: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955944] platform fixed-factor-clock-13m: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.955952] platform fixed-factor-clock-13m: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955965] psci-cpuidle-domain psci: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.955973] psci-cpuidle-domain psci: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.955986] armv8-pmu pmu-a73: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.955994] armv8-pmu pmu-a73: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956006] armv8-pmu pmu-a53: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.956014] armv8-pmu pmu-a53: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956026] platform firmware:chromeos: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.956034] platform firmware:chromeos: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956069] coreboot_table ffed9000.coreboot: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.956078] coreboot_table ffed9000.coreboot: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956093] ramoops ffedb000.ramoops: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.956101] ramoops ffedb000.ramoops: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956135] regulator regulator.0: PM: calling regulator_suspend+0x0/0x128 @ 10509, parent: reg-dummy
[  855.956144] regulator regulator.0: PM: regulator_suspend+0x0/0x128 returned 0 after 0 usecs
[  855.956157] reg-dummy reg-dummy: PM: calling platform_pm_suspend+0x0/0x64 @ 10509, parent: platform
[  855.956165] reg-dummy reg-dummy: PM: platform_pm_suspend+0x0/0x64 returned 0 after 0 usecs
[  855.956572] i2c 0-0010: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-0
[  855.956582] i2c 0-0010: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.956753] i2c i2c-13: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: 3-005c
[  855.956762] i2c i2c-13: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.956789] it6505 3-005c: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-3
[  855.956798] it6505 3-005c: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.956824] sbs-battery 12-000b: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-12
[  855.956833] sbs-battery 12-000b: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.956846] i2c i2c-12: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: 11012000.spi:cros-ec@0:i2c-tunnel
[  855.956854] i2c i2c-12: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957172] mtk-smi-larb 1a002000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957183] mtk-smi-larb 1a002000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957195] mtk-smi-larb 1a001000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957204] mtk-smi-larb 1a001000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957216] mtk-smi-larb 17010000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957225] mtk-smi-larb 17010000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957237] dummy 4-002c: PM: calling i2c_suspend_late+0x0/0x7c @ 9528, parent: i2c-4
[  855.957242] mtk-smi-larb 16010000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957249] dummy 4-002a: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-4
[  855.957253] mtk-smi-larb 16010000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957259] dummy 4-002a: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957264] dummy 4-0042: PM: calling i2c_suspend_late+0x0/0x7c @ 198, parent: i2c-4
[  855.957270] dummy 4-0042: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957278] dummy 4-0039: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-4
[  855.957283] dummy 4-003f: PM: calling i2c_suspend_late+0x0/0x7c @ 195, parent: i2c-4
[  855.957288] dummy 4-003d: PM: calling i2c_suspend_late+0x0/0x7c @ 198, parent: i2c-4
[  855.957292] dummy 4-0039: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957296] dummy 4-003f: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957302] dummy 4-003d: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957306] dummy 4-0038: PM: calling i2c_suspend_late+0x0/0x7c @ 9529, parent: i2c-4
[  855.957311] anx7625 4-0058: PM: calling i2c_suspend_late+0x0/0x7c @ 195, parent: i2c-4
[  855.957315] dummy 4-0038: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957321] anx7625 4-0058: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957340] mtk-smi-larb 1502f000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957346] mtk-smi-larb 1502f000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957355] mtk-smi-larb 15021000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957361] mtk-smi-larb 15021000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957370] dummy 4-002c: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957374] mtk-smi-larb 14017000.larb: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957380] mtk-smi-larb 14017000.larb: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957391] mtk-smi-common 14019000.smi: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957401] mtk-smi-common 14019000.smi: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957415] mtk-iommu 10205000.iommu: PM: calling pm_runtime_force_suspend+0x0/0xc8 @ 10509, parent: soc
[  855.957423] mtk-iommu 10205000.iommu: PM: pm_runtime_force_suspend+0x0/0xc8 returned 0 after 0 usecs
[  855.957678] i2c_hid_of 2-002c: PM: calling i2c_suspend_late+0x0/0x7c @ 9528, parent: i2c-2
[  855.957688] i2c_hid_of 2-002c: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957712] i2c 0-0040: PM: calling i2c_suspend_late+0x0/0x7c @ 9528, parent: i2c-0
[  855.957721] i2c 0-0040: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957854] ts3a227e 5-003b: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: i2c-5
[  855.957864] ts3a227e 5-003b: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957892] i2c i2c-5: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11016000.i2c
[  855.957901] i2c i2c-5: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957938] i2c i2c-1: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11011000.i2c
[  855.957947] i2c i2c-1: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.957977] i2c i2c-3: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 1100f000.i2c
[  855.957986] i2c i2c-3: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.958010] i2c 2-0015: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: i2c-2
[  855.958019] i2c 2-0015: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.958047] i2c i2c-2: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11009000.i2c
[  855.958056] i2c i2c-2: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.958086] i2c i2c-4: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11008000.i2c
[  855.958095] i2c i2c-4: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.958123] i2c i2c-0: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11007000.i2c
[  855.958132] i2c i2c-0: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  855.958159] i2c i2c-6: PM: calling i2c_suspend_late+0x0/0x7c @ 9, parent: 11005000.i2c
[  855.958168] i2c i2c-6: PM: i2c_suspend_late+0x0/0x7c returned 0 after 0 usecs
[  856.024113] mtk-cam-p1 1a000000.camisp: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024126] mtk-cam-p1 1a000000.camisp: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 2 usecs
[  856.024140] mtk-vcodec-dec 16000000.vcodec: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024150] mtk-vcodec-dec 16000000.vcodec: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 1 usecs
[  856.024163] mtk-jpeg 17030000.venc_jpg: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024172] mtk-jpeg 17030000.venc_jpg: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024184] mtk-vcodec-enc 17020000.vcodec: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024193] mtk-vcodec-enc 17020000.vcodec: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024221] mtk-fd-4.0 1502b000.fd: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024230] mtk-fd-4.0 1502b000.fd: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 1 usecs
[  856.024260] mtk-cam-dip 15022000.dip: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024269] mtk-cam-dip 15022000.dip: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024335] mtk-mdp3 14001000.mdp3_rdma0: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024345] mtk-mdp3 14001000.mdp3_rdma0: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024677] mediatek-dpi 14015000.dpi: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024687] mediatek-dpi 14015000.dpi: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024781] genpd genpd:2:13040000.mali: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: none
[  856.024791] genpd genpd:2:13040000.mali: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024802] genpd genpd:1:13040000.mali: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: none
[  856.024811] genpd genpd:1:13040000.mali: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024822] genpd genpd:0:13040000.mali: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: none
[  856.024831] genpd genpd:0:13040000.mali: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024841] mtk-dsi 14014000.dsi: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024850] mtk-dsi 14014000.dsi: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.024987] mediatek-disp-rdma 1400c000.rdma: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.024996] mediatek-disp-rdma 1400c000.rdma: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025008] mediatek-disp-rdma 1400b000.rdma: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025016] mediatek-disp-rdma 1400b000.rdma: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025027] mediatek-disp-ovl 1400a000.ovl: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025035] mediatek-disp-ovl 1400a000.ovl: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025045] mediatek-disp-ovl 14009000.ovl: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025054] mediatek-disp-ovl 14009000.ovl: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025064] mediatek-disp-ovl 14008000.ovl: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025072] mediatek-disp-ovl 14008000.ovl: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025083] mtk-smi-larb 1a002000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025092] mtk-smi-larb 1a002000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025102] mtk-smi-larb 1a001000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025111] mtk-smi-larb 1a001000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025121] mtk-smi-larb 17010000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025129] mtk-smi-larb 17010000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025139] mtk-smi-larb 16010000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025147] mtk-smi-larb 16010000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025157] mtk-smi-larb 1502f000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025166] mtk-smi-larb 1502f000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025176] mtk-smi-larb 15021000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025184] mtk-smi-larb 15021000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025194] mtk-smi-larb 14017000.larb: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025203] mtk-smi-larb 14017000.larb: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025213] mtk-smi-common 14019000.smi: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025222] mtk-smi-common 14019000.smi: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025234] clk-mt8183-mfg 13000000.syscon: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025244] clk-mt8183-mfg 13000000.syscon: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025260] mediatek-disp-pwm 1100e000.pwm: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025269] mediatek-disp-pwm 1100e000.pwm: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025283] mediatek-disp-gamma 14011000.gamma: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025291] mediatek-disp-gamma 14011000.gamma: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025302] mediatek-disp-color 1400e000.color: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025310] mediatek-disp-color 1400e000.color: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025321] mediatek-disp-ccorr 1400f000.ccorr: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025330] mediatek-disp-ccorr 1400f000.ccorr: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025341] mediatek-disp-aal 14010000.aal: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025350] mediatek-disp-aal 14010000.aal: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 0 usecs
[  856.025360] mediatek-mutex 14016000.mutex: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: soc
[  856.025411] mediatek-mutex 14016000.mutex: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 41 usecs
[  856.025975] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: PM: calling genpd_suspend_noirq+0x0/0x28 @ 10509, parent: 11220000.audio-controller
[  856.025986] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: PM: genpd_suspend_noirq+0x0/0x28 returned 0 after 1 usecs
[  856.026100] i2c-mt65xx 11016000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026113] i2c-mt65xx 11016000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 2 usecs
[  856.026125] i2c-mt65xx 11011000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026134] i2c-mt65xx 11011000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026145] i2c-mt65xx 1100f000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026154] i2c-mt65xx 1100f000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026168] i2c-mt65xx 11009000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026177] i2c-mt65xx 11009000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026188] i2c-mt65xx 11008000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026197] i2c-mt65xx 11008000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026207] i2c-mt65xx 11007000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026216] i2c-mt65xx 11007000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026227] i2c-mt65xx 11005000.i2c: PM: calling mtk_i2c_suspend_noirq+0x0/0x84 @ 10509, parent: soc
[  856.026236] i2c-mt65xx 11005000.i2c: PM: mtk_i2c_suspend_noirq+0x0/0x84 returned 0 after 0 usecs
[  856.026262] mt8183-pinctrl 10005000.pinctrl: PM: calling mtk_paris_pinctrl_suspend+0x0/0x2c @ 10509, parent: soc
[  856.026271] mt8183-pinctrl 10005000.pinctrl: PM: mtk_paris_pinctrl_suspend+0x0/0x2c returned 0 after 0 usecs
[  856.026346] Disabling non-boot CPUs ...
[  856.027356] CPU1: shutdown
[  856.028382] psci: CPU1 killed (polled 1 ms)
[  856.030309] CPU2: shutdown
[  856.030337] psci: CPU2 killed (polled 0 ms)
[  856.032158] CPU3: shutdown
[  856.033184] psci: CPU3 killed (polled 1 ms)
[  856.035336] CPU4: shutdown
[  856.036361] psci: CPU4 killed (polled 1 ms)
[  856.038089] CPU5: shutdown
[  856.039110] psci: CPU5 killed (polled 1 ms)
[  856.040688] CPU6: shutdown
[  856.041882] psci: CPU6 killed (polled 1 ms)
[  856.046029] CPU7: shutdown
[  856.046039] psci: CPU7 killed (polled 0 ms)
[  856.047187] PM: pm_system_irq_wakeup: 227 triggered chromeos-ec
[  856.047245] Enabling non-boot CPUs ...
[  856.047691] Detected VIPT I-cache on CPU1
[  856.047721] GICv3: CPU1: found redistributor 1 region 0:0x000000000c120000
[  856.047770] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
[  856.048367] CPU1 is up
[  856.048754] Detected VIPT I-cache on CPU2
[  856.048769] GICv3: CPU2: found redistributor 2 region 0:0x000000000c140000
[  856.048790] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
[  856.049120] CPU2 is up
[  856.049454] Detected VIPT I-cache on CPU3
[  856.049469] GICv3: CPU3: found redistributor 3 region 0:0x000000000c160000
[  856.049490] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
[  856.049843] CPU3 is up
[  856.050392] Detected VIPT I-cache on CPU4
[  856.050424] GICv3: CPU4: found redistributor 100 region 0:0x000000000c180000
[  856.050453] arch_timer: CPU4: Trapping CNTVCT access
[  856.050473] CPU4: Booted secondary processor 0x0000000100 [0x410fd092]
[  856.051367] CPU4 is up
[  856.051778] Detected VIPT I-cache on CPU5
[  856.051803] GICv3: CPU5: found redistributor 101 region 0:0x000000000c1a0000
[  856.051825] arch_timer: CPU5: Trapping CNTVCT access
[  856.051841] CPU5: Booted secondary processor 0x0000000101 [0x410fd092]
[  856.052456] CPU5 is up
[  856.052879] Detected VIPT I-cache on CPU6
[  856.052905] GICv3: CPU6: found redistributor 102 region 0:0x000000000c1c0000
[  856.052926] arch_timer: CPU6: Trapping CNTVCT access
[  856.052943] CPU6: Booted secondary processor 0x0000000102 [0x410fd092]
[  856.053548] CPU6 is up
[  856.053880] Detected VIPT I-cache on CPU7
[  856.053906] GICv3: CPU7: found redistributor 103 region 0:0x000000000c1e0000
[  856.053927] arch_timer: CPU7: Trapping CNTVCT access
[  856.053944] CPU7: Booted secondary processor 0x0000000103 [0x410fd092]
[  856.054578] CPU7 is up
[  856.055204] mt8183-pinctrl 10005000.pinctrl: PM: calling mtk_paris_pinctrl_resume+0x0/0x2c @ 10509, parent: soc
[  856.055215] mt8183-pinctrl 10005000.pinctrl: PM: mtk_paris_pinctrl_resume+0x0/0x2c returned 0 after 0 usecs
[  856.055248] i2c-mt65xx 11005000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.055367] i2c-mt65xx 11005000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 106 usecs
[  856.055396] i2c-mt65xx 11007000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.055496] i2c-mt65xx 11007000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 88 usecs
[  856.055516] i2c-mt65xx 11008000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.055617] i2c-mt65xx 11008000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 89 usecs
[  856.055646] i2c-mt65xx 11009000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.055746] i2c-mt65xx 11009000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 88 usecs
[  856.055772] i2c-mt65xx 1100f000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.055889] i2c-mt65xx 1100f000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 104 usecs
[  856.055926] i2c-mt65xx 11011000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.056026] i2c-mt65xx 11011000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 88 usecs
[  856.056048] i2c-mt65xx 11016000.i2c: PM: calling mtk_i2c_resume_noirq+0x0/0x134 @ 10509, parent: soc
[  856.056149] i2c-mt65xx 11016000.i2c: PM: mtk_i2c_resume_noirq+0x0/0x134 returned 0 after 89 usecs
[  856.056304] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: 11220000.audio-controller
[  856.056340] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 25 usecs
[  856.056723] mediatek-mutex 14016000.mutex: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056791] mediatek-mutex 14016000.mutex: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 57 usecs
[  856.056803] mediatek-disp-aal 14010000.aal: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056812] mediatek-disp-aal 14010000.aal: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056822] mediatek-disp-ccorr 1400f000.ccorr: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056831] mediatek-disp-ccorr 1400f000.ccorr: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056842] mediatek-disp-color 1400e000.color: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056861] mediatek-disp-color 1400e000.color: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056872] mediatek-disp-gamma 14011000.gamma: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056881] mediatek-disp-gamma 14011000.gamma: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056895] mediatek-disp-pwm 1100e000.pwm: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056904] mediatek-disp-pwm 1100e000.pwm: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056921] clk-mt8183-mfg 13000000.syscon: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056966] clk-mt8183-mfg 13000000.syscon: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 35 usecs
[  856.056979] mtk-smi-common 14019000.smi: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.056988] mtk-smi-common 14019000.smi: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.056999] mtk-smi-larb 14017000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057007] mtk-smi-larb 14017000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057018] mtk-smi-larb 15021000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057096] mtk-smi-larb 15021000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 67 usecs
[  856.057108] mtk-smi-larb 1502f000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057116] mtk-smi-larb 1502f000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057127] mtk-smi-larb 16010000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057170] mtk-smi-larb 16010000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 32 usecs
[  856.057181] mtk-smi-larb 17010000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057200] mtk-smi-larb 17010000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 9 usecs
[  856.057211] mtk-smi-larb 1a001000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057293] mtk-smi-larb 1a001000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 71 usecs
[  856.057305] mtk-smi-larb 1a002000.larb: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057313] mtk-smi-larb 1a002000.larb: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057324] mediatek-disp-ovl 14008000.ovl: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057333] mediatek-disp-ovl 14008000.ovl: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057343] mediatek-disp-ovl 14009000.ovl: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057351] mediatek-disp-ovl 14009000.ovl: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057361] mediatek-disp-ovl 1400a000.ovl: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057369] mediatek-disp-ovl 1400a000.ovl: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057379] mediatek-disp-rdma 1400b000.rdma: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057388] mediatek-disp-rdma 1400b000.rdma: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057398] mediatek-disp-rdma 1400c000.rdma: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057407] mediatek-disp-rdma 1400c000.rdma: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057424] mtk-dsi 14014000.dsi: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.057432] mtk-dsi 14014000.dsi: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.057444] genpd genpd:0:13040000.mali: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: none
[  856.057919] genpd genpd:0:13040000.mali: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 455 usecs
[  856.057931] genpd genpd:1:13040000.mali: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: none
[  856.057996] genpd genpd:1:13040000.mali: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 54 usecs
[  856.058008] genpd genpd:2:13040000.mali: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: none
[  856.058075] genpd genpd:2:13040000.mali: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 56 usecs
[  856.058149] mediatek-dpi 14015000.dpi: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058159] mediatek-dpi 14015000.dpi: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058224] mtk-mdp3 14001000.mdp3_rdma0: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058233] mtk-mdp3 14001000.mdp3_rdma0: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058278] mtk-cam-dip 15022000.dip: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058287] mtk-cam-dip 15022000.dip: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058306] mtk-fd-4.0 1502b000.fd: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058315] mtk-fd-4.0 1502b000.fd: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058336] mtk-vcodec-enc 17020000.vcodec: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058345] mtk-vcodec-enc 17020000.vcodec: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058356] mtk-jpeg 17030000.venc_jpg: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058365] mtk-jpeg 17030000.venc_jpg: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058376] mtk-vcodec-dec 16000000.vcodec: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058385] mtk-vcodec-dec 16000000.vcodec: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058396] mtk-cam-p1 1a000000.camisp: PM: calling genpd_resume_noirq+0x0/0xe0 @ 10509, parent: soc
[  856.058405] mtk-cam-p1 1a000000.camisp: PM: genpd_resume_noirq+0x0/0xe0 returned 0 after 0 usecs
[  856.058932] i2c i2c-6: PM: calling i2c_resume_early+0x0/0x84 @ 201, parent: 11005000.i2c
[  856.058942] i2c i2c-6: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.058990] i2c i2c-4: PM: calling i2c_resume_early+0x0/0x84 @ 192, parent: 11008000.i2c
[  856.058999] i2c i2c-4: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059040] i2c i2c-2: PM: calling i2c_resume_early+0x0/0x84 @ 10514, parent: 11009000.i2c
[  856.059050] i2c i2c-2: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059068] i2c i2c-5: PM: calling i2c_resume_early+0x0/0x84 @ 192, parent: 11016000.i2c
[  856.059076] i2c i2c-5: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059097] i2c_hid_of 2-002c: PM: calling i2c_resume_early+0x0/0x84 @ 192, parent: i2c-2
[  856.059106] i2c_hid_of 2-002c: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059122] i2c 2-0015: PM: calling i2c_resume_early+0x0/0x84 @ 201, parent: i2c-2
[  856.059130] i2c 2-0015: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059141] dummy 4-0038: PM: calling i2c_resume_early+0x0/0x84 @ 201, parent: i2c-4
[  856.059149] dummy 4-0038: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059155] dummy 4-003d: PM: calling i2c_resume_early+0x0/0x84 @ 9528, parent: i2c-4
[  856.059170] i2c i2c-0: PM: calling i2c_resume_early+0x0/0x84 @ 10510, parent: 11007000.i2c
[  856.059176] dummy 4-003d: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059185] i2c i2c-0: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059192] dummy 4-0039: PM: calling i2c_resume_early+0x0/0x84 @ 9528, parent: i2c-4
[  856.059197] dummy 4-0039: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059205] dummy 4-003f: PM: calling i2c_resume_early+0x0/0x84 @ 9528, parent: i2c-4
[  856.059213] dummy 4-0042: PM: calling i2c_resume_early+0x0/0x84 @ 10510, parent: i2c-4
[  856.059218] dummy 4-003f: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059226] i2c 0-0040: PM: calling i2c_resume_early+0x0/0x84 @ 7, parent: i2c-0
[  856.059232] dummy 4-0042: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059239] dummy 4-002a: PM: calling i2c_resume_early+0x0/0x84 @ 9528, parent: i2c-4
[  856.059243] i2c 0-0040: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059251] dummy 4-002c: PM: calling i2c_resume_early+0x0/0x84 @ 10510, parent: i2c-4
[  856.059256] dummy 4-002a: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059264] dummy 4-002c: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059277] i2c i2c-1: PM: calling i2c_resume_early+0x0/0x84 @ 10517, parent: 11011000.i2c
[  856.059287] i2c i2c-1: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059316] ts3a227e 5-003b: PM: calling i2c_resume_early+0x0/0x84 @ 195, parent: i2c-5
[  856.059325] ts3a227e 5-003b: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059352] i2c i2c-3: PM: calling i2c_resume_early+0x0/0x84 @ 10515, parent: 1100f000.i2c
[  856.059360] i2c i2c-3: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059490] anx7625 4-0058: PM: calling i2c_resume_early+0x0/0x84 @ 192, parent: i2c-4
[  856.059499] anx7625 4-0058: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059662] it6505 3-005c: PM: calling i2c_resume_early+0x0/0x84 @ 10510, parent: i2c-3
[  856.059680] it6505 3-005c: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059691] i2c 0-0010: PM: calling i2c_resume_early+0x0/0x84 @ 10511, parent: i2c-0
[  856.059700] i2c 0-0010: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059750] i2c i2c-13: PM: calling i2c_resume_early+0x0/0x84 @ 10517, parent: 3-005c
[  856.059760] i2c i2c-13: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.059826] mtk-iommu 10205000.iommu: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.059835] mtk-iommu 10205000.iommu: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.059846] mtk-smi-common 14019000.smi: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060027] mtk-smi-common 14019000.smi: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060038] mtk-smi-larb 14017000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060046] mtk-smi-larb 14017000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060055] mtk-smi-larb 15021000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060063] mtk-smi-larb 15021000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060073] mtk-smi-larb 1502f000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060081] mtk-smi-larb 1502f000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060091] mtk-smi-larb 16010000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060099] mtk-smi-larb 16010000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060109] mtk-smi-larb 17010000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060117] mtk-smi-larb 17010000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060126] mtk-smi-larb 1a001000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060134] mtk-smi-larb 1a001000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060144] mtk-smi-larb 1a002000.larb: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10509, parent: soc
[  856.060152] mtk-smi-larb 1a002000.larb: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.060196] i2c i2c-12: PM: calling i2c_resume_early+0x0/0x84 @ 7, parent: 11012000.spi:cros-ec@0:i2c-tunnel
[  856.060206] i2c i2c-12: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.060230] sbs-battery 12-000b: PM: calling i2c_resume_early+0x0/0x84 @ 9528, parent: i2c-12
[  856.060239] sbs-battery 12-000b: PM: i2c_resume_early+0x0/0x84 returned 0 after 0 usecs
[  856.060627] reg-dummy reg-dummy: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060655] reg-dummy reg-dummy: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060670] regulator regulator.0: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: reg-dummy
[  856.060680] regulator regulator.0: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.060695] ramoops ffedb000.ramoops: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060703] ramoops ffedb000.ramoops: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060714] coreboot_table ffed9000.coreboot: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060721] coreboot_table ffed9000.coreboot: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060731] platform firmware:chromeos: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060739] platform firmware:chromeos: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060750] armv8-pmu pmu-a53: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060758] armv8-pmu pmu-a53: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060768] armv8-pmu pmu-a73: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060776] armv8-pmu pmu-a73: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060786] psci-cpuidle-domain psci: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060794] psci-cpuidle-domain psci: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060804] platform fixed-factor-clock-13m: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060812] platform fixed-factor-clock-13m: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060822] platform timer: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060830] platform timer: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060841] platform soc: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.060849] platform soc: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060881] mediatek,efuse 8000000.soc_data: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060889] mediatek,efuse 8000000.soc_data: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060900] clk-mt8183 c530000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060908] clk-mt8183 c530000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060918] clk-mt8183 10000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060926] clk-mt8183 10000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060937] clk-mt8183 10001000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060944] clk-mt8183 10001000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060955] clk-mt8183 10003000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060963] clk-mt8183 10003000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060973] mt8183-pinctrl 10005000.pinctrl: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.060981] mt8183-pinctrl 10005000.pinctrl: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.060992] platform 10006000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061000] platform 10006000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.061010] mtk-wdt 10007000.watchdog: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061021] mtk-wdt 10007000.watchdog: PM: platform_pm_resume+0x0/0x5c returned 0 after 3 usecs
[  856.061031] clk-mt8183 1000c000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061039] clk-mt8183 1000c000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.061049] mt-pmic-pwrap 1000d000.pwrap: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061057] mt-pmic-pwrap 1000d000.pwrap: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.061067] mtk-scp 10500000.scp: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061075] mtk-scp 10500000.scp: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.061086] platform 10017000.timer: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061093] platform 10017000.timer: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.061104] mtk_cmdq 10238000.mailbox: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.061117] mtk_cmdq 10238000.mailbox: PM: platform_pm_resume+0x0/0x5c returned 0 after 4 usecs
[  856.061128] mt6577-auxadc 11001000.auxadc: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062140] mt6577-auxadc 11001000.auxadc: PM: platform_pm_resume+0x0/0x5c returned 0 after 980 usecs
[  856.062152] mt6577-uart 11002000.serial: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062256] mt6577-uart 11002000.serial: PM: platform_pm_resume+0x0/0x5c returned 0 after 92 usecs
[  856.062267] mt6577-uart 11003000.serial: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062362] mt6577-uart 11003000.serial: PM: platform_pm_resume+0x0/0x5c returned 0 after 84 usecs
[  856.062373] i2c-mt65xx 11005000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062382] i2c-mt65xx 11005000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062401] i2c-mt65xx 11007000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062409] i2c-mt65xx 11007000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062426] i2c-mt65xx 11008000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062434] i2c-mt65xx 11008000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062453] i2c-mt65xx 11009000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062460] i2c-mt65xx 11009000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062478] mtk-spi 1100a000.spi: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062497] mtk-spi 1100a000.spi: PM: platform_pm_resume+0x0/0x5c returned 0 after 10 usecs
[  856.062508] mtk-thermal 1100b000.thermal: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062545] mtk-thermal 1100b000.thermal: PM: platform_pm_resume+0x0/0x5c returned 0 after 28 usecs
[  856.062556] platform 11006000.pwm: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062564] platform 11006000.pwm: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062574] i2c-mt65xx 1100f000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062582] i2c-mt65xx 1100f000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062602] mtk-spi 11010000.spi: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062621] mtk-spi 11010000.spi: PM: platform_pm_resume+0x0/0x5c returned 0 after 11 usecs
[  856.062632] i2c-mt65xx 11011000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062639] i2c-mt65xx 11011000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062656] mtk-spi 11012000.spi: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062673] mtk-spi 11012000.spi: PM: platform_pm_resume+0x0/0x5c returned 0 after 8 usecs
[  856.062685] i2c-mt65xx 11016000.i2c: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062692] i2c-mt65xx 11016000.i2c: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062709] clk-mt8183-audio 11220000.audio-controller: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062717] clk-mt8183-audio 11220000.audio-controller: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062727] mediatek-mipi-tx 11e50000.mipi-dphy: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062735] mediatek-mipi-tx 11e50000.mipi-dphy: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062746] mediatek,efuse 11f10000.efuse: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062754] mediatek,efuse 11f10000.efuse: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062764] mtk-tphy soc:usb-phy@11f40000: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062772] mtk-tphy soc:usb-phy@11f40000: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062782] mtk-mmsys 14000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062790] mtk-mmsys 14000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062800] platform 14003000.mdp3_rsz0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062807] platform 14003000.mdp3_rsz0: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062817] platform 14004000.mdp3_rsz1: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062826] platform 14004000.mdp3_rsz1: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062836] platform 14005000.mdp3_wrot0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062844] platform 14005000.mdp3_wrot0: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062862] platform 14006000.mdp3_wdma: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062870] platform 14006000.mdp3_wdma: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062880] platform 14012000.dither: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062891] ts3a227e 5-003b: PM: calling ts3a227e_resume+0x0/0x30 [snd_soc_ts3a227e] @ 198, parent: i2c-5
[  856.062899] ts3a227e 5-003b: PM: ts3a227e_resume+0x0/0x30 [snd_soc_ts3a227e] returned 0 after 2 usecs
[  856.062907] platform 14012000.dither: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062915] i2c_hid_of 2-002c: PM: calling i2c_hid_core_resume+0x0/0xec @ 198, parent: i2c-2
[  856.062927] platform 1401c000.mdp3_ccorr: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062934] platform 1401c000.mdp3_ccorr: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062945] clk-mt8183-img 15020000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062953] clk-mt8183-img 15020000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062963] clk-mt8183-vdec 16000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062971] clk-mt8183-vdec 16000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.062982] clk-mt8183-venc 17000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.062990] clk-mt8183-venc 17000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063001] clk-mt8183-ipu_conn 19000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.063009] clk-mt8183-ipu_conn 19000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063019] clk-mt8183-ipu_adl 19010000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.063027] clk-mt8183-ipu_adl 19010000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063037] clk-mt8183-ipu_core0 19180000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.063046] clk-mt8183-ipu_core0 19180000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063056] clk-mt8183-ipu_core1 19280000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.063064] clk-mt8183-ipu_core1 19280000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063075] clk-mt8183-cam 1a000000.syscon: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.063083] clk-mt8183-cam 1a000000.syscon: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063093] reg-fixed-voltage regulator0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063101] reg-fixed-voltage regulator0: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063111] reg-fixed-voltage regulator1: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063119] reg-fixed-voltage regulator1: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063129] reg-fixed-voltage regulator2: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063136] reg-fixed-voltage regulator2: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063146] reg-fixed-voltage regulator3: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063154] reg-fixed-voltage regulator3: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063165] reg-fixed-voltage regulator4: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063172] reg-fixed-voltage regulator4: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063182] reg-fixed-voltage regulator5: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063190] reg-fixed-voltage regulator5: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063201] reg-fixed-voltage regulator6: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063208] reg-fixed-voltage regulator6: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063219] bt-sco bt-sco: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063227] bt-sco bt-sco: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063238] pwrseq_simple wifi-pwrseq: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063245] pwrseq_simple wifi-pwrseq: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063255] gpio-keys wifi-wakeup: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063272] gpio-keys wifi-wakeup: PM: platform_pm_resume+0x0/0x5c returned 0 after 8 usecs
[  856.063283] reg-fixed-voltage pp1200-mipibrdg: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063291] reg-fixed-voltage pp1200-mipibrdg: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063301] reg-fixed-voltage pp1800-mipibrdg: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063309] reg-fixed-voltage pp1800-mipibrdg: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063319] reg-fixed-voltage pp3300-panel: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063327] reg-fixed-voltage pp3300-panel: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063337] reg-fixed-voltage vddio-mipibrdg: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063345] reg-fixed-voltage vddio-mipibrdg: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063355] gpio-keys volume-buttons: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063369] gpio-keys volume-buttons: PM: platform_pm_resume+0x0/0x5c returned 0 after 6 usecs
[  856.063380] max98357a max98357a: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063388] max98357a max98357a: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063407] regulator regulator.1: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator0
[  856.063416] regulator regulator.1: PM: regulator_resume+0x0/0x104 returned 0 after 1 usecs
[  856.063428] regulator regulator.2: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator1
[  856.063437] regulator regulator.2: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063449] regulator regulator.3: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator2
[  856.063457] regulator regulator.3: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063468] regulator regulator.4: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator3
[  856.063477] regulator regulator.4: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063487] regulator regulator.5: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator4
[  856.063496] regulator regulator.5: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063507] regulator regulator.6: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator5
[  856.063516] regulator regulator.6: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063526] regulator regulator.7: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: regulator6
[  856.063535] regulator regulator.7: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063546] regulator regulator.8: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: pp1200-mipibrdg
[  856.063555] regulator regulator.8: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063567] regulator regulator.9: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: pp1800-mipibrdg
[  856.063575] regulator regulator.9: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063586] regulator regulator.10: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: pp3300-panel
[  856.063595] regulator regulator.10: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063606] regulator regulator.11: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: vddio-mipibrdg
[  856.063615] regulator regulator.11: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063626] platform mtk-socinfo.0.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 8000000.soc_data
[  856.063634] platform mtk-socinfo.0.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063645] mtk-socinfo mtk-socinfo.1.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 11f10000.efuse
[  856.063653] mtk-socinfo mtk-socinfo.1.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063689] mt6397 1000d000.pwrap:mt6358: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 1000d000.pwrap
[  856.063698] mt6397 1000d000.pwrap:mt6358: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063708] clk-mt8183-mm clk-mt8183-mm.2.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 14000000.syscon
[  856.063716] clk-mt8183-mm clk-mt8183-mm.2.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063728] serial8250 serial8250: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.063737] serial8250 serial8250: PM: platform_pm_resume+0x0/0x5c returned 0 after 1 usecs
[  856.063764] hci_uart_qca serial0-0: PM: calling qca_resume+0x0/0x54 [hci_uart] @ 10509, parent: serial0
[  856.063780] hci_uart_qca serial0-0: PM: qca_resume+0x0/0x54 [hci_uart] returned 0 after 0 usecs
[  856.063802] mt6358-regulator mt6358-regulator: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 1000d000.pwrap:mt6358
[  856.063811] mt6358-regulator mt6358-regulator: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.063823] regulator regulator.12: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.063832] regulator regulator.12: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.063843] regulator regulator.13: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064085] anx7625 4-0058: PM: calling pm_runtime_force_resume+0x0/0xb4 @ 10515, parent: i2c-4
[  856.064095] anx7625 4-0058: PM: pm_runtime_force_resume+0x0/0xb4 returned 0 after 0 usecs
[  856.064187] regulator regulator.13: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064218] regulator regulator.14: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064244] regulator regulator.14: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064257] regulator regulator.15: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064266] regulator regulator.15: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064277] regulator regulator.16: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064286] regulator regulator.16: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064297] regulator regulator.17: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064306] regulator regulator.17: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064317] regulator regulator.18: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064326] regulator regulator.18: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064337] regulator regulator.19: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064345] regulator regulator.19: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064356] regulator regulator.20: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064365] regulator regulator.20: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064376] regulator regulator.21: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064385] regulator regulator.21: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064396] regulator regulator.22: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064404] regulator regulator.22: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064416] regulator regulator.23: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064425] regulator regulator.23: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064436] regulator regulator.24: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064445] regulator regulator.24: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064457] regulator regulator.25: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064466] regulator regulator.25: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064477] regulator regulator.26: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064486] regulator regulator.26: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064506] regulator regulator.27: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064515] regulator regulator.27: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064522] mtu3 11201000.usb: PM: calling platform_pm_resume+0x0/0x5c @ 9528, parent: soc
[  856.064532] regulator regulator.28: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064541] regulator regulator.28: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064552] regulator regulator.29: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064561] regulator regulator.29: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064572] regulator regulator.30: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064582] regulator regulator.30: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064587] mtu3 11201000.usb: PM: platform_pm_resume+0x0/0x5c returned 0 after 58 usecs
[  856.064598] regulator regulator.31: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064607] regulator regulator.31: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064612] xhci-mtk 11200000.xhci: PM: calling platform_pm_resume+0x0/0x5c @ 7, parent: 11201000.usb
[  856.064625] regulator regulator.32: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064629] xhci-mtk 11200000.xhci: PM: platform_pm_resume+0x0/0x5c returned 0 after 8 usecs
[  856.064640] regulator regulator.32: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064652] regulator regulator.33: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064660] regulator regulator.33: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064670] usb usb1: PM: calling usb_dev_resume+0x0/0x28 @ 9529, parent: 11200000.xhci
[  856.064678] regulator regulator.34: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064687] regulator regulator.34: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064698] regulator regulator.35: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064707] regulator regulator.35: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064717] regulator regulator.36: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064727] regulator regulator.36: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064737] regulator regulator.37: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064746] regulator regulator.37: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064757] regulator regulator.38: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064765] regulator regulator.38: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064777] regulator regulator.39: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064785] regulator regulator.39: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064796] regulator regulator.40: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064805] regulator regulator.40: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064815] regulator regulator.41: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064824] regulator regulator.41: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064834] regulator regulator.42: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064843] regulator regulator.42: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064883] regulator regulator.43: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064892] regulator regulator.43: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064903] regulator regulator.44: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064912] regulator regulator.44: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064923] regulator regulator.45: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064932] regulator regulator.45: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064943] regulator regulator.46: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064958] usb usb2: PM: calling usb_dev_resume+0x0/0x28 @ 10516, parent: 11200000.xhci
[  856.064971] regulator regulator.46: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.064981] usb usb2: PM: usb_dev_resume+0x0/0x28 returned 0 after 11 usecs
[  856.064990] regulator regulator.47: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.064998] regulator regulator.47: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065007] regulator regulator.48: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.065014] regulator regulator.48: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065023] regulator regulator.49: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.065034] regulator regulator.49: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065046] regulator regulator.50: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.065054] regulator regulator.50: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065066] regulator regulator.51: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.065075] regulator regulator.51: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065086] regulator regulator.52: PM: calling regulator_resume+0x0/0x104 @ 10509, parent: mt6358-regulator
[  856.065095] regulator regulator.52: PM: regulator_resume+0x0/0x104 returned 0 after 0 usecs
[  856.065119] it6505 3-005c: PM: calling it6505_bridge_resume+0x0/0x28 @ 192, parent: i2c-3
[  856.065146] mt6397-rtc mt6358-rtc: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 1000d000.pwrap:mt6358
[  856.065160] mt6397-rtc mt6358-rtc: PM: platform_pm_resume+0x0/0x5c returned 0 after 4 usecs
[  856.065181] tpm_tis_spi spi0.0: PM: calling tpm_tis_spi_resume+0x0/0x38 @ 10509, parent: spi0
[  856.068777] tpm_tis_spi spi0.0: PM: tpm_tis_spi_resume+0x0/0x38 returned 0 after 3501 usecs
[  856.068798] mtd mtd0: PM: calling mtd_cls_resume+0x0/0x64 @ 10509, parent: spi1.0
[  856.068959] mtd mtd0: PM: mtd_cls_resume+0x0/0x64 returned 0 after 147 usecs
[  856.068972] mtd mtd0ro: PM: calling mtd_cls_resume+0x0/0x64 @ 10509, parent: spi1.0
[  856.068980] mtd mtd0ro: PM: mtd_cls_resume+0x0/0x64 returned 0 after 0 usecs
[  856.068998] cros-ec-spi spi2.0: PM: calling cros_ec_spi_resume+0x0/0x28 @ 10509, parent: spi2
[  856.071649] cros-ec-spi spi2.0: PM: cros_ec_spi_resume+0x0/0x28 returned 0 after 2579 usecs
[  856.071661] platform Fixed MDIO bus.0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.071670] platform Fixed MDIO bus.0: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071693] rtc rtc0: PM: calling rtc_resume+0x0/0x140 @ 10509, parent: mt6358-rtc
[  856.071702] rtc rtc0: PM: rtc_resume+0x0/0x140 returned 0 after 0 usecs
[  856.071712] alarmtimer alarmtimer.4.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: rtc0
[  856.071724] alarmtimer alarmtimer.4.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 3 usecs
[  856.071745] mtk-cpufreq mtk-cpufreq: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.071753] mtk-cpufreq mtk-cpufreq: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071767] psci-cpuidle psci-cpuidle: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.071775] psci-cpuidle psci-cpuidle: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071810] mtk-msdc 11240000.mmc: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.071819] mtk-msdc 11240000.mmc: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071841] mtk-msdc 11230000.mmc: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.071866] mtk-msdc 11230000.mmc: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071890] mediatek-cci-devfreq cci: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.071898] mediatek-cci-devfreq cci: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071913] cros-ec-dev cros-ec-dev.5.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: spi2.0
[  856.071928] mmcblk mmc0:0001: PM: calling mmc_bus_resume+0x0/0x6c @ 10510, parent: mmc0
[  856.071940] cros-ec-dev cros-ec-dev.5.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071950] mmcblk mmc0:0001: PM: mmc_bus_resume+0x0/0x6c returned 0 after 10 usecs
[  856.071963] snd-soc-dummy snd-soc-dummy: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.071971] snd-soc-dummy snd-soc-dummy: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.071986] cros-usbpd-charger cros-usbpd-charger.6.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072004] cros-usbpd-charger cros-usbpd-charger.6.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 9 usecs
[  856.072020] cros-usbpd-logger cros-usbpd-logger.7.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072030] cros-usbpd-logger cros-usbpd-logger.7.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 2 usecs
[  856.072042] cros-usbpd-notify cros-usbpd-notify.8.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072051] cros-usbpd-notify cros-usbpd-notify.8.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072061] cros-ec-chardev cros-ec-chardev.9.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072070] cros-ec-chardev cros-ec-chardev.9.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072082] cros-ec-debugfs cros-ec-debugfs.10.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072092] cros-ec-debugfs cros-ec-debugfs.10.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 1 usecs
[  856.072103] platform cros-ec-lightbar.11.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072111] platform cros-ec-lightbar.11.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072123] cros-ec-pd-sysfs cros-ec-pd-sysfs.12.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072131] cros-ec-pd-sysfs cros-ec-pd-sysfs.12.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072145] amba d410000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072153] amba d410000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072164] amba d510000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072172] amba d510000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072183] amba d610000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072191] amba d610000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072202] cros-ec-sysfs cros-ec-sysfs.13.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072210] cros-ec-sysfs cros-ec-sysfs.13.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072221] amba d710000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072229] amba d710000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072240] cros-ec-pd-update cros-ec-pd-update.14.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072250] cros-ec-pd-update cros-ec-pd-update.14.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 2 usecs
[  856.072262] amba d810000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072270] amba d810000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072282] amba d910000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072290] amba d910000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072301] amba da10000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072309] amba da10000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072319] amba db10000.cpu-debug: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: soc
[  856.072327] amba db10000.cpu-debug: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.072339] mtk-power-controller 10006000.syscon:power-controller: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 10006000.syscon
[  856.072347] mtk-power-controller 10006000.syscon:power-controller: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072370] generic-adc-thermal thermal-sensor1: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.072379] generic-adc-thermal thermal-sensor1: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072390] generic-adc-thermal thermal-sensor2: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.072397] generic-adc-thermal thermal-sensor2: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072415] pwm pwmchip0: PM: calling pwm_class_resume+0x0/0x13c @ 10509, parent: 1100e000.pwm
[  856.072425] pwm pwmchip0: PM: pwm_class_resume+0x0/0x13c returned 0 after 1 usecs
[  856.072437] pwm-backlight backlight_lcd0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.072447] pwm-backlight backlight_lcd0: PM: platform_pm_resume+0x0/0x5c returned 0 after 2 usecs
[  856.072460] backlight backlight_lcd0: PM: calling backlight_resume+0x0/0x94 @ 10509, parent: backlight_lcd0
[  856.072469] backlight backlight_lcd0: PM: backlight_resume+0x0/0x94 returned 0 after 0 usecs
[  856.072482] mtk-iommu 10205000.iommu: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.072490] mtk-iommu 10205000.iommu: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072535] panel-edp panel: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.072544] panel-edp panel: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072556] platform cros-ec-pchg.15.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.072564] platform cros-ec-pchg.15.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.072576] mali 13040000.mali: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.072605] mmc mmc1:0001: PM: calling mmc_bus_resume+0x0/0x6c @ 9, parent: mmc1
[  856.073318] mali 13040000.mali: PM: platform_pm_resume+0x0/0x5c returned 0 after 715 usecs
[  856.073340] platform cros-ec-throttler.16.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.5.auto
[  856.073348] platform cros-ec-throttler.16.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.073360] cros-ec-i2c-tunnel 11012000.spi:cros-ec@0:i2c-tunnel: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: spi2.0
[  856.073368] cros-ec-i2c-tunnel 11012000.spi:cros-ec@0:i2c-tunnel: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.073393] input input0: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: wifi-wakeup
[  856.073409] input input0: PM: input_dev_resume+0x0/0x50 returned 0 after 6 usecs
[  856.073422] input input1: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: volume-buttons
[  856.073431] input input1: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.073591] extcon-usbc-cros-ec 11012000.spi:cros-ec@0:extcon0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: spi2.0
[  856.078415] extcon-usbc-cros-ec 11012000.spi:cros-ec@0:extcon0: PM: platform_pm_resume+0x0/0x5c returned 0 after 4700 usecs
[  856.117062] usb usb1: PM: usb_dev_resume+0x0/0x28 returned 0 after 51151 usecs
[  856.117306] usb 1-1: PM: calling usb_dev_resume+0x0/0x28 @ 10511, parent: usb1
[  856.128012] it6505 3-005c: PM: it6505_bridge_resume+0x0/0x28 returned 0 after 61407 usecs
[  856.128046] hdmi-audio-codec hdmi-audio-codec.17.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 3-005c
[  856.128055] hdmi-audio-codec hdmi-audio-codec.17.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.128067] mtk-svs 1100b000.svs: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: soc
[  856.128107]  SVSB_CPU_LITTLE: svs_init02_isr_handler: VOP74~30:0x1b232b32~0x363a3e44, DC:0x00000000
[  856.128228]  SVSB_CPU_BIG: svs_init02_isr_handler: VOP74~30:0x1c252d34~0x393e4348, DC:0x00000000
[  856.128277]  SVSB_CCI: svs_init02_isr_handler: VOP74~30:0x1d232b32~0x373b4247, DC:0x00000138
[  856.128406]  SVSB_GPU: svs_init02_isr_handler: VOP74~30:0x181a1c1e~0x2125282c, DC:0x00000108
[  856.128464] mtk-svs 1100b000.svs: PM: platform_pm_resume+0x0/0x5c returned 0 after 378 usecs
[  856.128480] cros-ec-typec 11012000.spi:cros-ec@0:typec: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: spi2.0
[  856.128493] cros-ec-typec 11012000.spi:cros-ec@0:typec: PM: platform_pm_resume+0x0/0x5c returned 0 after 4 usecs
[  856.128505] cros-ec-keyb 11012000.spi:cros-ec@0:keyboard-controller: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: spi2.0
[  856.130616] cros-ec-keyb 11012000.spi:cros-ec@0:keyboard-controller: PM: platform_pm_resume+0x0/0x5c returned 0 after 2051 usecs
[  856.130630] input input2: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: 11012000.spi:cros-ec@0:keyboard-controller
[  856.130640] input input2: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.130653] input input3: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: 11012000.spi:cros-ec@0:keyboard-controller
[  856.130662] input input3: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.130680] mipi-dsi 14014000.dsi.0: PM: calling pm_generic_resume+0x0/0x44 @ 10509, parent: 14014000.dsi
[  856.130688] mipi-dsi 14014000.dsi.0: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.130703] mediatek-drm mediatek-drm.3.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 14000000.syscon
[  856.130806] mediatek-drm mediatek-drm.3.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 92 usecs
[  856.131898] usb 1-1: PM: usb_dev_resume+0x0/0x28 returned 0 after 14220 usecs
[  856.132062] usb 1-1.3: PM: calling usb_dev_resume+0x0/0x28 @ 9531, parent: 1-1
[  856.137224] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
[  856.139535] i2c_hid_of 2-002c: PM: i2c_hid_core_resume+0x0/0xec returned 0 after 74814 usecs
[  856.139776] input input6: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: 0018:06CB:CDB5.0001
[  856.139786] input input6: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.139811] platform regulatory.0: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.139820] platform regulatory.0: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.139849] rfkill rfkill0: PM: calling rfkill_resume+0x0/0x88 @ 10509, parent: hci0
[  856.139874] rfkill rfkill0: PM: rfkill_resume+0x0/0x88 returned 0 after 7 usecs
[  856.139895] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: PM: calling cros_ec_rpmsg_resume+0x0/0x28 [cros_ec_rpmsg] @ 10509, parent: 10500000.scp
[  856.140103] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: PM: cros_ec_rpmsg_resume+0x0/0x28 [cros_ec_rpmsg] returned 0 after 192 usecs
[  856.140129] mtk-mdp3 14001000.mdp3_rdma0: PM: calling mdp_resume+0x0/0x64 [mtk_mdp3] @ 10509, parent: soc
[  856.140137] mtk-mdp3 14001000.mdp3_rdma0: resume enter : stage flag 1st 0, 2nd 0
[  856.140143] mtk-mdp3 14001000.mdp3_rdma0: resume done : stage flag 1st 0, 2nd 0
[  856.140157] mtk-mdp3 14001000.mdp3_rdma0: PM: mdp_resume+0x0/0x64 [mtk_mdp3] returned 0 after 13 usecs
[  856.140170] mt8183_mt6358_ts3a227 mt8183-sound: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: platform
[  856.140179] mt8183_mt6358_ts3a227 mt8183-sound: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140212] mt6358-sound mt6358-sound: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 1000d000.pwrap:mt6358
[  856.140220] mt6358-sound mt6358-sound: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140270] input input7: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: card0
[  856.140279] input input7: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.140293] input input8: PM: calling input_dev_resume+0x0/0x50 @ 10509, parent: card0
[  856.140302] input input8: PM: input_dev_resume+0x0/0x50 returned 0 after 0 usecs
[  856.140322] mtk-cam-dip 15022000.dip: PM: calling mtk_dip_pm_resume+0x0/0xb4 [mtk_dip] @ 10509, parent: soc
[  856.140333] mtk-cam-dip 15022000.dip: PM: mtk_dip_pm_resume+0x0/0xb4 [mtk_dip] returned 0 after 0 usecs
[  856.140360] mtk-fd-4.0 1502b000.fd: PM: calling mtk_fd_resume+0x0/0xb8 [mtk_fd] @ 10509, parent: soc
[  856.140370] mtk-fd-4.0 1502b000.fd: PM: mtk_fd_resume+0x0/0xb8 [mtk_fd] returned 0 after 0 usecs
[  856.140407] mtk-jpeg 17030000.venc_jpg: PM: calling mtk_jpeg_resume+0x0/0x48 [mtk_jpeg] @ 10509, parent: soc
[  856.140420] mtk-jpeg 17030000.venc_jpg: PM: mtk_jpeg_resume+0x0/0x48 [mtk_jpeg] returned 0 after 3 usecs
[  856.140444] mtk-cam-p1 1a000000.camisp: PM: calling mtk_isp_pm_resume+0x0/0xb4 [mtk_cam_isp] @ 10509, parent: soc
[  856.140455] mtk-cam-p1 1a000000.camisp: PM: mtk_isp_pm_resume+0x0/0xb4 [mtk_cam_isp] returned 0 after 0 usecs
[  856.140480] cros-ec-dev cros-ec-dev.18.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: 10500000.scp.cros-ec-rpmsg.13.-1
[  856.140488] cros-ec-dev cros-ec-dev.18.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140500] cros-ec-chardev cros-ec-chardev.19.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140508] cros-ec-chardev cros-ec-chardev.19.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140521] cros-ec-debugfs cros-ec-debugfs.20.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140534] cros-ec-debugfs cros-ec-debugfs.20.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 4 usecs
[  856.140545] platform cros-ec-lightbar.21.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140554] platform cros-ec-lightbar.21.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140565] cros-ec-pd-sysfs cros-ec-pd-sysfs.22.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140573] cros-ec-pd-sysfs cros-ec-pd-sysfs.22.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140584] cros-ec-sysfs cros-ec-sysfs.23.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140592] cros-ec-sysfs cros-ec-sysfs.23.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140604] cros-ec-pd-update cros-ec-pd-update.24.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140615] cros-ec-pd-update cros-ec-pd-update.24.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 2 usecs
[  856.140626] platform cros-ec-pchg.25.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140634] platform cros-ec-pchg.25.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.140646] platform cros-ec-throttler.26.auto: PM: calling platform_pm_resume+0x0/0x5c @ 10509, parent: cros-ec-dev.18.auto
[  856.140654] platform cros-ec-throttler.26.auto: PM: platform_pm_resume+0x0/0x5c returned 0 after 0 usecs
[  856.145124] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
[  856.148300] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
[  856.148939] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
[  856.151627] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
[  856.152672] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
[  856.152693] mmc mmc1:0001: PM: mmc_bus_resume+0x0/0x6c returned 0 after 78189 usecs
[  856.152823] ath10k_sdio mmc1:0001:1: PM: calling pm_generic_resume+0x0/0x44 @ 10514, parent: mmc1:0001
[  856.152833] ath10k_sdio mmc1:0001:1: PM: pm_generic_resume+0x0/0x44 returned 0 after 0 usecs
[  856.153143] ieee80211 phy0: PM: calling wiphy_resume+0x0/0x1b4 [cfg80211] @ 10519, parent: mmc1:0001:1
[  856.186919] usb 1-1.3: PM: usb_dev_resume+0x0/0x28 returned 0 after 53557 usecs
[  856.518356] ieee80211 phy0: PM: wiphy_resume+0x0/0x1b4 [cfg80211] returned 0 after 356536 usecs
[  856.518395] rfkill rfkill1: PM: calling rfkill_resume+0x0/0x88 @ 10509, parent: phy0
[  856.518411] rfkill rfkill1: PM: rfkill_resume+0x0/0x88 returned 0 after 5 usecs
[  856.520330] OOM killer enabled.
[  856.520341] Restarting tasks ... done.
[  856.535027] Resume caused by IRQ 227, chromeos-ec
[  856.535046] PM: suspend exit
[  856.590627] mtk-msdc 11230000.mmc: phase: [map:ffffff3f] [maxlen:24] [final:20]
[  860.228623] wlan0: authenticate with 84:17:ef:e4:dc:b6
[  860.282576] wlan0: send auth to 84:17:ef:e4:dc:b6 (try 1/3)
[  860.283650] wlan0: authenticated
[  860.284870] wlan0: associate with 84:17:ef:e4:dc:b6 (try 1/3)
[  860.288843] wlan0: RX AssocResp from 84:17:ef:e4:dc:b6 (capab=0x1511 status=0 aid=7)
[  860.293183] wlan0: associated
[  860.362042] wlan0: dropped frame to 84:17:ef:e4:dc:b6 (unauthorized port)
[  872.680016] tun: Universal TUN/TAP device driver, 1.6
[  872.695764] udevd[10874]: Using default interface naming scheme 'v249'.
[  872.696241] udevd[10877]: Using default interface naming scheme 'v249'.
[  872.698500] udevd[10878]: Using default interface naming scheme 'v249'.
[  872.700944] udevd[10873]: Using default interface naming scheme 'v249'.
[  872.705929] udevd[10881]: Using default interface naming scheme 'v249'.
[  872.709503] udevd[10885]: Using default interface naming scheme 'v249'.
[  872.764660] arcbr0: port 1(vmtap0) entered blocking state
[  872.764686] arcbr0: port 1(vmtap0) entered disabled state
[  872.764958] device vmtap0 entered promiscuous mode
[  872.778382] arc_wlan0: port 1(vmtap5) entered blocking state
[  872.778463] arc_wlan0: port 1(vmtap5) entered disabled state
[  872.778752] device vmtap5 entered promiscuous mode
[  872.778912] arc_wlan0: port 1(vmtap5) entered blocking state
[  872.778920] arc_wlan0: port 1(vmtap5) entered forwarding state
[  872.883853] arcbr0: port 1(vmtap0) entered blocking state
[  872.883885] arcbr0: port 1(vmtap0) entered forwarding state
[  872.913398] IPv6: ADDRCONF(NETDEV_CHANGE): veth2: link becomes ready
[  872.999278] EXT4-fs (loop9): Using encoding defined by superblock: utf8-12.1.0 with flags 0x0
[  873.000617] EXT4-fs (loop9): mounted filesystem without journal. Opts: noload
[  951.341151] init: ui_stop_waiter main process (11702) killed by TERM signal
[  951.341603] init: shill_stop_waiter main process (11720) killed by TERM signal
[  951.375599] wlan0: deauthenticating from 84:17:ef:e4:dc:b6 by local choice (Reason: 3=DEAUTH_LEAVING)
[  951.575488] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
[  951.583111] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
[  951.586463] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
[  951.587153] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
[  951.589782] mtk-msdc 11240000.mmc: phase: [map:ff80003f] [maxlen:9] [final:27]
[  951.590741] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
[  954.153367] arc_wlan0: port 1(vmtap5) entered disabled state
[  954.242234] device vmtap5 left promiscuous mode
[  954.242347] arc_wlan0: port 1(vmtap5) entered disabled state
[  954.267166] arcbr0: port 1(vmtap0) entered disabled state
[  954.269182] device vmtap0 left promiscuous mode
[  954.269352] arcbr0: port 1(vmtap0) entered disabled state
[  955.555619] init: Sending KILL signal to vhost_user_starter main process (3856)
[  955.557952] init: vhost_user_starter main process (3856) killed by KILL signal
[  957.097477] audit: type=1300 audit(1740769824.271:580): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed9794c0 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.102816] audit: type=1300 audit(1740769824.276:581): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed9794c0 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.113398] init: powerd main process (1033) killed by TERM signal
[  957.114652] audit: type=1300 audit(1740769824.288:582): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5653efd a1=0 a2=5bed995d68 a3=5bed995d68 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.114742] audit: type=1300 audit(1740769824.288:583): arch=c00000b7 syscall=279 success=yes exit=21 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed9997a0 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.115225] init: btmanagerd main process (1164) terminated with status 143
[  957.118314] init: secanomalyd main process (1665) terminated with status 143
[  957.119578] init: cras main process (1700) terminated with status 143
[  957.123679] audit: type=1300 audit(1740769824.297:584): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5653efd a1=0 a2=5bed995d68 a3=5bed995d68 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.125065] audit: type=1300 audit(1740769824.297:585): arch=c00000b7 syscall=279 success=yes exit=21 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed97e830 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.131675] init: resourced main process (3229) killed by TERM signal
[  957.135788] init: timberslide-watcher (/sys/kernel/debug/cros_scp/console_log) main process (3372) killed by TERM signal
[  957.139084] init: traced_probes main process (3598) killed by TERM signal
[  957.150275] init: traced main process (3176) killed by TERM signal
[  957.161840] audit: type=1300 audit(1740769824.335:586): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed99de10 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.169938] audit: type=1300 audit(1740769824.343:587): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed9794c0 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.177565] audit: type=1300 audit(1740769824.351:588): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5652c98 a1=0 a2=5be5652c98 a3=5bed9794c0 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.184356] audit: type=1300 audit(1740769824.358:589): arch=c00000b7 syscall=279 success=yes exit=20 a0=5be5653efd a1=0 a2=5bed995d68 a3=5bed995d68 items=0 ppid=1 pid=1825 auid=4294967295 uid=284 gid=284 euid=284 suid=284 fsuid=284 egid=284 sgid=284 fsgid=284 tty=(none) ses=4294967295 comm="patchpaneld" exe="/usr/bin/patchpaneld" subj=u:r:minijail:s0 key=(null)
[  957.269123] init: cryptohomed-client main process (11925) terminated with status 1
[  957.280386] init: cryptohomed main process (1386) killed by TERM signal
[  957.365962] zram0: detected capacity change from 8136663040 to 0
[  957.387997] device-mapper: ioctl: remove_all left 2 open device(s)
[  957.388013] device-mapper: ioctl: remove_all left 2 open device(s)
[  957.898331] init: console-ttyS0 main process (637) killed by TERM signal
[  957.932196] EXT4-fs (dm-0): re-mounted. Opts: 
[  958.168312] INFO crash_reporter: [unclean_shutdown_collector.cc(167)] Clean shutdown signalled
[  958.170116] INFO crash_reporter: [user_collector.cc(209)] Disabling user crash handling
[  958.170292] Unsafe core_pattern used with fs.suid_dumpable=2.
[  958.170292] Pipe handler or fully qualified core dump path required.
[  958.170292] Set kernel.core_pattern before fs.suid_dumpable.
[  962.628475] kvm: exiting hardware virtualization
[  962.850270] reboot: Restarting system

