<6>[    0.000000] Booting Linux on physical CPU 0x0000000000 [0x410fd034]
<5>[    0.000000] Linux version 5.10.230-25844-gdc65f732bf53 (cros-kernel@chromium.org) (Chromium OS 19.0_pre530567 clang version 19.0.0git (/mnt/host/source/src/third_party/llvm-project 3b5e7c83a6e226d5bd7ed2e9b67449b64812074c), LLD 19.0.0) #1 SMP PREEMPT Thu, 2 Jan 2025 01:16:47 -0800
<5>[    0.000000] random: crng init done
<6>[    0.000000] Machine model: Google kenzo sku17 board
<6>[    0.000000] Reserved memory: created DMA memory pool at 0x0000000050000000, size 41 MiB
<6>[    0.000000] OF: reserved mem: initialized node memory@50000000, compatible id shared-dma-pool
<6>[    0.000000] Zone ranges:
<6>[    0.000000]   DMA      [mem 0x0000000040000000-0x00000000ffffffff]
<6>[    0.000000]   DMA32    empty
<6>[    0.000000]   Normal   [mem 0x0000000100000000-0x000000013fffffff]
<6>[    0.000000] Movable zone start for each node
<6>[    0.000000] Early memory node ranges
<6>[    0.000000]   node   0: [mem 0x0000000040000000-0x000000004fffffff]
<6>[    0.000000]   node   0: [mem 0x0000000050000000-0x00000000528fffff]
<6>[    0.000000]   node   0: [mem 0x0000000052900000-0x00000000545fffff]
<6>[    0.000000]   node   0: [mem 0x0000000054700000-0x00000000ffdfffff]
<6>[    0.000000]   node   0: [mem 0x0000000100000000-0x000000013fffffff]
<6>[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000013fffffff]
<7>[    0.000000] On node 0 totalpages: 1047808
<7>[    0.000000]   DMA zone: 12288 pages used for memmap
<7>[    0.000000]   DMA zone: 0 pages reserved
<7>[    0.000000]   DMA zone: 785664 pages, LIFO batch:63
<7>[    0.000000]   Normal zone: 4096 pages used for memmap
<7>[    0.000000]   Normal zone: 262144 pages, LIFO batch:63
<6>[    0.000000] On node 0, zone DMA: 256 pages in unavailable ranges
<6>[    0.000000] On node 0, zone Normal: 512 pages in unavailable ranges
<6>[    0.000000] psci: probing for conduit method from DT.
<6>[    0.000000] psci: PSCIv1.1 detected in firmware.
<6>[    0.000000] psci: Using standard PSCI v0.2 function IDs
<6>[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
<6>[    0.000000] psci: SMC Calling Convention v1.2
<6>[    0.000000] percpu: Embedded 32 pages/cpu s93592 r8192 d29288 u131072
<7>[    0.000000] pcpu-alloc: s93592 r8192 d29288 u131072 alloc=32*4096
<7>[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 [0] 4 [0] 5 [0] 6 [0] 7 
<6>[    0.000000] Detected VIPT I-cache on CPU0
<6>[    0.000000] CPU features: detected: ARM erratum 845719
<6>[    0.000000] CPU features: detected: GIC system register CPU interface
<6>[    0.000000] CPU features: kernel page table isolation forced ON by KASLR
<6>[    0.000000] CPU features: detected: Kernel page table isolation (KPTI)
<6>[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031424
<5>[    0.000000] Kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
<6>[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes, linear)
<6>[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes, linear)
<6>[    0.000000] mem auto-init: stack:all(zero), heap alloc:on, heap free:off
<6>[    0.000000] software IO TLB: mapped [mem 0x00000000fbe00000-0x00000000ffe00000] (64MB)
<6>[    0.000000] Memory: 3971572K/4191232K available (13758K kernel code, 2436K rwdata, 9280K rodata, 1408K init, 1075K bss, 219660K reserved, 0K cma-reserved)
<6>[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=8, Nodes=1
<6>[    0.000000] ftrace: allocating 40629 entries in 159 pages
<6>[    0.000000] ftrace: allocated 159 pages with 6 groups
<6>[    0.000000] rcu: Preemptible hierarchical RCU implementation.
<6>[    0.000000] 	Trampoline variant of Tasks RCU enabled.
<6>[    0.000000] 	Rude variant of Tasks RCU enabled.
<6>[    0.000000] 	Tracing variant of Tasks RCU enabled.
<6>[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 100 jiffies.
<6>[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
<6>[    0.000000] GIC: enabling workaround for GICv3: Mediatek Chromebook GICR save problem
<6>[    0.000000] GICv3: GIC: Using split EOI/Deactivate mode
<6>[    0.000000] GICv3: 640 SPIs implemented
<6>[    0.000000] GICv3: 0 Extended SPIs implemented
<6>[    0.000000] GICv3: Distributor has no Range Selector support
<6>[    0.000000] GICv3: 16 PPIs implemented
<6>[    0.000000] GICv3: CPU0: found redistributor 0 region 0:0x000000000c100000
<6>[    0.000000] GICv3: GIC: PPI partition interrupt-partition-0[0] { /cpus/cpu@0[0] /cpus/cpu@1[1] /cpus/cpu@2[2] /cpus/cpu@3[3] }
<6>[    0.000000] GICv3: GIC: PPI partition interrupt-partition-1[1] { /cpus/cpu@100[4] /cpus/cpu@101[5] /cpus/cpu@102[6] /cpus/cpu@103[7] }
<6>[    0.000000] rcu: 	Offload RCU callbacks from CPUs: 0-7.
<6>[    0.000000] kfence: initialized - using 2097152 bytes for 255 objects at 0x(____ptrval____)-0x(____ptrval____)
<6>[    0.000000] arch_timer: cp15 timer(s) running at 13.00MHz (phys).
<6>[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x2ff89eacb, max_idle_ns: 440795202429 ns
<6>[    0.000002] sched_clock: 56 bits at 13MHz, resolution 76ns, wraps every 4398046511101ns
<6>[    0.000354] Calibrating delay loop (skipped), value calculated using timer frequency.. 26.00 BogoMIPS (lpj=13000)
<6>[    0.000361] pid_max: default: 32768 minimum: 301
<6>[    0.000440] LSM: Security Framework initializing
<6>[    0.000472] landlock: Up and running.
<6>[    0.000475] Yama: becoming mindful.
<6>[    0.000486] LoadPin: ready to pin (currently enforcing)
<6>[    0.000502] Chromium OS LSM: enabled
<6>[    0.000505] SELinux:  Initializing.
<6>[    0.000549] LSM support for eBPF active
<6>[    0.000585] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
<6>[    0.000599] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
<6>[    0.001969] rcu: Hierarchical SRCU implementation.
<6>[    0.002633] smp: Bringing up secondary CPUs ...
<6>[    0.003244] Detected VIPT I-cache on CPU1
<6>[    0.003268] GICv3: CPU1: found redistributor 1 region 0:0x000000000c120000
<6>[    0.003297] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
<6>[    0.003920] Detected VIPT I-cache on CPU2
<6>[    0.003931] GICv3: CPU2: found redistributor 2 region 0:0x000000000c140000
<6>[    0.003942] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
<6>[    0.004517] Detected VIPT I-cache on CPU3
<6>[    0.004526] GICv3: CPU3: found redistributor 3 region 0:0x000000000c160000
<6>[    0.004537] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
<6>[    0.005225] CPU features: detected: ARM erratum 858921
<6>[    0.005231] CPU features: detected: Spectre-v2
<6>[    0.005237] CPU features: detected: Spectre-BHB
<6>[    0.005242] Detected VIPT I-cache on CPU4
<6>[    0.005257] GICv3: CPU4: found redistributor 100 region 0:0x000000000c180000
<6>[    0.005263] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.005271] arch_timer: CPU4: Trapping CNTVCT access
<6>[    0.005281] CPU4: Booted secondary processor 0x0000000100 [0x410fd092]
<6>[    0.005823] Detected VIPT I-cache on CPU5
<6>[    0.005836] GICv3: CPU5: found redistributor 101 region 0:0x000000000c1a0000
<6>[    0.005841] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.005846] arch_timer: CPU5: Trapping CNTVCT access
<6>[    0.005852] CPU5: Booted secondary processor 0x0000000101 [0x410fd092]
<6>[    0.006424] Detected VIPT I-cache on CPU6
<6>[    0.006436] GICv3: CPU6: found redistributor 102 region 0:0x000000000c1c0000
<6>[    0.006442] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.006447] arch_timer: CPU6: Trapping CNTVCT access
<6>[    0.006453] CPU6: Booted secondary processor 0x0000000102 [0x410fd092]
<6>[    0.007025] Detected VIPT I-cache on CPU7
<6>[    0.007037] GICv3: CPU7: found redistributor 103 region 0:0x000000000c1e0000
<6>[    0.007043] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.007048] arch_timer: CPU7: Trapping CNTVCT access
<6>[    0.007054] CPU7: Booted secondary processor 0x0000000103 [0x410fd092]
<6>[    0.007125] smp: Brought up 1 node, 8 CPUs
<6>[    0.007164] SMP: Total of 8 processors activated.
<6>[    0.007168] CPU features: detected: 32-bit EL0 Support
<6>[    0.007172] CPU features: detected: CRC32 instructions
<6>[    0.007175] CPU features: detected: 32-bit EL1 Support
<6>[    0.007318] CPU features: emulated: Privileged Access Never (PAN) using TTBR0_EL1 switching
<6>[    0.020713] CPU: All CPU(s) started at EL2
<6>[    0.020743] alternatives: patching kernel code
<6>[    0.021950] devtmpfs: initialized
<6>[    0.027467] KASLR enabled
<6>[    0.027602] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
<6>[    0.027628] futex hash table entries: 2048 (order: 5, 131072 bytes, linear)
<6>[    0.027800] pinctrl core: initialized pinctrl subsystem
<6>[    0.028159] NET: Registered protocol family 16
<6>[    0.028858] DMA: preallocated 512 KiB GFP_KERNEL pool for atomic allocations
<6>[    0.029065] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
<6>[    0.029269] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
<6>[    0.029292] audit: initializing netlink subsys (disabled)
<5>[    0.029401] audit: type=2000 audit(0.029:1): state=initialized audit_enabled=0 res=1
<6>[    0.029600] thermal_sys: Registered thermal governor 'step_wise'
<6>[    0.029603] thermal_sys: Registered thermal governor 'user_space'
<6>[    0.029607] thermal_sys: Registered thermal governor 'power_allocator'
<4>[    0.030072] thermal thermal_zone7: power_allocator: sustainable_power will be estimated
<4>[    0.030117] thermal thermal_zone8: power_allocator: sustainable_power will be estimated
<6>[    0.030206] cpuidle: using governor ladder
<6>[    0.030290] cpuidle: using governor menu
<6>[    0.030304] cpuidle: using governor teo
<6>[    0.030487] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
<6>[    0.030593] ASID allocator initialised with 32768 entries
<6>[    0.032713] printk: console [ramoops-1] enabled
<6>[    0.032830] pstore: Registered ramoops as persistent store backend
<6>[    0.032836] ramoops: using 0x100000@0xffedb000, ecc: 0
<7>[    0.089664] gpiochip_find_base: found new base at 320
<7>[    0.089702] gpio gpiochip0: (pinctrl_paris): created GPIO range 0->191 ==> 10005000.pinctrl PIN 0->191
<7>[    0.089958] gpio gpiochip0: (pinctrl_paris): added GPIO chardev (254:0)
<7>[    0.090004] gpio gpiochip0: registered GPIOs 320 to 511 on pinctrl_paris
<6>[    0.098911] cryptd: max_cpu_qlen set to 1000
<7>[    0.100397] reg-fixed-voltage regulator0: GPIO lookup for consumer (null)
<7>[    0.100402] reg-fixed-voltage regulator0: using device tree for GPIO lookup
<7>[    0.100417] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator0[0]'
<7>[    0.100441] of_get_named_gpiod_flags: parsed 'gpio' property of node '/regulator0[0]' - status (0)
<7>[    0.100461] gpio gpiochip0: Persistence not supported for GPIO 178
<7>[    0.100594] reg-fixed-voltage regulator1: GPIO lookup for consumer (null)
<7>[    0.100598] reg-fixed-voltage regulator1: using device tree for GPIO lookup
<7>[    0.100605] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator1[0]'
<7>[    0.100612] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator1[0]'
<7>[    0.100617] reg-fixed-voltage regulator1: using lookup tables for GPIO lookup
<7>[    0.100621] reg-fixed-voltage regulator1: No GPIO consumer (null) found
<7>[    0.100715] reg-fixed-voltage regulator2: GPIO lookup for consumer (null)
<7>[    0.100718] reg-fixed-voltage regulator2: using device tree for GPIO lookup
<7>[    0.100725] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator2[0]'
<7>[    0.100732] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator2[0]'
<7>[    0.100736] reg-fixed-voltage regulator2: using lookup tables for GPIO lookup
<7>[    0.100739] reg-fixed-voltage regulator2: No GPIO consumer (null) found
<7>[    0.100829] reg-fixed-voltage regulator3: GPIO lookup for consumer (null)
<7>[    0.100832] reg-fixed-voltage regulator3: using device tree for GPIO lookup
<7>[    0.100839] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator3[0]'
<7>[    0.100846] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator3[0]'
<7>[    0.100850] reg-fixed-voltage regulator3: using lookup tables for GPIO lookup
<7>[    0.100853] reg-fixed-voltage regulator3: No GPIO consumer (null) found
<7>[    0.100941] reg-fixed-voltage regulator4: GPIO lookup for consumer (null)
<7>[    0.100944] reg-fixed-voltage regulator4: using device tree for GPIO lookup
<7>[    0.100953] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator4[0]'
<7>[    0.100960] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator4[0]'
<7>[    0.100964] reg-fixed-voltage regulator4: using lookup tables for GPIO lookup
<7>[    0.100967] reg-fixed-voltage regulator4: No GPIO consumer (null) found
<7>[    0.101064] reg-fixed-voltage regulator5: GPIO lookup for consumer (null)
<7>[    0.101067] reg-fixed-voltage regulator5: using device tree for GPIO lookup
<7>[    0.101074] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator5[0]'
<7>[    0.101080] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator5[0]'
<7>[    0.101084] reg-fixed-voltage regulator5: using lookup tables for GPIO lookup
<7>[    0.101087] reg-fixed-voltage regulator5: No GPIO consumer (null) found
<7>[    0.101178] reg-fixed-voltage regulator6: GPIO lookup for consumer (null)
<7>[    0.101181] reg-fixed-voltage regulator6: using device tree for GPIO lookup
<7>[    0.101187] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator6[0]'
<7>[    0.101194] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator6[0]'
<7>[    0.101198] reg-fixed-voltage regulator6: using lookup tables for GPIO lookup
<7>[    0.101201] reg-fixed-voltage regulator6: No GPIO consumer (null) found
<7>[    0.101357] reg-fixed-voltage pp1200-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.101360] reg-fixed-voltage pp1200-mipibrdg: using device tree for GPIO lookup
<7>[    0.101368] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp1200-mipibrdg[0]'
<7>[    0.101378] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp1200-mipibrdg[0]' - status (0)
<7>[    0.101387] gpio gpiochip0: Persistence not supported for GPIO 54
<6>[    0.101408] pp1200_mipibrdg: supplied by pp1800_alw
<7>[    0.101685] reg-fixed-voltage pp1800-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.101688] reg-fixed-voltage pp1800-mipibrdg: using device tree for GPIO lookup
<7>[    0.101696] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp1800-mipibrdg[0]'
<7>[    0.101707] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp1800-mipibrdg[0]' - status (0)
<7>[    0.101715] gpio gpiochip0: Persistence not supported for GPIO 36
<6>[    0.101728] pp1800_mipibrdg: supplied by pp1800_alw
<7>[    0.101924] reg-fixed-voltage pp3300-panel: GPIO lookup for consumer (null)
<7>[    0.101927] reg-fixed-voltage pp3300-panel: using device tree for GPIO lookup
<7>[    0.101935] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp3300-panel[0]'
<7>[    0.101946] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp3300-panel[0]' - status (0)
<7>[    0.101954] gpio gpiochip0: Persistence not supported for GPIO 35
<6>[    0.101969] pp3300_panel: supplied by pp3300_alw
<7>[    0.102164] reg-fixed-voltage vddio-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.102168] reg-fixed-voltage vddio-mipibrdg: using device tree for GPIO lookup
<7>[    0.102175] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/vddio-mipibrdg[0]'
<7>[    0.102185] of_get_named_gpiod_flags: parsed 'gpio' property of node '/vddio-mipibrdg[0]' - status (0)
<7>[    0.102193] gpio gpiochip0: Persistence not supported for GPIO 37
<6>[    0.102206] vddio_mipibrdg: supplied by pp3300_alw
<6>[    0.102606] iommu: Default domain type: Translated 
<6>[    0.102717] vgaarb: loaded
<5>[    0.102979] SCSI subsystem initialized
<6>[    0.103063] usbcore: registered new interface driver usbfs
<6>[    0.103083] usbcore: registered new interface driver hub
<6>[    0.103105] usbcore: registered new device driver usb
<6>[    0.103133] mc: Linux media interface: v0.10
<6>[    0.103148] videodev: Linux video capture interface: v2.00
<7>[    0.104172] mediatek,efuse 8000000.soc_data: GPIO lookup for consumer wp
<7>[    0.104177] mediatek,efuse 8000000.soc_data: using device tree for GPIO lookup
<7>[    0.104188] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/soc_data@8000000[0]'
<7>[    0.104196] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/soc_data@8000000[0]'
<7>[    0.104203] mediatek,efuse 8000000.soc_data: using lookup tables for GPIO lookup
<7>[    0.104207] mediatek,efuse 8000000.soc_data: No GPIO consumer wp found
<7>[    0.104394] mediatek,efuse 11f10000.efuse: GPIO lookup for consumer wp
<7>[    0.104398] mediatek,efuse 11f10000.efuse: using device tree for GPIO lookup
<7>[    0.104410] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/efuse@11f10000[0]'
<7>[    0.104417] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/efuse@11f10000[0]'
<7>[    0.104423] mediatek,efuse 11f10000.efuse: using lookup tables for GPIO lookup
<7>[    0.104427] mediatek,efuse 11f10000.efuse: No GPIO consumer wp found
<6>[    0.104615] Advanced Linux Sound Architecture Driver Initialized.
<6>[    0.105238] clocksource: Switched to clocksource arch_sys_counter
<5>[    0.124459] VFS: Disk quotas dquot_6.6.0
<6>[    0.124507] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
<6>[    0.125180] NET: Registered protocol family 2
<6>[    0.125317] IP idents hash table entries: 65536 (order: 7, 524288 bytes, linear)
<6>[    0.127128] tcp_listen_portaddr_hash hash table entries: 2048 (order: 3, 32768 bytes, linear)
<6>[    0.127240] TCP established hash table entries: 32768 (order: 6, 262144 bytes, linear)
<6>[    0.127424] TCP bind hash table entries: 32768 (order: 7, 524288 bytes, linear)
<6>[    0.127676] TCP: Hash tables configured (established 32768 bind 32768)
<6>[    0.127767] UDP hash table entries: 2048 (order: 4, 65536 bytes, linear)
<6>[    0.127838] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes, linear)
<6>[    0.128009] NET: Registered protocol family 1
<6>[    0.128036] PCI: CLS 0 bytes, default 64
<6>[    0.128865] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
<6>[    0.129063] hw perfevents: enabled with armv8_cortex_a73 PMU driver, 7 counters available
<6>[    0.129492] kvm [1]: IPA Size Limit: 40 bits
<6>[    0.130181] kvm [1]: vgic-v2@c420000
<6>[    0.130198] kvm [1]: GIC system register CPU interface enabled
<6>[    0.130322] kvm [1]: vgic interrupt IRQ18
<6>[    0.130449] kvm [1]: Hyp mode initialized successfully
<5>[    0.134165] Initialise system trusted keyrings
<6>[    0.134261] workingset: timestamp_bits=62 max_order=20 bucket_order=0
<6>[    0.137208] squashfs: version 4.0 (2009/01/31) Phillip Lougher
<6>[    0.137432] Registering esdfs 0.2
<6>[    0.137571] alt_syscall: table 'read_write_test' available.
<6>[    0.137593] alt_syscall: table 'android' available.
<6>[    0.137615] alt_syscall: table 'android_permissive' available.
<6>[    0.137638] alt_syscall: table 'third_party' available.
<6>[    0.137657] alt_syscall: table 'third_party_permissive' available.
<6>[    0.137674] alt_syscall: table 'complete' available.
<6>[    0.137690] alt_syscall: table 'complete_permissive' available.
<5>[    0.163949] Key type asymmetric registered
<5>[    0.163957] Asymmetric key parser 'x509' registered
<6>[    0.163989] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 246)
<6>[    0.164062] io scheduler mq-deadline registered
<6>[    0.164069] io scheduler kyber registered
<6>[    0.164127] io scheduler bfq registered
<7>[    0.166297] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.166302] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.166320] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.166334] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.166337] gpio-496 (enable): no flags found for enable
<4>[    0.166590] of_fixed_factor_clk: probe of fixed-factor-clock-13m failed with error -17
<3>[    0.177313] mtk-socinfo mtk-socinfo.0.auto: error -ENOENT: Failed to get socinfo data
<4>[    0.177328] mtk-socinfo: probe of mtk-socinfo.0.auto failed with error -2
<6>[    0.177406] mtk-socinfo mtk-socinfo.1.auto: SoC detected, family: MediaTek, soc_id: MT8183, machine: Kompanio 500
<6>[    0.178047] Serial: 8250/16550 driver, 4 ports, IRQ sharing disabled
<7>[    0.179052] mt6577-uart 11002000.serial: GPIO lookup for consumer rs485-term
<7>[    0.179056] mt6577-uart 11002000.serial: using device tree for GPIO lookup
<7>[    0.179069] of_get_named_gpiod_flags: can't parse 'rs485-term-gpios' property of node '/soc/serial@11002000[0]'
<7>[    0.179078] of_get_named_gpiod_flags: can't parse 'rs485-term-gpio' property of node '/soc/serial@11002000[0]'
<7>[    0.179085] mt6577-uart 11002000.serial: using lookup tables for GPIO lookup
<7>[    0.179090] mt6577-uart 11002000.serial: No GPIO consumer rs485-term found
<6>[    0.199214] 11002000.serial: ttyS0 at MMIO 0x11002000 (irq = 33, base_baud = 1625000) is a ST16650V2
<7>[    0.199789] mt6577-uart 11003000.serial: GPIO lookup for consumer rs485-term
<7>[    0.199793] mt6577-uart 11003000.serial: using device tree for GPIO lookup
<7>[    0.199802] of_get_named_gpiod_flags: can't parse 'rs485-term-gpios' property of node '/soc/serial@11003000[0]'
<7>[    0.199810] of_get_named_gpiod_flags: can't parse 'rs485-term-gpio' property of node '/soc/serial@11003000[0]'
<7>[    0.199815] mt6577-uart 11003000.serial: using lookup tables for GPIO lookup
<7>[    0.199818] mt6577-uart 11003000.serial: No GPIO consumer rs485-term found
<6>[    0.219930] 11003000.serial: ttyS1 at MMIO 0x11003000 (irq = 34, base_baud = 1625000) is a ST16650V2
<6>[    0.220032] serial serial0: tty port ttyS1 registered
<6>[    0.224520] usbcore: registered new interface driver udl
<6>[    0.227171] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14008000
<6>[    0.227205] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14009000
<6>[    0.227238] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@1400a000
<6>[    0.227267] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400b000
<6>[    0.227293] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400c000
<6>[    0.227328] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/color@1400e000
<6>[    0.227355] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ccorr@1400f000
<6>[    0.227381] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/aal@14010000
<6>[    0.227408] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/gamma@14011000
<6>[    0.227486] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dsi@14014000
<6>[    0.227515] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dpi@14015000
<7>[    0.230643] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.230647] panel-edp panel: using device tree for GPIO lookup
<7>[    0.230658] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.230666] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.230672] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.230676] panel-edp panel: No GPIO consumer hpd found
<7>[    0.230763] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.230766] panel-edp panel: using device tree for GPIO lookup
<7>[    0.230775] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.230782] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.230786] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.230790] panel-edp panel: No GPIO consumer enable found
<6>[    0.231300] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.231315] mali 13040000.mali: IRQ JOB not found
<3>[    0.231366] mali 13040000.mali: IRQ MMU not found
<3>[    0.231379] mali 13040000.mali: IRQ GPU not found
<6>[    0.231404] mali 13040000.mali: GPU metrics tracepoint support enabled
<4>[    0.231527] cacheinfo: Unable to detect cache hierarchy for CPU 0
<6>[    0.233774] loop: module loaded
<6>[    0.233936] lkdtm: No crash points registered, enable through debugfs
<6>[    0.242646] vsim1: Bringing 1800000uV into 2700000-2700000uV
<7>[    0.252986] of_get_named_gpiod_flags: parsed 'cs-gpios' property of node '/soc/spi@1100a000[0]' - status (0)
<4>[    0.254358] spi-nor spi1.0: found w25q64jwm, expected w25q64dw
<6>[    0.254852] spi-nor spi1.0: w25q64jwm (8192 Kbytes)
<7>[    0.254981] mtd mtd0: GPIO lookup for consumer wp
<7>[    0.254985] mtd mtd0: using device tree for GPIO lookup
<7>[    0.254998] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/spi@11010000/spi-flash@0[0]'
<7>[    0.255007] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/spi@11010000/spi-flash@0[0]'
<7>[    0.255014] mtd mtd0: using lookup tables for GPIO lookup
<7>[    0.255018] mtd mtd0: No GPIO consumer wp found
<7>[    0.256816] mdio_bus fixed-0: GPIO lookup for consumer reset
<7>[    0.256821] mdio_bus fixed-0: using lookup tables for GPIO lookup
<7>[    0.256825] mdio_bus fixed-0: No GPIO consumer reset found
<6>[    0.256839] PPP generic driver version 2.4.2
<6>[    0.256927] PPP MPPE Compression module registered
<6>[    0.257645] mtu3 11201000.usb: uwk - reg:0x420, version:101
<4>[    0.257692] mtu3 11201000.usb: supply vbus not found, using dummy regulator
<6>[    0.257760] mtu3 11201000.usb: dr_mode: 1, is_u3_dr: 0, u3p_dis_msk: 0, drd: auto
<6>[    0.258451] mtu3 11201000.usb: xHCI platform device register success...
<6>[    0.258651] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
<6>[    0.258658] ehci-pci: EHCI PCI platform driver
<6>[    0.258693] ehci-platform: EHCI generic platform driver
<6>[    0.258840] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
<6>[    0.258853] ohci-pci: OHCI PCI platform driver
<6>[    0.258873] ohci-platform: OHCI generic platform driver
<4>[    0.259472] xhci-mtk 11200000.xhci: supply vbus not found, using dummy regulator
<6>[    0.259611] tpm_tis_spi spi0.0: TPM ready IRQ confirmed on attempt 2
<6>[    0.259753] xhci-mtk 11200000.xhci: xHCI Host Controller
<6>[    0.259909] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 1
<6>[    0.259988] xhci-mtk 11200000.xhci: hcc params 0x01400f99 hci version 0x110 quirks 0x0000000000210010
<6>[    0.260022] xhci-mtk 11200000.xhci: irq 290, io mem 0x11200000
<6>[    0.260107] xhci-mtk 11200000.xhci: xHCI Host Controller
<6>[    0.260186] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 2
<6>[    0.260196] xhci-mtk 11200000.xhci: Host supports USB 3.0 SuperSpeed
<6>[    0.260286] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.10
<6>[    0.260293] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    0.260299] usb usb1: Product: xHCI Host Controller
<6>[    0.260305] usb usb1: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
<6>[    0.260311] usb usb1: SerialNumber: 11200000.xhci
<6>[    0.260569] hub 1-0:1.0: USB hub found
<6>[    0.260591] hub 1-0:1.0: 1 port detected
<6>[    0.260770] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
<6>[    0.260816] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.10
<6>[    0.260823] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    0.260829] usb usb2: Product: xHCI Host Controller
<6>[    0.260834] usb usb2: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
<6>[    0.260839] usb usb2: SerialNumber: 11200000.xhci
<6>[    0.261041] hub 2-0:1.0: USB hub found
<3>[    0.261058] hub 2-0:1.0: config failed, hub doesn't have any ports! (err -19)
<6>[    0.261298] usbcore: registered new interface driver cdc_acm
<6>[    0.261304] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
<6>[    0.261337] usbcore: registered new interface driver usb-storage
<6>[    0.262488] mt6397-rtc mt6358-rtc: registered as rtc0
<6>[    0.262662] mt6397-rtc mt6358-rtc: setting system clock to 2025-02-28T19:10:35 UTC (1740769835)
<6>[    0.262695] i2c /dev entries driver
<4>[    0.266043] elan_i2c 2-0015: supply vcc not found, using dummy regulator
<6>[    0.268816] tpm_tis_spi spi0.0: 2.0 TPM (device-id 0x28, rev-id 0)
<6>[    0.269744] mtk-wdt 10007000.watchdog: Watchdog enabled (timeout=31 sec, nowayout=0)
<6>[    0.270086] device-mapper: ioctl: 4.43.0-ioctl (2020-10-01) initialised: dm-devel@redhat.com
<6>[    0.270226] device-mapper: verity-chromeos: dm-verity-chromeos registered
<4>[    0.270585] cpu cpu0: dummy supplies not allowed for exclusive requests
<4>[    0.271385] cpu cpu4: dummy supplies not allowed for exclusive requests
<6>[    0.272227] cpu cpu0: EM: created perf domain
<6>[    0.272577] cpu cpu4: EM: created perf domain
<6>[    0.273322] cpufreq: cpufreq_online: CPU4: Running at unlisted initial frequency: 1199999 KHz, changing to: 1248000 KHz
<7>[    0.274499] pwrseq_simple wifi-pwrseq: GPIO lookup for consumer reset
<7>[    0.274502] pwrseq_simple wifi-pwrseq: using device tree for GPIO lookup
<7>[    0.274515] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/wifi-pwrseq[0]' - status (0)
<7>[    0.274527] gpio gpiochip0: Persistence not supported for GPIO 119
<6>[    0.274690] sdhci: Secure Digital Host Controller Interface driver
<6>[    0.274694] sdhci: Copyright(c) Pierre Ossman
<6>[    0.274873] sdhci-pltfm: SDHCI platform and OF driver helper
<3>[    0.275666] SMCCC: SOC_ID: ARCH_SOC_ID(0) returned error: ffffffffffffffff
<7>[    0.275678] mtk-msdc 11230000.mmc: GPIO lookup for consumer wp
<7>[    0.275682] mtk-msdc 11230000.mmc: using device tree for GPIO lookup
<7>[    0.275693] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/mmc@11230000[0]'
<6>[    0.275695] hid: raw HID events driver (C) Jiri Kosina
<7>[    0.275701] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/mmc@11230000[0]'
<7>[    0.275708] mtk-msdc 11230000.mmc: using lookup tables for GPIO lookup
<7>[    0.275712] mtk-msdc 11230000.mmc: No GPIO consumer wp found
<7>[    0.275714] mtk-msdc 11240000.mmc: GPIO lookup for consumer wp
<7>[    0.275717] mtk-msdc 11240000.mmc: using device tree for GPIO lookup
<7>[    0.275728] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/mmc@11240000[0]'
<7>[    0.275737] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/mmc@11240000[0]'
<7>[    0.275741] mtk-msdc 11240000.mmc: using lookup tables for GPIO lookup
<7>[    0.275744] mtk-msdc 11240000.mmc: No GPIO consumer wp found
<6>[    0.275857] mtk-msdc 11240000.mmc: allocated mmc-pwrseq
<6>[    0.275998] usbcore: registered new interface driver usbhid
<6>[    0.276003] usbhid: USB HID core driver
<6>[    0.276222] ashmem: initialized
<4>[    0.276238] i2c_hid_of 0-0040: supply vdd not found, using dummy regulator
<4>[    0.276307] i2c_hid_of 0-0040: supply vddl not found, using dummy regulator
<4>[    0.276467] i2c_hid_of 2-002c: supply vdd not found, using dummy regulator
<6>[    0.276487] spi_master spi2: will run message pump with realtime priority
<4>[    0.276535] i2c_hid_of 2-002c: supply vddl not found, using dummy regulator
<6>[    0.280479] GACT probability NOT on
<6>[    0.280618] xt_time: kernel timezone is -0000
<6>[    0.280808] Initializing XFRM netlink socket
<6>[    0.280984] NET: Registered protocol family 10
<6>[    0.281351] Segment Routing with IPv6
<6>[    0.281467] NET: Registered protocol family 17
<6>[    0.281476] NET: Registered protocol family 15
<6>[    0.281554] NET: Registered protocol family 40
<6>[    0.281782] registered taskstats version 1
<5>[    0.281789] Loading compiled-in X.509 certificates
<5>[    0.281881] Key type .fscrypt registered
<5>[    0.281885] Key type fscrypt-provisioning registered
<6>[    0.282081] pstore: Using crash dump compression: deflate
<5>[    0.282707] Key type encrypted registered
<7>[    0.292055] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.292062] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.292078] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.292090] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.292092] gpio-496 (enable): no flags found for enable
<7>[    0.295486] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.295492] panel-edp panel: using device tree for GPIO lookup
<7>[    0.295501] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.295506] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.295510] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.295513] panel-edp panel: No GPIO consumer hpd found
<7>[    0.295619] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.295621] panel-edp panel: using device tree for GPIO lookup
<7>[    0.295626] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.295631] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.295634] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.295636] panel-edp panel: No GPIO consumer enable found
<6>[    0.295942] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.295953] mali 13040000.mali: IRQ JOB not found
<3>[    0.295967] mali 13040000.mali: IRQ MMU not found
<3>[    0.295977] mali 13040000.mali: IRQ GPU not found
<6>[    0.295998] mali 13040000.mali: GPU metrics tracepoint support enabled
<7>[    0.298637] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.298643] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.298656] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.298668] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.298670] gpio-496 (enable): no flags found for enable
<6>[    0.299855] mtk-iommu 10205000.iommu: bound 14017000.larb (ops 0xffffffe4970c6448)
<6>[    0.299868] mtk-iommu 10205000.iommu: bound 16010000.larb (ops 0xffffffe4970c6448)
<6>[    0.299874] mtk-iommu 10205000.iommu: bound 1502f000.larb (ops 0xffffffe4970c6448)
<6>[    0.299879] mtk-iommu 10205000.iommu: bound 1a002000.larb (ops 0xffffffe4970c6448)
<6>[    0.299884] mtk-iommu 10205000.iommu: bound 17010000.larb (ops 0xffffffe4970c6448)
<6>[    0.299889] mtk-iommu 10205000.iommu: bound 15021000.larb (ops 0xffffffe4970c6448)
<6>[    0.299894] mtk-iommu 10205000.iommu: bound 1a001000.larb (ops 0xffffffe4970c6448)
<6>[    0.300003] mediatek-disp-ovl 14008000.ovl: Adding to iommu group 0
<6>[    0.300502] mediatek-disp-ovl 14009000.ovl: Adding to iommu group 0
<6>[    0.300688] mediatek-disp-ovl 1400a000.ovl: Adding to iommu group 0
<6>[    0.300871] mediatek-disp-rdma 1400b000.rdma: Adding to iommu group 0
<6>[    0.301045] mediatek-disp-rdma 1400c000.rdma: Adding to iommu group 0
<7>[    0.301814] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.301817] panel-edp panel: using device tree for GPIO lookup
<7>[    0.301826] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.301831] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.301835] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.301838] panel-edp panel: No GPIO consumer hpd found
<7>[    0.301894] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.301896] panel-edp panel: using device tree for GPIO lookup
<7>[    0.301901] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.301906] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.301908] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.301910] panel-edp panel: No GPIO consumer enable found
<7>[    0.302178] anx7625 4-0058: GPIO lookup for consumer enable
<7>[    0.302180] anx7625 4-0058: using device tree for GPIO lookup
<7>[    0.302192] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/soc/i2c@11008000/anx7625@58[0]' - status (0)
<7>[    0.302203] gpio gpiochip0: Persistence not supported for GPIO 45
<7>[    0.302210] anx7625 4-0058: GPIO lookup for consumer reset
<7>[    0.302212] anx7625 4-0058: using device tree for GPIO lookup
<7>[    0.302218] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@11008000/anx7625@58[0]' - status (0)
<7>[    0.302224] gpio gpiochip0: Persistence not supported for GPIO 73
<6>[    0.303052] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.303108] mali 13040000.mali: IRQ JOB not found
<3>[    0.303127] mali 13040000.mali: IRQ MMU not found
<3>[    0.303135] mali 13040000.mali: IRQ GPU not found
<6>[    0.303161] mali 13040000.mali: GPU metrics tracepoint support enabled
<6>[    0.305137] mali 13040000.mali: GPU identified as 0x1 arch 6.2.2 r0p3 status 0
<6>[    0.305609] mali 13040000.mali: No priority control manager is configured
<6>[    0.305762] mali 13040000.mali: No memory group manager is configured
<6>[    0.307115] mali 13040000.mali: Using configured power model mali-g72-power-model, and fallback mali-simple-power-model
<6>[    0.307137] mali 13040000.mali: No volt-bin detected, using default OPP table
<6>[    0.307165] mali 13040000.mali: OPP 0 : opp_freq=300000000 core_mask=f
<6>[    0.307172] mali 13040000.mali: OPP 1 : opp_freq=320000000 core_mask=f
<6>[    0.307181] mali 13040000.mali: OPP 2 : opp_freq=340000000 core_mask=f
<7>[    0.307193] of_get_named_gpiod_flags: parsed 'gpios' property of node '/wifi-wakeup/wowlan[0]' - status (0)
<6>[    0.307196] mali 13040000.mali: OPP 3 : opp_freq=360000000 core_mask=f
<6>[    0.307201] mali 13040000.mali: OPP 4 : opp_freq=380000000 core_mask=f
<6>[    0.307206] mali 13040000.mali: OPP 5 : opp_freq=400000000 core_mask=f
<6>[    0.307214] mali 13040000.mali: OPP 6 : opp_freq=420000000 core_mask=f
<7>[    0.307219] gpio gpiochip0: Persistence not supported for GPIO 113
<6>[    0.307224] mali 13040000.mali: OPP 7 : opp_freq=460000000 core_mask=f
<6>[    0.307238] mali 13040000.mali: OPP 8 : opp_freq=500000000 core_mask=f
<6>[    0.307246] mali 13040000.mali: OPP 9 : opp_freq=540000000 core_mask=f
<6>[    0.307253] mali 13040000.mali: OPP 10 : opp_freq=580000000 core_mask=f
<6>[    0.307261] mali 13040000.mali: OPP 11 : opp_freq=620000000 core_mask=f
<6>[    0.307268] mali 13040000.mali: OPP 12 : opp_freq=653000000 core_mask=f
<6>[    0.307275] mali 13040000.mali: OPP 13 : opp_freq=698000000 core_mask=f
<6>[    0.307282] mali 13040000.mali: OPP 14 : opp_freq=743000000 core_mask=f
<6>[    0.307289] mali 13040000.mali: OPP 15 : opp_freq=800000000 core_mask=f
<6>[    0.307324] input: wifi-wakeup as /devices/platform/wifi-wakeup/input/input0
<7>[    0.307670] of_get_named_gpiod_flags: parsed 'gpios' property of node '/volume-buttons/volume_down[0]' - status (0)
<7>[    0.307678] gpio gpiochip0: Persistence not supported for GPIO 6
<7>[    0.307708] of_get_named_gpiod_flags: parsed 'gpios' property of node '/volume-buttons/volume_up[0]' - status (0)
<7>[    0.307714] gpio gpiochip0: Persistence not supported for GPIO 5
<6>[    0.307770] input: volume-buttons as /devices/platform/volume-buttons/input/input1
<6>[    0.307892] mali 13040000.mali: Probed as mali0
<6>[    0.307964] device-mapper: init: waiting for all devices to be available before creating mapped devices
<4>[    0.310421] cros-ec-pchg cros-ec-pchg.15.auto: Unable to get number or ports (err:-95)
<6>[    0.310427] cros-ec-pchg cros-ec-pchg.15.auto: No peripheral charge ports (err:-95)
<7>[    0.311100] sbs-battery 12-000b: GPIO lookup for consumer sbs,battery-detect
<7>[    0.311104] sbs-battery 12-000b: using device tree for GPIO lookup
<7>[    0.311117] of_get_named_gpiod_flags: can't parse 'sbs,battery-detect-gpios' property of node '/soc/spi@11012000/cros-ec@0/i2c-tunnel/sbs-battery@b[0]'
<7>[    0.311125] of_get_named_gpiod_flags: can't parse 'sbs,battery-detect-gpio' property of node '/soc/spi@11012000/cros-ec@0/i2c-tunnel/sbs-battery@b[0]'
<7>[    0.311130] sbs-battery 12-000b: using lookup tables for GPIO lookup
<7>[    0.311133] sbs-battery 12-000b: No GPIO consumer sbs,battery-detect found
<6>[    0.311487] mtk-svs 1100b000.svs: M_HW_RES0: 0x00120090
<6>[    0.311493] mtk-svs 1100b000.svs: M_HW_RES1: 0xe7fcbb1b
<6>[    0.311497] mtk-svs 1100b000.svs: M_HW_RES2: 0x478b47c7
<6>[    0.311501] mtk-svs 1100b000.svs: M_HW_RES3: 0xabfbf757
<6>[    0.311505] mtk-svs 1100b000.svs: M_HW_RES4: 0xe6fca5ed
<6>[    0.311508] mtk-svs 1100b000.svs: M_HW_RES5: 0x47bb4bc0
<6>[    0.311512] mtk-svs 1100b000.svs: M_HW_RES6: 0xe6fcc7e6
<6>[    0.311515] mtk-svs 1100b000.svs: M_HW_RES7: 0xe7fc980f
<6>[    0.311519] mtk-svs 1100b000.svs: M_HW_RES8: 0x4bbb4bef
<6>[    0.311522] mtk-svs 1100b000.svs: M_HW_RES9: 0xabfb366c
<6>[    0.311525] mtk-svs 1100b000.svs: M_HW_RES14: 0x9e862dbb
<6>[    0.311529] mtk-svs 1100b000.svs: M_HW_RES15: 0x015a0010
<6>[    0.311532] mtk-svs 1100b000.svs: M_HW_RES16: 0xe7fc8e1c
<6>[    0.311536] mtk-svs 1100b000.svs: M_HW_RES17: 0x47bb47ef
<6>[    0.311539] mtk-svs 1100b000.svs: M_HW_RES18: 0xabfbc84d
<4>[    0.314044] devfreq 13040000.mali: Couldn't update frequency transition information.
<6>[    0.314720]  SVSB_CPU_LITTLE: svs_init01_isr_handler: VDN74~30:0x141c242b~0x2f33373d, DC:0x031701cf
<6>[    0.315000]  SVSB_CPU_BIG: svs_init01_isr_handler: VDN74~30:0x151e262d~0x32373c41, DC:0x031a016a
<6>[    0.315268]  SVSB_CCI: svs_init01_isr_handler: VDN74~30:0x13192229~0x2d32383d, DC:0x031afed0
<6>[    0.315530]  SVSB_GPU: svs_init01_isr_handler: VDN74~30:0x1416181a~0x1d202428, DC:0x031ffef8
<4>[    0.316867] thermal thermal_zone9: power_allocator: sustainable_power will be estimated
<6>[    0.316993] sbs-battery 12-000b: sbs-battery: battery gas gauge device registered
<6>[    0.317996]  SVSB_CPU_LITTLE: svs_init02_isr_handler: VOP74~30:0x1b232b32~0x363a3e44, DC:0x03170000
<6>[    0.318197]  SVSB_CPU_BIG: svs_init02_isr_handler: VOP74~30:0x1c252d34~0x393e4348, DC:0x031a0000
<6>[    0.318286]  SVSB_CCI: svs_init02_isr_handler: VOP74~30:0x1d232b32~0x373b4246, DC:0x031a0130
<6>[    0.318415]  SVSB_GPU: svs_init02_isr_handler: VOP74~30:0x181a1c1e~0x2125282c, DC:0x031f0108
<6>[    0.324730] tpm_tis_spi spi0.0: Cr50 firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d
<7>[    0.326719] it6505 3-005c: GPIO lookup for consumer reset
<7>[    0.326725] it6505 3-005c: using device tree for GPIO lookup
<7>[    0.326755] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@1100f000/it6505dptx@5c[0]' - status (0)
<7>[    0.326776] gpio gpiochip0: Persistence not supported for GPIO 179
<6>[    0.327640] input: cros_ec as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input2
<6>[    0.328281] mediatek-dpi 14015000.dpi: Found bridge node: /soc/i2c@1100f000/it6505dptx@5c
<6>[    0.329020] mediatek-drm mediatek-drm.3.auto: bound 14008000.ovl (ops 0xffffffe497058738)
<6>[    0.329033] mediatek-drm mediatek-drm.3.auto: bound 14009000.ovl (ops 0xffffffe497058738)
<6>[    0.329045] mediatek-drm mediatek-drm.3.auto: bound 1400a000.ovl (ops 0xffffffe497058738)
<6>[    0.329056] mediatek-drm mediatek-drm.3.auto: bound 1400b000.rdma (ops 0xffffffe4970590f8)
<6>[    0.329067] mediatek-drm mediatek-drm.3.auto: bound 1400c000.rdma (ops 0xffffffe4970590f8)
<6>[    0.329078] mediatek-drm mediatek-drm.3.auto: bound 1400e000.color (ops 0xffffffe497057bf0)
<6>[    0.329089] mediatek-drm mediatek-drm.3.auto: bound 1400f000.ccorr (ops 0xffffffe4970578b8)
<6>[    0.329100] mediatek-drm mediatek-drm.3.auto: bound 14010000.aal (ops 0xffffffe497057648)
<6>[    0.329111] mediatek-drm mediatek-drm.3.auto: bound 14011000.gamma (ops 0xffffffe497057f30)
<6>[    0.330413] mediatek-drm mediatek-drm.3.auto: bound 14014000.dsi (ops 0xffffffe49705e8c0)
<6>[    0.330825] mediatek-drm mediatek-drm.3.auto: bound 14015000.dpi (ops 0xffffffe49705e2f0)
<6>[    0.331871] [drm] Initialized mediatek 1.0.0 20150513 for mediatek-drm.3.auto on minor 0
<6>[    0.332083] input: cros_ec_buttons as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input3
<4>[    0.338572] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
<6>[    0.344014] cros-ec-spi spi2.0: Chrome EC device registered
<4>[    0.345882] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
<4>[    0.349059] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
<4>[    0.349712] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
<6>[    0.352448] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
<4>[    0.352495] sbs-battery 12-000b: I2C adapter does not support I2C_FUNC_SMBUS_READ_BLOCK_DATA.
                  Fallback method does not support PEC.
<6>[    0.353624] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
<4>[    0.354569] mmc1: queuing unknown CIS tuple 0x80 (1 bytes)
<4>[    0.354630] mmc1: queuing unknown CIS tuple 0x81 (1 bytes)
<4>[    0.354682] mmc1: queuing unknown CIS tuple 0x82 (1 bytes)
<6>[    0.354720] mmc1: new ultra high speed SDR104 SDIO card at address 0001
<6>[    0.370508] mtk-msdc 11230000.mmc: phase: [map:ffffff3f] [maxlen:24] [final:20]
<6>[    0.372855] mmc0: new HS400 MMC card at address 0001
<6>[    0.374118] mmcblk0: mmc0:0001 DA4032 29.1 GiB 
<6>[    0.375158] mmcblk0boot0: mmc0:0001 DA4032 partition 1 4.00 MiB
<6>[    0.376197] mmcblk0boot1: mmc0:0001 DA4032 partition 2 4.00 MiB
<6>[    0.376377] mmcblk0rpmb: mmc0:0001 DA4032 partition 3 16.0 MiB, chardev (241:0)
<6>[    0.381187]  mmcblk0: p1 p2 p3 p4 p5 p6 p7 p8 p9 p10 p11 p12
<6>[    0.407000] input: hid-over-i2c 06CB:CDB5 Mouse as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input4
<6>[    0.407689] hid-generic 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
<6>[    0.408838] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    0.409505] device-mapper: ioctl: dm-0 (vroot) is ready
<6>[    0.409798] clk: Disabling unused clocks
<6>[    0.410436] ALSA device list:
<6>[    0.410446]   No soundcards found.
<3>[    0.410517] Warning: unable to open an initial console. Fallback to ttynull.
<6>[    0.410534] printk: console [ttynull0] enabled
<6>[    0.422476] EXT4-fs (dm-0): mounting ext2 file system using the ext4 subsystem
<6>[    0.424604] EXT4-fs (dm-0): mounted filesystem without journal. Opts: (null)
<6>[    0.424647] VFS: Mounted root (ext2 filesystem) readonly on device 254:0.
<6>[    0.430386] devtmpfs: mounted
<6>[    0.432251] Freeing unused kernel memory: 1408K
<6>[    0.432321] Run /sbin/init as init process
<7>[    0.432326]   with arguments:
<7>[    0.432328]     /sbin/init
<7>[    0.432331]     cros_secure
<7>[    0.432333]   with environment:
<7>[    0.432335]     HOME=/
<7>[    0.432337]     TERM=linux
<7>[    0.432341]     dm=1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583
<7>[    0.432344]     cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4=
<5>[    0.528179] audit: type=1404 audit(1740769835.764:2): enforcing=1 old_enforcing=0 auid=4294967295 ses=4294967295 enabled=1 old-enabled=1 lsm=selinux res=1
<6>[    0.593758] SELinux:  Permission bpf in class capability2 not defined in policy.
<6>[    0.593785] SELinux:  Permission checkpoint_restore in class capability2 not defined in policy.
<6>[    0.593814] SELinux:  Permission bpf in class cap2_userns not defined in policy.
<6>[    0.593821] SELinux:  Permission checkpoint_restore in class cap2_userns not defined in policy.
<6>[    0.593984] SELinux: the above unknown classes and permissions will be denied
<6>[    0.602737] SELinux:  policy capability network_peer_controls=1
<6>[    0.602760] SELinux:  policy capability open_perms=1
<6>[    0.602767] SELinux:  policy capability extended_socket_class=1
<6>[    0.602773] SELinux:  policy capability always_check_network=0
<6>[    0.602779] SELinux:  policy capability cgroup_seclabel=0
<6>[    0.602785] SELinux:  policy capability nnp_nosuid_transition=1
<6>[    0.602791] SELinux:  policy capability genfs_seclabel_symlinks=0
<6>[    0.602797] SELinux:  policy capability ioctl_skip_cloexec=0
<5>[    0.657557] audit: type=1403 audit(1740769835.894:3): auid=4294967295 ses=4294967295 lsm=selinux res=1
<6>[    0.658287] usb 1-1: new high-speed USB device number 2 using xhci-mtk
<6>[    0.785796] usb 1-1: New USB device found, idVendor=05e3, idProduct=0608, bcdDevice=60.90
<6>[    0.785814] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
<6>[    0.785821] usb 1-1: Product: USB2.0 Hub
<6>[    0.786830] hub 1-1:1.0: USB hub found
<6>[    0.787131] hub 1-1:1.0: 3 ports detected
<5>[    0.965546] audit: type=1400 audit(1740769836.202:4): avc:  granted  { execute } for  pid=346 comm="sh" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:cros_init_scripts:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
<6>[    1.066459] usb 1-1.3: new high-speed USB device number 3 using xhci-mtk
<6>[    1.154664] usb 1-1.3: New USB device found, idVendor=0408, idProduct=a064, bcdDevice= 0.04
<6>[    1.154683] usb 1-1.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
<6>[    1.154691] usb 1-1.3: Product: HD User Facing
<6>[    1.154696] usb 1-1.3: Manufacturer: Quanta
<7>[    1.181209] udevd[359]: Starting version 249
<6>[    1.360742] EXT4-fs (mmcblk0p1): mounted filesystem with ordered data mode. Opts: commit=600,discard
<6>[    1.364087] EXT4-fs (mmcblk0p8): mounted filesystem with ordered data mode. Opts: 
<6>[    1.409391] LoadPin: dm-0 (254:0): read-only
<6>[    1.409413] LoadPin: load pinning engaged.
<5>[    1.409460] LoadPin: kernel-module pinned obj="/lib/modules/5.10.230-25844-gdc65f732bf53/kernel/drivers/input/serio/serio.ko.gz" pid=381 cmdline="udevd --daemon"
<6>[    1.476520] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
<5>[    1.496593] INFO chromeos_startup: [tpm.cc(323)] TPM ready
<5>[    1.496770] INFO chromeos_startup: [tpm2.cc(121)] Getting key from TPM2 NVRAM index 8388613
<6>[    1.502819] rmi4_f01 rmi4-00.fn01: found RMI device, manufacturer: Synaptics, product: TM3509-001, fw id: 3010219
<5>[    1.509402] INFO chromeos_startup: [tpm.cc(440)] Found encstateful NVRAM area.
<5>[    1.525597] INFO chromeos_startup: [encryption_key.cc(181)] Using NVRAM as system key; already populated.
<6>[    1.581871] input: Synaptics TM3509-001 as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input6
<6>[    1.582273] hid-rmi 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
<5>[    1.608074] INFO chromeos_startup: [tpm_setup.cc(98)] There is no bio_crypto_init binary, so skip sending TPM seed.
<5>[    1.646706] INFO chromeos_startup: [tpm.cc(421)] Version 2 Lockbox NVRAM area found.
<5>[    1.646755] INFO chromeos_startup: [tpm_setup.cc(245)] Lockbox is valid, exporting.
<5>[    1.649113] INFO chromeos_startup: [dmcrypt_container.cc(112)] Setting up backing device
<5>[    1.756400] INFO chromeos_startup: [dmcrypt_container.cc(177)] Waiting for dm-crypt device to appear
<5>[    1.765635] INFO chromeos_startup: [dmcrypt_container.cc(143)] Removing provisioned dmcrypt key from kernel keyring.
<5>[    1.780525] INFO chromeos_startup: [encrypted_fs.cc(275)] Mounting /dev/mapper/encstateful onto /mnt/stateful_partition/encrypted
<5>[    1.781455] INFO chromeos_startup: [encrypted_fs.cc(89)] Using vm.dirty_expire_centisecs/100 as the commit interval
<6>[    1.787357] EXT4-fs (dm-1): mounted filesystem with ordered data mode. Opts: discard,commit=600
<5>[    1.787530] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/var onto /var
<5>[    1.795121] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/chronos onto /home/chronos
<6>[    1.878971] fscrypt: AES-256-CTS-CBC using implementation "cts-cbc-aes-ce"
<5>[    1.889561] audit: type=1400 audit(1740769837.126:5): avc:  granted  { execute } for  pid=603 comm="chromeos_startu" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:chromeos_startup:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
<5>[    1.896385] WARNING chromeos_startup: [stateful_mount.cc(470)] Failed to read from /mnt/stateful_partition/.update_available: No such file or directory (2)
<6>[    1.896624] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
<7>[    2.078256] frecon[595]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<5>[    2.185814] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/var)
<5>[    2.374723] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/user)
<5>[    2.375765] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/root)
<5>[    2.376794] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/chronos)
<5>[    2.454681] audit: type=1400 audit(1740769837.691:6): avc:  denied  { search } for  pid=635 comm="rsyslogd" name="hosts.d" dev="dm-0" ino=23817 scontext=u:r:cros_rsyslogd:s0 tcontext=u:object_r:cros_run_crosdns:s0 tclass=dir permissive=0
<5>[    2.457848] audit: type=1400 audit(1740769837.694:7): avc:  denied  { create } for  pid=635 comm="rsyslogd" scontext=u:r:cros_rsyslogd:s0 tcontext=u:r:cros_rsyslogd:s0 tclass=udp_socket permissive=0
<7>[    2.694042] frecon[595]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<7>[    2.724420] frecon[595]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<3>[    3.050517] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050547] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050556] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050721] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050732] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050739] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050749] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050757] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050765] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050810] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.050820] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<5>[    3.056319] init: bluetoothd pre-start process (760) terminated with status 1
<7>[    3.082422] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    3.082437] gpio gpiochip0: registered chardev handle for line 150
<7>[    3.082451] gpio gpiochip0: registered chardev handle for 1 lines
<6>[    3.642401] Bluetooth: bt_init() Core ver 2.22
<6>[    3.642603] NET: Registered protocol family 31
<6>[    3.642610] Bluetooth: bt_init() HCI device and connection manager initialized
<6>[    3.642629] Bluetooth: hci_sock_init() HCI socket layer initialized
<6>[    3.642637] Bluetooth: l2cap_init_sockets() L2CAP socket layer initialized
<6>[    3.642667] Bluetooth: sco_init() SCO socket layer initialized
<6>[    3.674046] ath10k_sdio mmc1:0001:1: qca6174 hw3.2 sdio target 0x05030000 chip_id 0x00000000 sub 0000:0000
<6>[    3.674072] ath10k_sdio mmc1:0001:1: kconfig debug 1 debugfs 1 tracing 1 dfs 0 testmode 1
<6>[    3.674353] ath10k_sdio mmc1:0001:1: firmware ver WLAN.RMH.4.4.1-00189 api 6 features wowlan,ignore-otp,mfp crc32 595e0108
<6>[    3.828934] ath10k_sdio mmc1:0001:1: board_file api 2 bmi_id 0:4 crc32 e57aadc7
<6>[    4.157325] ath10k_sdio mmc1:0001:1: htt-ver 3.87 wmi-op 4 htt-op 3 cal otp max-sta 32 raw 0 hwcrypto 1
<4>[    4.225636] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
<4>[    4.233372] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
<4>[    4.236951] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
<6>[    4.240544] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
<6>[    4.241598] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
<7>[    4.241788] ath: EEPROM regdomain: 0x6c
<7>[    4.241792] ath: EEPROM indicates we should expect a direct regpair map
<7>[    4.241803] ath: Country alpha2 being used: 00
<7>[    4.241807] ath: Regpair used: 0x6c
<7>[    4.257341] udevd[485]: Using default interface naming scheme 'v249'.
<7>[    4.576048] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    4.576068] gpio gpiochip0: registered chardev handle for line 150
<7>[    4.576084] gpio gpiochip0: registered chardev handle for 1 lines
<7>[    4.773321] ath: EEPROM regdomain: 0x8348
<7>[    4.773329] ath: EEPROM indicates we should expect a country code
<7>[    4.773333] ath: doing EEPROM country->regdmn map search
<7>[    4.773336] ath: country maps to regdmn code: 0x3a
<7>[    4.773339] ath: Country alpha2 being used: US
<7>[    4.773341] ath: Regpair used: 0x3a
<7>[    4.773350] ath: regdomain 0x8348 dynamically updated by user
<5>[    5.569541] init: failsafe-delay main process (745) killed by TERM signal
<5>[    5.608158] init: secagentd post-start process (1659) terminated with status 2
<7>[    6.070038] max98357a max98357a: GPIO lookup for consumer sdmode
<7>[    6.070049] max98357a max98357a: using device tree for GPIO lookup
<7>[    6.070080] of_get_named_gpiod_flags: parsed 'sdmode-gpios' property of node '/max98357a[0]' - status (0)
<7>[    6.070104] gpio gpiochip0: Persistence not supported for GPIO 175
<6>[    6.091205] fuse: init (API version 7.32)
<6>[    6.120795] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<3>[    6.262001] mtk-scp 10500000.scp: invalid resource
<6>[    6.262079] mtk-scp 10500000.scp: assigned reserved memory node memory@50000000
<4>[    6.270045] elants_i2c 0-0010: supply vcc33 not found, using dummy regulator
<4>[    6.270421] elants_i2c 0-0010: supply vccio not found, using dummy regulator
<7>[    6.270520] elants_i2c 0-0010: GPIO lookup for consumer reset
<7>[    6.270524] elants_i2c 0-0010: using device tree for GPIO lookup
<7>[    6.270560] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@11007000/touchscreen@10[0]' - status (0)
<7>[    6.270583] gpio gpiochip0: Persistence not supported for GPIO 156
<6>[    6.294191] mt6358-sound mt6358-sound: mt6358_platform_driver_probe(), dev name mt6358-sound
<3>[    6.294853] elants_i2c 0-0010: nothing at this address
<6>[    6.296972] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<6>[    6.309673] remoteproc remoteproc0: scp is available
<6>[    6.311488] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<6>[    6.334725] remoteproc remoteproc0: powering up scp
<6>[    6.334755] remoteproc remoteproc0: Booting fw image mediatek/mt8183/scp_legacy.img, size 1032064
<6>[    6.334777] mtk-scp 10500000.scp: IPI buf addr 0x0007bdb0
<6>[    6.343969] Bluetooth: hci_uart_init() HCI UART driver ver 2.3
<6>[    6.343995] Bluetooth: hci_uart_register_proto() HCI UART protocol H4 registered
<6>[    6.344072] Bluetooth: hci_uart_register_proto() HCI UART protocol Three-wire (H5) registered
<6>[    6.344129] Bluetooth: hci_uart_register_proto() HCI UART protocol QCA registered
<7>[    6.344849] hci_uart_qca serial0-0: GPIO lookup for consumer enable
<7>[    6.344858] hci_uart_qca serial0-0: using device tree for GPIO lookup
<7>[    6.344893] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/soc/serial@11003000/bluetooth[0]' - status (0)
<7>[    6.344911] gpio gpiochip0: Persistence not supported for GPIO 120
<6>[    6.346095] Bluetooth: qca_setup() hci0: setting up ROME/QCA6390
<6>[    6.386227] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<6>[    6.537856] mtk-scp 10500000.scp: creating channel cros-ec-rpmsg addr 0xd
<6>[    6.537863] mtk-scp 10500000.scp: SCP is ready. FW version kukui_scp_v2.0.2796-7246101293
<6>[    6.537875] remoteproc remoteproc0: remote processor scp is now up
<3>[    6.559378] Bluetooth: qca_recv() hci0: Frame reassembly failed (-84)
<4>[    6.610320] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: No cache defaults, reading back from HW
<6>[    6.610997] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mtk_afe_combine_sub_dai(), num of dai 20
<6>[    6.619002] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<3>[    6.619883] debugfs: Directory '11220000.audio-controller:mt8183-afe-pcm' with parent 'mt8183_mt6358_ts3a227_max98357' already present!
<4>[    6.630176] hdmi-audio-codec hdmi-audio-codec.17.auto: ASoC: sink widget TX overwritten
<3>[    6.665636] debugfs: File 'Playback' in directory 'dapm' already present!
<3>[    6.665663] debugfs: File 'Capture' in directory 'dapm' already present!
<6>[    6.669141] input: mt8183_mt6358_ts3a227_max98357 Headset Jack as /devices/platform/mt8183-sound/sound/card0/input7
<6>[    6.669688] input: mt8183_mt6358_ts3a227_max98357 HDMI Jack as /devices/platform/mt8183-sound/sound/card0/input8
<6>[    6.778408] mtk-mdp3 14001000.mdp3_rdma0: Adding to iommu group 0
<3>[    6.778772] mtk-mdp3 14001000.mdp3_rdma0: can't get node mediatek,mmsys2
<3>[    6.778786] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mmsys2
<3>[    6.779186] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mm-mutex2
<6>[    6.781135] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:3 alias:0 id:11 base:0x14001000 regs:00000000e3859cdd
<6>[    6.782172] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:23 alias:0 id:9 base:0x14000000 regs:00000000c1216aa1
<6>[    6.786160] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:24 alias:1 id:10 base:0x14000000 regs:00000000ac316e60
<6>[    6.792473] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:7 alias:0 id:18 base:0x14005000 regs:00000000790501ab
<6>[    6.792879] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:8 alias:1 id:19 base:0x14006000 regs:00000000cea9a803
<6>[    6.792923] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:1 alias:0 id:4 base:0x15020000 regs:00000000aa291148
<6>[    6.792957] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:22 alias:1 id:6 base:0x15020000 regs:00000000e154807f
<6>[    6.793010] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:0 id:14 base:0x14003000 regs:00000000019ec311
<6>[    6.793137] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:1 id:15 base:0x14004000 regs:000000006c011526
<6>[    6.793190] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:5 alias:0 id:20 base:0x14005000 regs:00000000f1e7e0ba
<6>[    6.796603] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:6 alias:0 id:21 base:0x14006000 regs:00000000d17655ea
<6>[    6.796742] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:18 alias:0 id:13 base:0x1401c000 regs:00000000c3c27c76
<3>[    6.800131] mdp_debug_init:start
<3>[    6.806136] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-tdshp0
<3>[    6.806157] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-color0
<3>[    6.806164] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-aal0
<3>[    6.806181] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mediatek,larb
<3>[    6.806203] mdp_debug_init:end
<6>[    6.807194] mtk-mdp3 14001000.mdp3_rdma0: Driver registered as /dev/video2
<6>[    6.844245] Bluetooth: qca_read_soc_version() hci0: QCA Product ID   :0x00000008
<6>[    6.844295] Bluetooth: qca_read_soc_version() hci0: QCA SOC Version  :0x00000044
<6>[    6.844302] Bluetooth: qca_read_soc_version() hci0: QCA ROM Version  :0x00000302
<6>[    6.844310] Bluetooth: qca_read_soc_version() hci0: QCA Patch Version:0x00000111
<6>[    6.844322] Bluetooth: qca_uart_setup() hci0: QCA controller version 0x00440302
<6>[    6.844333] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/rampatch_00440302.bin
<6>[    6.975170] mtk-fd-4.0 1502b000.fd: Adding to iommu group 0
<6>[    6.976058] mtk-cam-dip 15022000.dip: Adding to iommu group 0
<6>[    6.976751] mtk-fd-4.0 1502b000.fd: scp addr:0x0000000050800000 va:ffffffc018800000
<6>[    6.976796] mtk-fd-4.0 1502b000.fd: scp iova addr:0x00000000fde00000
<6>[    6.987943] mtk-cam-p1 1a000000.camisp: Adding to iommu group 0
<6>[    6.993680] mtk-vcodec-enc 17020000.vcodec: Adding to iommu group 0
<6>[    6.999810] mtk-cam-p1 1a000000.camisp: Registered media2
<6>[    6.999839] mtk-cam-p1 1a000000.camisp: Registered mtk-cam-p1 1a000000.camisp
<6>[    7.020583] mtk-vcodec-dec 16000000.vcodec: Adding to iommu group 0
<6>[    7.022152] mtk-jpeg 17030000.venc_jpg: Adding to iommu group 0
<6>[    7.023477] mtk-jpeg 17030000.venc_jpg: mtk-jpeg-enc device registered as /dev/video34 (81,37)
<7>[    7.048170] udevd[378]: Using default interface naming scheme 'v249'.
<4>[    7.052157] memfd_create() without MFD_EXEC nor MFD_NOEXEC_SEAL, pid=2260 'patchpaneld'
<6>[    7.259464] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/nvm_00440302_i2s.bin
<6>[    7.353158] Bluetooth: qca_uart_setup() hci0: QCA setup on UART is completed
<6>[    7.487395] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[    7.487418] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[    7.487425] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[    7.487431] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<3>[    7.545460] mtk-scp 10500000.scp: No such ipi id = 13
<6>[    7.561099] cros-ec-dev cros-ec-dev.18.auto: CrOS System Control Processor MCU detected
<4>[    7.585839] cros-ec-pchg cros-ec-pchg.25.auto: Unable to get number or ports (err:-95)
<6>[    7.585869] cros-ec-pchg cros-ec-pchg.25.auto: No peripheral charge ports (err:-95)
<6>[    7.586719] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: Chrome EC device registered
<7>[    7.945029] usb 1-1.3: GPIO lookup for consumer privacy
<7>[    7.945044] usb 1-1.3: using lookup tables for GPIO lookup
<7>[    7.945051] usb 1-1.3: No GPIO consumer privacy found
<6>[    7.945059] usb 1-1.3: Found UVC 1.00 device HD User Facing (0408:a064)
<6>[    7.966631] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    7.972814] usbcore: registered new interface driver uvcvideo
<6>[    8.082825] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mt8183_adda_dmic_set(), kcontrol name MTKAIF_DMIC, mtkaif_dmic 1
<6>[    8.093824] IPv6: ADDRCONF(NETDEV_CHANGE): arc_ns0: link becomes ready
<6>[    8.094045] IPv6: ADDRCONF(NETDEV_CHANGE): veth0: link becomes ready
<6>[    8.224755] IPv6: ADDRCONF(NETDEV_CHANGE): veth1: link becomes ready
<7>[    8.406962] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.406979] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.406990] gpio gpiochip0: registered chardev handle for 1 lines
<5>[    8.415924] init: send-boot-elog-metrics main process (3113) terminated with status 1
<6>[    8.476986] wlan0: authenticate with 84:17:ef:e4:dc:b6
<7>[    8.497855] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.497873] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.497887] gpio gpiochip0: registered chardev handle for 1 lines
<6>[    8.535384] wlan0: send auth to 84:17:ef:e4:dc:b6 (try 1/3)
<6>[    8.537018] wlan0: authenticated
<6>[    8.538459] wlan0: associate with 84:17:ef:e4:dc:b6 (try 1/3)
<6>[    8.541624] wlan0: RX AssocResp from 84:17:ef:e4:dc:b6 (capab=0x1511 status=0 aid=7)
<6>[    8.555924] wlan0: associated
<7>[    8.558291] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.558315] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.558334] gpio gpiochip0: registered chardev handle for 1 lines
<7>[    8.570905] wlan0: Limiting TX power to 30 (30 - 0) dBm as advertised by 84:17:ef:e4:dc:b6
<6>[    8.598565] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[    8.601349] wlan0: dropped frame to 84:17:ef:e4:dc:b6 (unauthorized port)
<6>[    8.752896] 8021q: 802.1Q VLAN Support v1.8
<6>[    8.794828] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    8.909815] zram: Added device: zram0
<6>[    9.002803] zram0: detected capacity change from 0 to 8136663040
<6>[    9.035834] Adding 7945956k swap on /dev/zram0.  Priority:-2 extents:1 across:7945956k SS
<6>[    9.181351] async_tx: api initialized (async)
<6>[    9.186300] xor: measuring software checksum speed
<6>[    9.189299]    8regs           :  3348 MB/sec
<6>[    9.191343]    32regs          :  4973 MB/sec
<6>[    9.193731]    arm64_neon      :  4234 MB/sec
<6>[    9.193747] xor: using function: 32regs (4973 MB/sec)
<3>[    9.333559] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.334407] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.335252] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.336107] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.336976] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.337826] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.338672] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.339461] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.340306] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.341140] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.341990] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.342841] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.343692] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.344467] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.345402] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.346258] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.347111] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.347962] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.348812] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.349659] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.350469] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.351311] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.352138] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.352962] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.353807] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.354654] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.355472] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.356309] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.357139] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.357965] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.358789] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.359612] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<6>[    9.413451] zram: setup backing device /dev/mapper/zram-writeback
<3>[   15.010327] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.011227] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.012326] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.013492] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.014570] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.015689] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.016681] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.017512] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.018395] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.019276] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.020147] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.021019] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.021888] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.022758] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.023648] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.024530] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.025413] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.026295] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.027177] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.028060] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.028943] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.029824] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.030704] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.031521] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.032407] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.033290] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.034174] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.035056] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.035938] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.036822] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.037705] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.038522] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<6>[   30.688920] vaux18: disabling
<6>[   30.689094] vio28: disabling
<6>[   46.468235] fscrypt: AES-256-XTS using implementation "xts-aes-ce"
<6>[   58.908940] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   58.908957] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   58.908962] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   58.908966] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.027497] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.027523] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.027528] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.027534] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.076851] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.076869] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.076873] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.076878] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.117932] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.117949] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.117954] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.117959] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   62.433593] PDLOG 2025/02/28 19:10:33.178 P0 Disconnected
<3>[   66.009996] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.011383] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.013360] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.014569] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.015561] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.016567] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.017569] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.018566] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.019868] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.020956] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.021961] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.023018] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.023913] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.024805] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.025759] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.026757] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.027805] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.028758] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.029756] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.030757] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.031757] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.032768] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.033814] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.034755] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.035762] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.036774] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.037767] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.038774] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.039905] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.040756] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.041624] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   66.042605] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<7>[   67.163517] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[   67.163535] gpio gpiochip0: registered chardev handle for line 150
<7>[   67.163549] gpio gpiochip0: registered chardev handle for 1 lines
<7>[   67.379543] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[   67.379565] gpio gpiochip0: registered chardev handle for line 150
<7>[   67.379584] gpio gpiochip0: registered chardev handle for 1 lines
<3>[   72.008979] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.009861] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.010720] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.011578] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.012434] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.013293] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.014151] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.014991] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.015817] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.016643] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.017459] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.018278] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.019097] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.019911] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.020723] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.021438] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.022249] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.023060] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.023871] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.024682] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.025436] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.026247] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.027057] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.027870] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.028682] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.029437] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.030250] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.031088] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.031909] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.032748] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.033582] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   72.034401] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
