/sys/class/power_supply/CROS_USBPD_CHARGER0
  charge_control_limit_max 0
  current_max          1500000
  input_current_limit  -1
  input_voltage_limit  -1
  manufacturer         0
  model_name           ed00
  online               0
  status               Not charging
  type                 USB
  usb_type             Unknown [SDP] DCP CDP C PD PD_DRP BrickID
  voltage_max_design   0
  voltage_now          0
/sys/class/power_supply/sbs-12-000b
  capacity             80
  capacity_error_margin 3
  capacity_level       Normal
  charge_full          3538000
  charge_full_design   4570000
  charge_now           2847000
  constant_charge_current_max 3200000
  constant_charge_voltage_max 8800000
  current_avg          -508000
  current_now          -700000
  cycle_count          18
  energy_full          27690000
  energy_full_design   35770000
  energy_now           22280000
  health               Unknown
  manufacture_day      12
  manufacture_month    4
  manufacture_year     2021
  manufacturer         PANASON
  model_name           AP16L5J
  present              1
  status               Discharging
  technology           Unknown
  temp                 270
  time_to_empty_avg    19440
  time_to_full_avg     3932100
  type                 Battery
  voltage_max_design   7700000
  voltage_min_design   7700000
  voltage_now          7783000
