

coreboot-v1.9308_26_0.0.22-10544-g50eadf7c92 Mon Feb  8 05:04:19 UTC 2021 verstage starting (log level: 8)...
ARM64: Exception handlers installed.
WDT: Last reset was cold boot
SPI0(PAD0) initialized at 992727 Hz
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
Probing TPM: . done!
TPM ready after 0 ms
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
tlcl_send_startup: Startup return code is 0
TPM: setup succeeded
src/security/tpm/tss/tcg-2.0/tss.c:223 index 0x1007 return code 0
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
Phase 1
FMAP: area GBB found @ 3f5000 (12032 bytes)
VB2:vb2_check_recovery() Recovery reason from previous boot: 0x0 / 0x0
Phase 2
Phase 3
FMAP: area GBB found @ 3f5000 (12032 bytes)
read SPI 0x3f5180 0x1000: 1293 us, 3167 KB/s, 25.336 Mbps
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_keyblock() Checking key block signature...
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_fw_preamble() Verifying preamble.
Phase 4
FMAP: area FW_MAIN_B found @ 5a9000 (1367808 bytes)
VB2:vb2api_init_hash() HW crypto for hash_alg 2 not supported, using SW
Saving nvdata
tlcl_extend: response is 0
tlcl_extend: response is 0
tlcl_lock_nv_write: response is 0
Slot B is selected


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 romstage starting (log level: 8)...
ARM64: Exception handlers installed.
[RTC]rtc_enable_dcxo,41: con=0x482, osc32con=0x826f, sec=0x2002
[RTC]rtc_check_state,142: con=482, pwrkey1=a357, pwrkey2=67d2
[RTC]rtc_eosc_cali,157: PMIC_RG_FQMTR_CKSEL=0x4a
[RTC]rtc_get_frequency_meter,134: input=0xf, output=796
[RTC]rtc_osc_init,208: EOSC32 cali val = 0x826f
[RTC]rtc_boot_common,186: irqsta=1, bbpu=0, con=482
[RTC]rtc_bbpu_power_on,373: rtc_write_trigger=1
[RTC]rtc_bbpu_power_on,376: done BBPU=0x9
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_DDR_TRAINING found @ 556000 (8192 bytes)
read_calibration_data_from_flash: ret=0x8f0, length=0x8f0
DRAM-K: Fast Calibration
Calibration params loaded from flash
Run calibration (freq: 1600, first: 1)
Vendor id is 0x6
Run calibration (freq: 2400, first: 0)
Vendor id is 0x6
Run calibration (freq: 3200, first: 0)
Vendor id is 0x6
[MEM] complex R/W mem test pass : 0
[MEM] complex R/W mem test pass : 0
Mapping address range [0000000040000000:0000000140000000) as     cacheable | read-write | non-secure | normal
CBMEM:
IMD: root @ 00000000fffff000 254 entries.
IMD: root @ 00000000ffffec00 62 entries.
VBOOT: copying vboot_working_data (3840 bytes) to CBMEM...
out: cmd=0xa4: 03 6c a4 00 00 00 0c 00 00 01 00 00 50 7f 11 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Chrome EC: clear events_b mask to 0x0000000020004000
out: cmd=0xa4: 03 ea a4 00 00 00 0c 00 02 01 00 00 00 40 00 20 00 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/ramstage'
CBFS: Found @ offset 10b40 size d3a0
read SPI 0x5b9b94 0xd384: 16506 us, 3280 KB/s, 26.240 Mbps
Accumulated console time in romstage 0 ms


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 ramstage starting (log level: 8)...
ARM64: Exception handlers installed.
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_VPD found @ 550000 (16384 bytes)
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
read SPI 0x3f8600 0x7a00: 9523 us, 3279 KB/s, 26.232 Mbps
FMAP: area RW_VPD found @ 550000 (16384 bytes)
read SPI 0x550600 0x3a00: 4532 us, 3276 KB/s, 26.208 Mbps
BS: BS_PRE_DEVICE times (ms): entry 0 run 0 exit 0
BS: BS_DEV_INIT_CHIPS times (ms): entry 0 run 0 exit 0
Enumerating buses...
Show all devs... Before device enumeration.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
Compare with tree...
Root Device: enabled 1
 CPU_CLUSTER: 0: enabled 1
  CPU: 00: enabled 1
Root Device scanning...
root_dev_scan_bus for Root Device
CPU_CLUSTER: 0 enabled
root_dev_scan_bus for Root Device done
scan_bus: scanning of bus Root Device took 6 usecs
done
BS: BS_DEV_ENUMERATE times (ms): entry 0 run 0 exit 0
Allocating resources...
Reading resources...
Root Device read_resources bus 0 link: 0
CPU_CLUSTER: 0 read_resources bus 0 link: 0
CPU: 00 missing read_resources
CPU_CLUSTER: 0 read_resources bus 0 link: 0 done
Root Device read_resources bus 0 link: 0 done
Done reading resources.
Show resources in subtree (Root Device)...After reading.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Setting resources...
Root Device assign_resources, bus 0 link: 0
CPU_CLUSTER: 0 missing set_resources
Root Device assign_resources, bus 0 link: 0
Done setting resources.
Show resources in subtree (Root Device)...After assigning values.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Done allocating resources.
BS: BS_DEV_RESOURCES times (ms): entry 0 run 0 exit 0
Enabling resources...
done.
BS: BS_DEV_ENABLE times (ms): entry 0 run 0 exit 0
Initializing devices...
Root Device init ...
mainboard_init: Starting display init.
ADC[4]: Raw value=214388 ID=1
anx7625_power_on_init: Init interface.
anx7625_disable_pd_protocol: Disabled PD feature.
anx7625_power_on_init: Firmware: ver 0x0, rev 0x0.
anx7625_start_dp_work: Secure OCM version=00
anx7625_hpd_change_detect: HPD received 0x7e:0x45=0x91
sp_tx_get_edid_block: EDID Block = 1
Extracted contents:
header:          00 ff ff ff ff ff ff 00
serial number:   2c 82 30 11 00 00 00 00 31 1e
version:         01 04
basic params:    95 1a 0e 78 02
chroma info:     e1 c1 94 5b 59 94 29 22 50 54
established:     00 00 00
standard:        01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1:    3e 1c 56 a0 50 00 16 30 28 20 55 00 00 90 10 00 00 18
descriptor 2:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 3:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 4:    00 00 00 fe 00 4b 44 31 31 36 4e 32 39 33 30 41 30 32
extensions:      00
checksum:        f0

Manufacturer: KDB Model 1130 Serial Number 0
Made week 49 of 2020
EDID version: 1.4
Digital display
6 bits per primary color channel
DisplayPort interface
Maximum image size: 26 cm x 14 cm
Gamma: 220%
Check DPMS levels
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Established timings supported:
Standard timings supported:
Detailed timings
Hex of detail: 3e1c56a05000163028205500009010000018
Detailed mode (IN HEX): Clock 72300 KHz, 100 mm x 90 mm
               0556 057e 059e 05f6 hborder 0
               0300 0305 030a 0316 vborder 0
               -hsync -vsync 
Did detailed timing
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000fe004b443131364e32393330413032
ASCII string: KD116N2930A02
Checksum
Checksum: 0xf0 (valid)
get_active_panel: Found ID 1: 'KDB KD116N2930A02' 1366x768@0Hz
DSI data_rate: 433800000 bps
anx7625_parse_edid: set default k value to 0x3d for panel
anx7625_parse_edid: pixelclock(72300).
 hactive(1366), hsync(32), hfp(40), hbp(88)
 vactive(768), vsync(5), vfp(5), vbp(12)
anx7625_dsi_config: config dsi.
anx7625_dsi_video_config: compute M(15794176), N(737280), divider(8).
anx7625_dsi_config: success to config DSI
anx7625_dp_start: MIPI phy setup OK.
[SSUSB] Setting up USB HOST controller...
[SSUSB] u3phy_ports_enable u2p:1, u3p:0
[SSUSB] phy power-on done.
out: cmd=0xf: 03 d9 0f 00 00 00 04 00 11 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
SPM: pcm index = 1
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'pcm_allinone_lp4_3200.bin'
CBFS: Found @ offset 1e400 size 1026
read SPI 0x5c7448 0x1026: 1271 us, 3252 KB/s, 26.016 Mbps
SPM: binary array size = 2988
SPM: version = pcm_allinone_v1.17.2_20180829
SPM binary loaded in 2 msecs
spm_kick_im_to_fetch: ptr = 000000004021ee82
spm_kick_im_to_fetch: len = 2988
SPM: spm_kick_pcm_to_run
SPM: spm_kick_pcm_to_run done
SPM: spm_init done in 5 msecs
Root Device init finished in 246173 usecs
CPU_CLUSTER: 0 init ...
Mapping address range [0000000000200000:0000000000280000) as     cacheable | read-write |     secure | device
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'sspm.bin'
CBFS: Found @ offset 20500 size 41cb
read SPI 0x5c9538 0x41cb: 5142 us, 3275 KB/s, 26.200 Mbps
CPU_CLUSTER: 0 init finished in 8338 usecs
Devices initialized
Show all devs... After init.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
BS: BS_DEV_INIT times (ms): entry 0 run 254 exit 0
FMAP: area RW_ELOG found @ 558000 (4096 bytes)
ELOG: NV offset 0x558000 size 0x1000
read SPI 0x558000 0x1000: 1263 us, 3243 KB/s, 25.944 Mbps
ELOG: area is 4096 bytes, full threshold 3842, shrink size 1024
ELOG: Event(17) added with size 13 at 2025-02-28 18:46:18 UTC
out: cmd=0x121: 03 db 21 01 00 00 00 00 
in-header: 03 ce 00 00 2c 00 00 00 
in-data: e2 04 00 00 00 00 00 00 02 08 00 00 08 00 00 00 74 36 95 9b 08 00 00 00 69 89 00 00 08 00 00 00 5c 37 00 00 08 00 00 00 5b 4a e1 0e 
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 54 a4 00 00 00 0c 00 00 01 00 00 f8 ff 01 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
ELOG: Event(A0) added with size 9 at 2025-02-28 18:46:18 UTC
elog_add_boot_reason: Logged dev mode boot
Finalize devices...
Devices finalized
BS: BS_POST_DEVICE times (ms): entry 3 run 0 exit 0
BS: BS_OS_RESUME_CHECK times (ms): entry 0 run 0 exit 0
Writing coreboot table at 0xffed9000
 0. 0000000000114000-000000000011efff: RAMSTAGE
 1. 0000000040000000-000000004023cfff: RAMSTAGE
 2. 000000004023d000-00000000545fffff: RAM
 3. 0000000054600000-000000005465ffff: BL31
 4. 0000000054660000-00000000ffed8fff: RAM
 5. 00000000ffed9000-00000000ffffffff: CONFIGURATION TABLES
 6. 0000000100000000-000000013fffffff: RAM
Passing 5 GPIOs to payload:
            NAME |       PORT | POLARITY |     VALUE
   write protect | 0x00000096 |      low |       low
        EC in RW | 0x000000b1 |     high | undefined
    EC interrupt | 0x00000097 |      low | undefined
   TPM interrupt | 0x00000099 |     high | undefined
  speaker enable | 0x000000af |     high | undefined
out: cmd=0x6: 03 f7 06 00 00 00 00 00 
in-header: 03 f2 00 00 02 00 00 00 
in-data: 09 00 
Board ID: 9
ADC[3]: Raw value=1249760 ID=10
RAM code: 10
SKU ID: 17
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
Wrote coreboot table at: 00000000ffed9000, 0x368 bytes, checksum a8c5
coreboot table: 896 bytes.
IMD ROOT    0. 00000000fffff000 00001000
IMD SMALL   1. 00000000ffffe000 00001000
CONSOLE     2. 00000000fffde000 00020000
FMAP        3. 00000000fffdd000 0000047c
TIME STAMP  4. 00000000fffdc000 00000910
VBOOT WORK  5. 00000000fffdb000 00000f00
RAMOOPS     6. 00000000ffedb000 00100000
COREBOOT    7. 00000000ffed9000 00002000
IMD small region:
  IMD ROOT    0. 00000000ffffec00 00000400
  EC HOSTEVENT 1. 00000000ffffebe0 00000008
  VPD         2. 00000000ffffe9a0 0000022d
BS: BS_WRITE_TABLES times (ms): entry 0 run 0 exit 0
out: cmd=0xa4: 03 e0 a4 00 00 00 0c 00 00 01 00 00 dc 2f 21 40 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Probing TPM:  done!
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
Checking cr50 for pending updates
Reading cr50 TPM mode
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/payload'
CBFS: Found @ offset 50180 size 16deb
read SPI 0x5f91b8 0x16deb: 28555 us, 3280 KB/s, 26.240 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000080000000 memsize 0x11809c0 srcaddr 0x000000004000b438 filesize 0x16db3
Loading Segment: addr: 0x0000000080000000 memsz: 0x00000000011809c0 filesz: 0x0000000000016db3
using LZMA
[ 0x80000000, 80033268, 0x811809c0) <- 4000b438
Clearing Segment: addr: 0x0000000080033268 memsz: 0x000000000114d758
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000080000000
Loaded segments
BS: BS_PAYLOAD_LOAD times (ms): entry 9 run 45 exit 0
Jumping to boot code at 0000000080000000(00000000ffed9000)
CPU0: stack: 0000000000114000 - 0000000000118000, lowest used address 00000000001176a0, stack used: 2400 bytes
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/bl31'
CBFS: Found @ offset 36a00 size 4b17
read SPI 0x5dfa28 0x4b17: 5866 us, 3277 KB/s, 26.216 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000054600000 memsize 0x27000 srcaddr 0x000000004000b438 filesize 0x4adf
Loading Segment: addr: 0x0000000054600000 memsz: 0x0000000000027000 filesz: 0x0000000000004adf
using LZMA
[ 0x54600000, 5460d408, 0x54627000) <- 4000b438
Clearing Segment: addr: 0x000000005460d408 memsz: 0x0000000000019bf8
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000054601000
Loaded segments
NOTICE:  MT8183 bl31_setup
NOTICE:  BL31: v2.1(release):v2.1-809-g62969c490
NOTICE:  BL31: Built : Mon May 30 03:26:46 UTC 2022
INFO:    [DEVAPC] dump DEVAPC registers:
INFO:    [DEVAPC] (INFRA)D0_APC_0 = 0x0, (INFRA)D1_APC_0 = 0xfcfffffc, (INFRA)D2_APC_0 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_1 = 0x0, (INFRA)D1_APC_1 = 0xffffffff, (INFRA)D2_APC_1 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_2 = 0x0, (INFRA)D1_APC_2 = 0xffffffff, (INFRA)D2_APC_2 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_3 = 0x0, (INFRA)D1_APC_3 = 0xffffffff, (INFRA)D2_APC_3 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_4 = 0x80000000, (INFRA)D1_APC_4 = 0xffffffff, (INFRA)D2_APC_4 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_5 = 0x2aaa, (INFRA)D1_APC_5 = 0xfcff3fff, (INFRA)D2_APC_5 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_6 = 0x0, (INFRA)D1_APC_6 = 0xffffffff, (INFRA)D2_APC_6 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_7 = 0x0, (INFRA)D1_APC_7 = 0xffffffff, (INFRA)D2_APC_7 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_8 = 0x0, (INFRA)D1_APC_8 = 0xffffffff, (INFRA)D2_APC_8 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_9 = 0x0, (INFRA)D1_APC_9 = 0xffffffff, (INFRA)D2_APC_9 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_10 = 0x0, (INFRA)D1_APC_10 = 0xffffffff, (INFRA)D2_APC_10 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_11 = 0x0, (INFRA)D1_APC_11 = 0xffffffff, (INFRA)D2_APC_11 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_12 = 0x0, (INFRA)D1_APC_12 = 0xff, (INFRA)D2_APC_12 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_0 = 0x0, (MM)D1_APC_0 = 0xffc000ff, (MM)D2_APC_0 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_1 = 0x0, (MM)D1_APC_1 = 0x3fffffff, (MM)D2_APC_1 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_2 = 0x0, (MM)D1_APC_2 = 0xcffff33c, (MM)D2_APC_2 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_3 = 0x0, (MM)D1_APC_3 = 0x3ccfc0ff, (MM)D2_APC_3 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_4 = 0x0, (MM)D1_APC_4 = 0xffff0000, (MM)D2_APC_4 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_5 = 0x0, (MM)D1_APC_5 = 0xffffffff, (MM)D2_APC_5 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_6 = 0x0, (MM)D1_APC_6 = 0xffffffff, (MM)D2_APC_6 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_7 = 0x0, (MM)D1_APC_7 = 0xffffffff, (MM)D2_APC_7 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_8 = 0x0, (MM)D1_APC_8 = 0x3ffffff, (MM)D2_APC_8 = 0x0
INFO:    [DEVAPC] MAS_DOM_0 = 0x1
INFO:    [DEVAPC] MAS_DOM_1 = 0x200
INFO:    [DEVAPC] MAS_DOM_2 = 0x0
INFO:    [DEVAPC] MAS_DOM_3 = 0x2000
INFO:    [DEVAPC] MAS_SEC_0 = 0x8000000
INFO:    [DEVAPC]  (INFRA)MAS_DOMAIN_REMAP_0 = 0x88, (INFRA)MAS_DOMAIN_REMAP_1 = 0x0
INFO:    [DEVAPC]  (MM)MAS_DOMAIN_REMAP_0 = 0x24
WARNING: region 0:
WARNING: 	apc:0x168, sa:0x0, ea:0xfff
WARNING: region 1:
WARNING: 	apc:0x140, sa:0x1000, ea:0x128f
WARNING: region 2:
WARNING: 	apc:0x168, sa:0x1290, ea:0x1fff
WARNING: region 3:
WARNING: 	apc:0x168, sa:0x2000, ea:0xbfff
WARNING: region 4:
WARNING: 	apc:0x168, sa:0xc000, ea:0x1ffff
WARNING: region 5:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 6:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 7:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
INFO:    GICv3 without legacy support detected. ARM GICv3 driver initialized in EL3
INFO:    SPM: enable SPMC mode
NOTICE:  spm_boot_init() start
NOTICE:  spm_boot_init() end
INFO:    BL31: Initializing runtime services
INFO:    BL31: Preparing for EL3 exit to normal world
INFO:    Entry point address = 0x80000000
INFO:    SPSR = 0x8


Starting depthcharge on Juniper...
vboot_handoff: creating legacy vboot_handoff structure
vboot_handoff: copying FW preamble
ec_init(0): CrosEC protocol v3 supported (544, 544)
Wipe memory regions:
	[0x00000040000000, 0x00000054600000)
	[0x00000054660000, 0x00000080000000)
	[0x000000811809c0, 0x000000ffed9000)
	[0x00000100000000, 0x00000140000000)
Initializing XHCI USB controller at 0x11200000.
Calling VbSelectAndLoadKernel().
Connected to device vid:did:rid of 1ae0:0028:00
tpm_get_response: command 0x14e, return code 0x0
ReadSpaceKernel: TPM: read secdata_kernel: 02 4c 57 52 47 01 00 01 00 00 00 00 55
RollbackKernelRead: TPM: RollbackKernelRead 0x10001
tpm_get_response: command 0x14e, return code 0x28b
RollbackFwmpRead: TPM: no FWMP space
VbSelectAndLoadKernel: GBB flags are 0x0
print_hash: RW(active) hash: fb5c0dfa6c2692bec07dda7f769b1ccaa90b944b36137e9ce9d22c3b38a385f7
Trying to locate 'ecrw.hash' in CBFS
sync_one_ec: devidx=0 select_rw=4
sync_one_ec: jumping to EC-RW
EC returned from reboot after 22924us
Waiting for EC to clear limit power flag.
vb2_developer_ui: Entering
vboot_draw_screen: screen=0x101 locale=1
CBGFX: cbgfx initialized: screen:width=1366, height=768, offset=0 canvas:width=768, height=768, offset=299
vboot_init_locale: Supported locales: en, es-419, pt-BR, fr, es, pt-PT, ca, it, de, el, nl, da, nb, sv, fi, et, lv, lt, ru, pl, cs, sk, hu, sl, sr, hr, bg, ro, uk, tr, he, ar, fa, hi, th, ms, vi, id, fil, zh-CN, zh-TW, ko, ja, bn, gu, kn, ml, mr, ta, te, (50 locales)
load_archive: loading vbgfx.bin
load_archive: loading font.bin
load_archive: loading locale_es-419.bin
vb2_developer_ui: VbBootDeveloper() - user pressed Ctrl+D; skip delay
vb2_developer_ui: VbBootDeveloper() - trying fixed disk
Man 000045 Snr 2556076829 Product DA4032 Revision 0.1
VbTryLoadKernel: trying disk 0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s0 t6 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 2
LoadKernel: Found kernel entry at 69 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
vb2_load_partition: read 13036 KB in 294 ms at 44225 KB/s.
vb2_load_partition: Partition is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s0 t5 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 4
LoadKernel: Found kernel entry at 65605 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65540
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s0 t5 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry no more kernels
WriteAndFreeGptData: Updating GPT header 1
WriteAndFreeGptData: Updating GPT entries 1
WriteAndFreeGptData: Updating GPT header 2
WriteAndFreeGptData: Updating GPT entries 2
LoadKernel: Good partition 2
VbTryLoadKernel: LoadKernel() = 0x0
vboot_draw_screen: screen=0x0 locale=1
tpm_get_response: command 0x121, return code 0x0
RollbackKernelLock: TPM: lock secdata_kernel returned 0x0
VbSelectAndLoadKernel: Returning 0
Boot policy: Match for type 0 with cmdline 1
Modified kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=47d76b39-16be-466f-b19f-dc9f958d5218/PARTNROFF=1 hashtree=PARTUUID=47d76b39-16be-466f-b19f-dc9f958d5218/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=37bb1d5b94fc22fc087a6fc30c52c8ff821888c7a42db52786f1757378f13209 salt=069192dc92974be001b40a2526a38f4beb643144cc0ab1d4fede1e0dc3713570" noinitrd vt.global_cursor_default=0 kern_guid=47d76b39-16be-466f-b19f-dc9f958d5218 cros_lsb_release_hash=2NJNHDfRNLBa6AWdW//FQQS/e8Wnw4rISSdAHuhgl2U= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
Loading FIT.
Image fdt-36 has 16926 bytes.
Image fdt-35 has 16925 bytes.
Image fdt-34 has 16908 bytes.
Image fdt-33 has 16949 bytes.
Image fdt-32 has 16948 bytes.
Image fdt-31 has 16906 bytes.
Image fdt-30 has 17326 bytes.
Image fdt-29 has 17015 bytes.
Image fdt-28 has 17370 bytes.
Image fdt-27 has 17045 bytes.
Image fdt-26 has 17379 bytes.
Image fdt-25 has 17262 bytes.
Image fdt-24 has 17520 bytes.
Image fdt-23 has 17472 bytes.
Image fdt-22 has 17222 bytes.
Image fdt-21 has 17239 bytes.
Image fdt-20 has 17182 bytes.
Image fdt-19 has 17230 bytes.
Image fdt-18 has 17489 bytes.
Image fdt-17 has 17485 bytes.
Image fdt-16 has 17224 bytes.
Image fdt-15 has 17269 bytes.
Image fdt-14 has 17105 bytes.
Image fdt-13 has 17202 bytes.
Image fdt-12 has 17476 bytes.
Image fdt-11 has 17217 bytes.
Image fdt-10 has 17236 bytes.
Image fdt-9 has 17492 bytes.
Image fdt-8 has 17550 bytes.
Image fdt-7 has 17462 bytes.
Image fdt-6 has 17196 bytes.
Image fdt-5 has 17430 bytes.
Image fdt-4 has 17178 bytes.
Image fdt-3 has 17199 bytes.
Image fdt-2 has 17151 bytes.
Image fdt-1 has 17405 bytes.
Image kernel-1 has 12637811 bytes.
Compat preference: google,juniper-rev9-sku17 google,juniper-sku17 google,juniper-rev9 google,juniper
Config conf-36, kernel kernel-1, fdt fdt-36, compat google,krane-sku176 google,krane mediatek,mt8183
Config conf-35, kernel kernel-1, fdt fdt-35, compat google,krane-sku0 google,krane mediatek,mt8183
Config conf-34, kernel kernel-1, fdt fdt-34, compat google,kodama-sku32 google,kodama mediatek,mt8183
Config conf-33, kernel kernel-1, fdt fdt-33, compat google,kodama-sku288 google,kodama mediatek,mt8183
Config conf-32, kernel kernel-1, fdt fdt-32, compat google,kodama-sku272 google,kodama mediatek,mt8183
Config conf-31, kernel kernel-1, fdt fdt-31, compat google,kodama-sku16 google,kodama mediatek,mt8183
Config conf-30, kernel kernel-1, fdt fdt-30, compat google,katsu mediatek,mt8183
Config conf-29, kernel kernel-1, fdt fdt-29, compat google,katsu-sku38 google,katsu mediatek,mt8183
Config conf-28, kernel kernel-1, fdt fdt-28, compat google,kakadu-rev3 google,kakadu-rev2 google,kakadu mediatek,mt8183
Config conf-27, kernel kernel-1, fdt fdt-27, compat google,kakadu-rev3-sku22 google,kakadu-rev2-sku22 google,kakadu mediatek,mt8183
Config conf-26, kernel kernel-1, fdt fdt-26, compat google,kakadu-rev1 google,kakadu-rev0 google,kakadu mediatek,mt8183
Config conf-25, kernel kernel-1, fdt fdt-25, compat google,willow-sku1 google,willow mediatek,mt8183
Config conf-24, kernel kernel-1, fdt fdt-24, compat google,willow-sku0 google,willow mediatek,mt8183
Config conf-23, kernel kernel-1, fdt fdt-23, compat google,cerise-sku1 google,cerise mediatek,mt8183
Config conf-22, kernel kernel-1, fdt fdt-22, compat google,cerise-rev3-sku1 google,cerise mediatek,mt8183
Config conf-21, kernel kernel-1, fdt fdt-21, compat google,pico-sku2 google,pico mediatek,mt8183
Config conf-20, kernel kernel-1, fdt fdt-20, compat google,pico-sku1 google,pico mediatek,mt8183
Config conf-19, kernel kernel-1, fdt fdt-19, compat google,makomo-rev4-sku1 google,makomo-rev5-sku1 google,makomo mediatek,mt8183
Config conf-18, kernel kernel-1, fdt fdt-18, compat google,makomo-rev4-sku0 google,makomo-rev5-sku0 google,makomo mediatek,mt8183
Config conf-17, kernel kernel-1, fdt fdt-17, compat google,makomo-rev3-sku0 google,makomo mediatek,mt8183
Config conf-16, kernel kernel-1, fdt fdt-16, compat google,makomo-rev0-sku0 google,makomo mediatek,mt8183
Config conf-15, kernel kernel-1, fdt fdt-15, compat google,juniper-sku17 (match) google,juniper mediatek,mt8183
Config conf-14, kernel kernel-1, fdt fdt-14, compat google,kappa mediatek,mt8183
Config conf-13, kernel kernel-1, fdt fdt-13, compat google,juniper-sku16 google,juniper (match) mediatek,mt8183
Config conf-12, kernel kernel-1, fdt fdt-12, compat google,fennel-sku0 google,fennel mediatek,mt8183
Config conf-11, kernel kernel-1, fdt fdt-11, compat google,fennel-sku2 google,fennel mediatek,mt8183
Config conf-10, kernel kernel-1, fdt fdt-10, compat google,fennel-sku7 google,fennel mediatek,mt8183
Config conf-9, kernel kernel-1, fdt fdt-9, compat google,fennel-sku6 google,fennel mediatek,mt8183
Config conf-8, kernel kernel-1, fdt fdt-8, compat google,fennel-sku1 google,fennel mediatek,mt8183
Config conf-7, kernel kernel-1, fdt fdt-7, compat google,damu mediatek,mt8183
Config conf-6, kernel kernel-1, fdt fdt-6, compat google,cozmo mediatek,mt8183
Config conf-5, kernel kernel-1, fdt fdt-5, compat google,cerise-sku0 google,cerise mediatek,mt8183
Config conf-4, kernel kernel-1, fdt fdt-4, compat google,cerise-rev3-sku0 google,cerise mediatek,mt8183
Config conf-3, kernel kernel-1, fdt fdt-3, compat google,burnet mediatek,mt8183
Config conf-2, kernel kernel-1, fdt fdt-2, compat google,bellis-rev0-sku1 google,bellis mediatek,mt8183
Config conf-1, kernel kernel-1, fdt fdt-1, compat google,bellis-rev0-sku0 google,bellis mediatek,mt8183
Choosing best match conf-15 for compat google,juniper-sku17.
LZ4 decompressing fdt-15 to 0x5f800000
tpm_get_response: command 0x17b, return code 0x0
tpm_cleanup: add release locality here.
Shutting down all USB controllers.
Exiting depthcharge with code 4 at timestamp: 5402854
LZ4 decompressing kernel-1 to 0x8017b418
LZ4 decompressing kernel-1 to 0x40000000
jumping to kernel
WARNING: Unimplemented Arm Architecture Service Call: 0x80000002 
INFO:    PSCI Power Domain Map:
INFO:      Domain Node : Level 2, parent_node -1, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      CPU Node : MPID 0x0, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x1, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x2, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x3, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x100, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x101, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x102, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x103, parent_node 2, State ON (0x0)


coreboot-v1.9308_26_0.0.22-10544-g50eadf7c92 Mon Feb  8 05:04:19 UTC 2021 verstage starting (log level: 8)...
ARM64: Exception handlers installed.
WDT: Last reset was cold boot
SPI0(PAD0) initialized at 992727 Hz
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
Probing TPM: . done!
TPM ready after 0 ms
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
tlcl_send_startup: Startup return code is 0
TPM: setup succeeded
src/security/tpm/tss/tcg-2.0/tss.c:223 index 0x1007 return code 0
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
Phase 1
FMAP: area GBB found @ 3f5000 (12032 bytes)
VB2:vb2_check_recovery() Recovery reason from previous boot: 0x0 / 0x0
Phase 2
Phase 3
FMAP: area GBB found @ 3f5000 (12032 bytes)
read SPI 0x3f5180 0x1000: 1295 us, 3162 KB/s, 25.296 Mbps
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_keyblock() Checking key block signature...
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_fw_preamble() Verifying preamble.
Phase 4
FMAP: area FW_MAIN_B found @ 5a9000 (1367808 bytes)
VB2:vb2api_init_hash() HW crypto for hash_alg 2 not supported, using SW
Saving nvdata
tlcl_extend: response is 0
tlcl_extend: response is 0
tlcl_lock_nv_write: response is 0
Slot B is selected


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 romstage starting (log level: 8)...
ARM64: Exception handlers installed.
[RTC]rtc_enable_dcxo,41: con=0x482, osc32con=0x826f, sec=0x2002
[RTC]rtc_check_state,142: con=482, pwrkey1=a357, pwrkey2=67d2
[RTC]rtc_eosc_cali,157: PMIC_RG_FQMTR_CKSEL=0x4a
[RTC]rtc_get_frequency_meter,134: input=0xf, output=792
[RTC]rtc_osc_init,208: EOSC32 cali val = 0x826f
[RTC]rtc_boot_common,186: irqsta=0, bbpu=0, con=482
[RTC]rtc_bbpu_power_on,373: rtc_write_trigger=1
[RTC]rtc_bbpu_power_on,376: done BBPU=0x9
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_DDR_TRAINING found @ 556000 (8192 bytes)
read_calibration_data_from_flash: ret=0x8f0, length=0x8f0
DRAM-K: Fast Calibration
Calibration params loaded from flash
Run calibration (freq: 1600, first: 1)
Vendor id is 0x6
Run calibration (freq: 2400, first: 0)
Vendor id is 0x6
Run calibration (freq: 3200, first: 0)
Vendor id is 0x6
[MEM] complex R/W mem test pass : 0
[MEM] complex R/W mem test pass : 0
Mapping address range [0000000040000000:0000000140000000) as     cacheable | read-write | non-secure | normal
CBMEM:
IMD: root @ 00000000fffff000 254 entries.
IMD: root @ 00000000ffffec00 62 entries.
VBOOT: copying vboot_working_data (3840 bytes) to CBMEM...
out: cmd=0xa4: 03 6c a4 00 00 00 0c 00 00 01 00 00 50 7f 11 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Chrome EC: clear events_b mask to 0x0000000020004000
out: cmd=0xa4: 03 ea a4 00 00 00 0c 00 02 01 00 00 00 40 00 20 00 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/ramstage'
CBFS: Found @ offset 10b40 size d3a0
read SPI 0x5b9b94 0xd384: 16506 us, 3280 KB/s, 26.240 Mbps
Accumulated console time in romstage 0 ms


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 ramstage starting (log level: 8)...
ARM64: Exception handlers installed.
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_VPD found @ 550000 (16384 bytes)
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
read SPI 0x3f8600 0x7a00: 9522 us, 3279 KB/s, 26.232 Mbps
FMAP: area RW_VPD found @ 550000 (16384 bytes)
read SPI 0x550600 0x3a00: 4533 us, 3275 KB/s, 26.200 Mbps
BS: BS_PRE_DEVICE times (ms): entry 0 run 0 exit 0
BS: BS_DEV_INIT_CHIPS times (ms): entry 0 run 0 exit 0
Enumerating buses...
Show all devs... Before device enumeration.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
Compare with tree...
Root Device: enabled 1
 CPU_CLUSTER: 0: enabled 1
  CPU: 00: enabled 1
Root Device scanning...
root_dev_scan_bus for Root Device
CPU_CLUSTER: 0 enabled
root_dev_scan_bus for Root Device done
scan_bus: scanning of bus Root Device took 7 usecs
done
BS: BS_DEV_ENUMERATE times (ms): entry 0 run 0 exit 0
Allocating resources...
Reading resources...
Root Device read_resources bus 0 link: 0
CPU_CLUSTER: 0 read_resources bus 0 link: 0
CPU: 00 missing read_resources
CPU_CLUSTER: 0 read_resources bus 0 link: 0 done
Root Device read_resources bus 0 link: 0 done
Done reading resources.
Show resources in subtree (Root Device)...After reading.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Setting resources...
Root Device assign_resources, bus 0 link: 0
CPU_CLUSTER: 0 missing set_resources
Root Device assign_resources, bus 0 link: 0
Done setting resources.
Show resources in subtree (Root Device)...After assigning values.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Done allocating resources.
BS: BS_DEV_RESOURCES times (ms): entry 0 run 0 exit 0
Enabling resources...
done.
BS: BS_DEV_ENABLE times (ms): entry 0 run 0 exit 0
Initializing devices...
Root Device init ...
mainboard_init: Starting display init.
ADC[4]: Raw value=214746 ID=1
anx7625_power_on_init: Init interface.
anx7625_disable_pd_protocol: Disabled PD feature.
anx7625_power_on_init: Firmware: ver 0x0, rev 0x0.
anx7625_start_dp_work: Secure OCM version=00
anx7625_hpd_change_detect: HPD received 0x7e:0x45=0x91
sp_tx_get_edid_block: EDID Block = 1
Extracted contents:
header:          00 ff ff ff ff ff ff 00
serial number:   2c 82 30 11 00 00 00 00 31 1e
version:         01 04
basic params:    95 1a 0e 78 02
chroma info:     e1 c1 94 5b 59 94 29 22 50 54
established:     00 00 00
standard:        01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1:    3e 1c 56 a0 50 00 16 30 28 20 55 00 00 90 10 00 00 18
descriptor 2:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 3:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 4:    00 00 00 fe 00 4b 44 31 31 36 4e 32 39 33 30 41 30 32
extensions:      00
checksum:        f0

Manufacturer: KDB Model 1130 Serial Number 0
Made week 49 of 2020
EDID version: 1.4
Digital display
6 bits per primary color channel
DisplayPort interface
Maximum image size: 26 cm x 14 cm
Gamma: 220%
Check DPMS levels
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Established timings supported:
Standard timings supported:
Detailed timings
Hex of detail: 3e1c56a05000163028205500009010000018
Detailed mode (IN HEX): Clock 72300 KHz, 100 mm x 90 mm
               0556 057e 059e 05f6 hborder 0
               0300 0305 030a 0316 vborder 0
               -hsync -vsync 
Did detailed timing
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000fe004b443131364e32393330413032
ASCII string: KD116N2930A02
Checksum
Checksum: 0xf0 (valid)
get_active_panel: Found ID 1: 'KDB KD116N2930A02' 1366x768@0Hz
DSI data_rate: 433800000 bps
anx7625_parse_edid: set default k value to 0x3d for panel
anx7625_parse_edid: pixelclock(72300).
 hactive(1366), hsync(32), hfp(40), hbp(88)
 vactive(768), vsync(5), vfp(5), vbp(12)
anx7625_dsi_config: config dsi.
anx7625_dsi_video_config: compute M(15794176), N(737280), divider(8).
anx7625_dsi_config: success to config DSI
anx7625_dp_start: MIPI phy setup OK.
[SSUSB] Setting up USB HOST controller...
[SSUSB] u3phy_ports_enable u2p:1, u3p:0
[SSUSB] phy power-on done.
out: cmd=0xf: 03 d9 0f 00 00 00 04 00 11 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
SPM: pcm index = 1
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'pcm_allinone_lp4_3200.bin'
CBFS: Found @ offset 1e400 size 1026
read SPI 0x5c7448 0x1026: 1271 us, 3252 KB/s, 26.016 Mbps
SPM: binary array size = 2988
SPM: version = pcm_allinone_v1.17.2_20180829
SPM binary loaded in 2 msecs
spm_kick_im_to_fetch: ptr = 000000004021ee82
spm_kick_im_to_fetch: len = 2988
SPM: spm_kick_pcm_to_run
SPM: spm_kick_pcm_to_run done
SPM: spm_init done in 5 msecs
Root Device init finished in 246164 usecs
CPU_CLUSTER: 0 init ...
Mapping address range [0000000000200000:0000000000280000) as     cacheable | read-write |     secure | device
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'sspm.bin'
CBFS: Found @ offset 20500 size 41cb
read SPI 0x5c9538 0x41cb: 5142 us, 3275 KB/s, 26.200 Mbps
CPU_CLUSTER: 0 init finished in 8334 usecs
Devices initialized
Show all devs... After init.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
BS: BS_DEV_INIT times (ms): entry 0 run 254 exit 0
FMAP: area RW_ELOG found @ 558000 (4096 bytes)
ELOG: NV offset 0x558000 size 0x1000
read SPI 0x558000 0x1000: 1259 us, 3253 KB/s, 26.024 Mbps
ELOG: area is 4096 bytes, full threshold 3842, shrink size 1024
ELOG: Event(17) added with size 13 at 2025-02-28 18:52:47 UTC
out: cmd=0x121: 03 db 21 01 00 00 00 00 
in-header: 03 57 00 00 2c 00 00 00 
in-data: 5c 04 00 00 00 00 00 00 02 08 00 00 08 00 00 00 69 89 00 00 08 00 00 00 5c 37 00 00 08 00 00 00 5b 4a e1 0e 08 00 00 00 e6 ec 05 00 
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 54 a4 00 00 00 0c 00 00 01 00 00 f8 ff 01 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
ELOG: Event(A0) added with size 9 at 2025-02-28 18:52:47 UTC
elog_add_boot_reason: Logged dev mode boot
Finalize devices...
Devices finalized
BS: BS_POST_DEVICE times (ms): entry 3 run 0 exit 0
BS: BS_OS_RESUME_CHECK times (ms): entry 0 run 0 exit 0
Writing coreboot table at 0xffed9000
 0. 0000000000114000-000000000011efff: RAMSTAGE
 1. 0000000040000000-000000004023cfff: RAMSTAGE
 2. 000000004023d000-00000000545fffff: RAM
 3. 0000000054600000-000000005465ffff: BL31
 4. 0000000054660000-00000000ffed8fff: RAM
 5. 00000000ffed9000-00000000ffffffff: CONFIGURATION TABLES
 6. 0000000100000000-000000013fffffff: RAM
Passing 5 GPIOs to payload:
            NAME |       PORT | POLARITY |     VALUE
   write protect | 0x00000096 |      low |       low
        EC in RW | 0x000000b1 |     high | undefined
    EC interrupt | 0x00000097 |      low | undefined
   TPM interrupt | 0x00000099 |     high | undefined
  speaker enable | 0x000000af |     high | undefined
out: cmd=0x6: 03 f7 06 00 00 00 00 00 
in-header: 03 f2 00 00 02 00 00 00 
in-data: 09 00 
Board ID: 9
ADC[3]: Raw value=1253346 ID=10
RAM code: 10
SKU ID: 17
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
Wrote coreboot table at: 00000000ffed9000, 0x368 bytes, checksum a8c5
coreboot table: 896 bytes.
IMD ROOT    0. 00000000fffff000 00001000
IMD SMALL   1. 00000000ffffe000 00001000
CONSOLE     2. 00000000fffde000 00020000
FMAP        3. 00000000fffdd000 0000047c
TIME STAMP  4. 00000000fffdc000 00000910
VBOOT WORK  5. 00000000fffdb000 00000f00
RAMOOPS     6. 00000000ffedb000 00100000
COREBOOT    7. 00000000ffed9000 00002000
IMD small region:
  IMD ROOT    0. 00000000ffffec00 00000400
  EC HOSTEVENT 1. 00000000ffffebe0 00000008
  VPD         2. 00000000ffffe9a0 0000022d
BS: BS_WRITE_TABLES times (ms): entry 0 run 0 exit 0
out: cmd=0xa4: 03 e0 a4 00 00 00 0c 00 00 01 00 00 dc 2f 21 40 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Probing TPM:  done!
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
Checking cr50 for pending updates
Reading cr50 TPM mode
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/payload'
CBFS: Found @ offset 50180 size 16deb
read SPI 0x5f91b8 0x16deb: 28554 us, 3280 KB/s, 26.240 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000080000000 memsize 0x11809c0 srcaddr 0x000000004000b438 filesize 0x16db3
Loading Segment: addr: 0x0000000080000000 memsz: 0x00000000011809c0 filesz: 0x0000000000016db3
using LZMA
[ 0x80000000, 80033268, 0x811809c0) <- 4000b438
Clearing Segment: addr: 0x0000000080033268 memsz: 0x000000000114d758
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000080000000
Loaded segments
BS: BS_PAYLOAD_LOAD times (ms): entry 9 run 45 exit 0
Jumping to boot code at 0000000080000000(00000000ffed9000)
CPU0: stack: 0000000000114000 - 0000000000118000, lowest used address 00000000001176a0, stack used: 2400 bytes
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/bl31'
CBFS: Found @ offset 36a00 size 4b17
read SPI 0x5dfa28 0x4b17: 5866 us, 3277 KB/s, 26.216 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000054600000 memsize 0x27000 srcaddr 0x000000004000b438 filesize 0x4adf
Loading Segment: addr: 0x0000000054600000 memsz: 0x0000000000027000 filesz: 0x0000000000004adf
using LZMA
[ 0x54600000, 5460d408, 0x54627000) <- 4000b438
Clearing Segment: addr: 0x000000005460d408 memsz: 0x0000000000019bf8
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000054601000
Loaded segments
NOTICE:  MT8183 bl31_setup
NOTICE:  BL31: v2.1(release):v2.1-809-g62969c490
NOTICE:  BL31: Built : Mon May 30 03:26:46 UTC 2022
INFO:    [DEVAPC] dump DEVAPC registers:
INFO:    [DEVAPC] (INFRA)D0_APC_0 = 0x0, (INFRA)D1_APC_0 = 0xfcfffffc, (INFRA)D2_APC_0 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_1 = 0x0, (INFRA)D1_APC_1 = 0xffffffff, (INFRA)D2_APC_1 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_2 = 0x0, (INFRA)D1_APC_2 = 0xffffffff, (INFRA)D2_APC_2 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_3 = 0x0, (INFRA)D1_APC_3 = 0xffffffff, (INFRA)D2_APC_3 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_4 = 0x80000000, (INFRA)D1_APC_4 = 0xffffffff, (INFRA)D2_APC_4 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_5 = 0x2aaa, (INFRA)D1_APC_5 = 0xfcff3fff, (INFRA)D2_APC_5 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_6 = 0x0, (INFRA)D1_APC_6 = 0xffffffff, (INFRA)D2_APC_6 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_7 = 0x0, (INFRA)D1_APC_7 = 0xffffffff, (INFRA)D2_APC_7 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_8 = 0x0, (INFRA)D1_APC_8 = 0xffffffff, (INFRA)D2_APC_8 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_9 = 0x0, (INFRA)D1_APC_9 = 0xffffffff, (INFRA)D2_APC_9 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_10 = 0x0, (INFRA)D1_APC_10 = 0xffffffff, (INFRA)D2_APC_10 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_11 = 0x0, (INFRA)D1_APC_11 = 0xffffffff, (INFRA)D2_APC_11 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_12 = 0x0, (INFRA)D1_APC_12 = 0xff, (INFRA)D2_APC_12 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_0 = 0x0, (MM)D1_APC_0 = 0xffc000ff, (MM)D2_APC_0 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_1 = 0x0, (MM)D1_APC_1 = 0x3fffffff, (MM)D2_APC_1 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_2 = 0x0, (MM)D1_APC_2 = 0xcffff33c, (MM)D2_APC_2 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_3 = 0x0, (MM)D1_APC_3 = 0x3ccfc0ff, (MM)D2_APC_3 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_4 = 0x0, (MM)D1_APC_4 = 0xffff0000, (MM)D2_APC_4 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_5 = 0x0, (MM)D1_APC_5 = 0xffffffff, (MM)D2_APC_5 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_6 = 0x0, (MM)D1_APC_6 = 0xffffffff, (MM)D2_APC_6 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_7 = 0x0, (MM)D1_APC_7 = 0xffffffff, (MM)D2_APC_7 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_8 = 0x0, (MM)D1_APC_8 = 0x3ffffff, (MM)D2_APC_8 = 0x0
INFO:    [DEVAPC] MAS_DOM_0 = 0x1
INFO:    [DEVAPC] MAS_DOM_1 = 0x200
INFO:    [DEVAPC] MAS_DOM_2 = 0x0
INFO:    [DEVAPC] MAS_DOM_3 = 0x2000
INFO:    [DEVAPC] MAS_SEC_0 = 0x8000000
INFO:    [DEVAPC]  (INFRA)MAS_DOMAIN_REMAP_0 = 0x88, (INFRA)MAS_DOMAIN_REMAP_1 = 0x0
INFO:    [DEVAPC]  (MM)MAS_DOMAIN_REMAP_0 = 0x24
WARNING: region 0:
WARNING: 	apc:0x168, sa:0x0, ea:0xfff
WARNING: region 1:
WARNING: 	apc:0x140, sa:0x1000, ea:0x128f
WARNING: region 2:
WARNING: 	apc:0x168, sa:0x1290, ea:0x1fff
WARNING: region 3:
WARNING: 	apc:0x168, sa:0x2000, ea:0xbfff
WARNING: region 4:
WARNING: 	apc:0x168, sa:0xc000, ea:0x1ffff
WARNING: region 5:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 6:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 7:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
INFO:    GICv3 without legacy support detected. ARM GICv3 driver initialized in EL3
INFO:    SPM: enable SPMC mode
NOTICE:  spm_boot_init() start
NOTICE:  spm_boot_init() end
INFO:    BL31: Initializing runtime services
INFO:    BL31: Preparing for EL3 exit to normal world
INFO:    Entry point address = 0x80000000
INFO:    SPSR = 0x8


Starting depthcharge on Juniper...
vboot_handoff: creating legacy vboot_handoff structure
vboot_handoff: copying FW preamble
ec_init(0): CrosEC protocol v3 supported (544, 544)
Wipe memory regions:
	[0x00000040000000, 0x00000054600000)
	[0x00000054660000, 0x00000080000000)
	[0x000000811809c0, 0x000000ffed9000)
	[0x00000100000000, 0x00000140000000)
Initializing XHCI USB controller at 0x11200000.
Calling VbSelectAndLoadKernel().
Connected to device vid:did:rid of 1ae0:0028:00
tpm_get_response: command 0x14e, return code 0x0
ReadSpaceKernel: TPM: read secdata_kernel: 02 4c 57 52 47 01 00 01 00 00 00 00 55
RollbackKernelRead: TPM: RollbackKernelRead 0x10001
tpm_get_response: command 0x14e, return code 0x28b
RollbackFwmpRead: TPM: no FWMP space
VbSelectAndLoadKernel: GBB flags are 0x0
print_hash: RW(active) hash: fb5c0dfa6c2692bec07dda7f769b1ccaa90b944b36137e9ce9d22c3b38a385f7
Trying to locate 'ecrw.hash' in CBFS
sync_one_ec: devidx=0 select_rw=4
sync_one_ec: jumping to EC-RW
EC returned from reboot after 23132us
Waiting for EC to clear limit power flag.
vb2_developer_ui: Entering
vboot_draw_screen: screen=0x101 locale=1
CBGFX: cbgfx initialized: screen:width=1366, height=768, offset=0 canvas:width=768, height=768, offset=299
vboot_init_locale: Supported locales: en, es-419, pt-BR, fr, es, pt-PT, ca, it, de, el, nl, da, nb, sv, fi, et, lv, lt, ru, pl, cs, sk, hu, sl, sr, hr, bg, ro, uk, tr, he, ar, fa, hi, th, ms, vi, id, fil, zh-CN, zh-TW, ko, ja, bn, gu, kn, ml, mr, ta, te, (50 locales)
load_archive: loading vbgfx.bin
load_archive: loading font.bin
load_archive: loading locale_es-419.bin
vb2_developer_ui: VbBootDeveloper() - user pressed Ctrl+D; skip delay
vb2_developer_ui: VbBootDeveloper() - trying fixed disk
Man 000045 Snr 2556076829 Product DA4032 Revision 0.1
VbTryLoadKernel: trying disk 0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s0 t6 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 4
LoadKernel: Found kernel entry at 65605 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
vb2_load_partition: read 13036 KB in 294 ms at 44208 KB/s.
vb2_load_partition: Partition is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s0 t5 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 2
LoadKernel: Found kernel entry at 69 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 4
GptNextKernelEntry: GptNextKernelEntry s0 t5 p2
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s0 t5 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry no more kernels
WriteAndFreeGptData: Updating GPT header 1
WriteAndFreeGptData: Updating GPT entries 1
WriteAndFreeGptData: Updating GPT header 2
WriteAndFreeGptData: Updating GPT entries 2
LoadKernel: Good partition 4
VbTryLoadKernel: LoadKernel() = 0x0
vboot_draw_screen: screen=0x0 locale=1
tpm_get_response: command 0x121, return code 0x0
RollbackKernelLock: TPM: lock secdata_kernel returned 0x0
VbSelectAndLoadKernel: Returning 0
Boot policy: Match for type 0 with cmdline 1
Modified kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
Loading FIT.
Image fdt-36 has 16926 bytes.
Image fdt-35 has 16925 bytes.
Image fdt-34 has 16908 bytes.
Image fdt-33 has 16949 bytes.
Image fdt-32 has 16948 bytes.
Image fdt-31 has 16906 bytes.
Image fdt-30 has 17326 bytes.
Image fdt-29 has 17015 bytes.
Image fdt-28 has 17370 bytes.
Image fdt-27 has 17045 bytes.
Image fdt-26 has 17379 bytes.
Image fdt-25 has 17262 bytes.
Image fdt-24 has 17520 bytes.
Image fdt-23 has 17472 bytes.
Image fdt-22 has 17222 bytes.
Image fdt-21 has 17239 bytes.
Image fdt-20 has 17182 bytes.
Image fdt-19 has 17230 bytes.
Image fdt-18 has 17489 bytes.
Image fdt-17 has 17485 bytes.
Image fdt-16 has 17224 bytes.
Image fdt-15 has 17269 bytes.
Image fdt-14 has 17105 bytes.
Image fdt-13 has 17202 bytes.
Image fdt-12 has 17476 bytes.
Image fdt-11 has 17217 bytes.
Image fdt-10 has 17236 bytes.
Image fdt-9 has 17492 bytes.
Image fdt-8 has 17550 bytes.
Image fdt-7 has 17462 bytes.
Image fdt-6 has 17196 bytes.
Image fdt-5 has 17430 bytes.
Image fdt-4 has 17178 bytes.
Image fdt-3 has 17199 bytes.
Image fdt-2 has 17151 bytes.
Image fdt-1 has 17405 bytes.
Image kernel-1 has 12637811 bytes.
Compat preference: google,juniper-rev9-sku17 google,juniper-sku17 google,juniper-rev9 google,juniper
Config conf-36, kernel kernel-1, fdt fdt-36, compat google,krane-sku176 google,krane mediatek,mt8183
Config conf-35, kernel kernel-1, fdt fdt-35, compat google,krane-sku0 google,krane mediatek,mt8183
Config conf-34, kernel kernel-1, fdt fdt-34, compat google,kodama-sku32 google,kodama mediatek,mt8183
Config conf-33, kernel kernel-1, fdt fdt-33, compat google,kodama-sku288 google,kodama mediatek,mt8183
Config conf-32, kernel kernel-1, fdt fdt-32, compat google,kodama-sku272 google,kodama mediatek,mt8183
Config conf-31, kernel kernel-1, fdt fdt-31, compat google,kodama-sku16 google,kodama mediatek,mt8183
Config conf-30, kernel kernel-1, fdt fdt-30, compat google,katsu mediatek,mt8183
Config conf-29, kernel kernel-1, fdt fdt-29, compat google,katsu-sku38 google,katsu mediatek,mt8183
Config conf-28, kernel kernel-1, fdt fdt-28, compat google,kakadu-rev3 google,kakadu-rev2 google,kakadu mediatek,mt8183
Config conf-27, kernel kernel-1, fdt fdt-27, compat google,kakadu-rev3-sku22 google,kakadu-rev2-sku22 google,kakadu mediatek,mt8183
Config conf-26, kernel kernel-1, fdt fdt-26, compat google,kakadu-rev1 google,kakadu-rev0 google,kakadu mediatek,mt8183
Config conf-25, kernel kernel-1, fdt fdt-25, compat google,willow-sku1 google,willow mediatek,mt8183
Config conf-24, kernel kernel-1, fdt fdt-24, compat google,willow-sku0 google,willow mediatek,mt8183
Config conf-23, kernel kernel-1, fdt fdt-23, compat google,cerise-sku1 google,cerise mediatek,mt8183
Config conf-22, kernel kernel-1, fdt fdt-22, compat google,cerise-rev3-sku1 google,cerise mediatek,mt8183
Config conf-21, kernel kernel-1, fdt fdt-21, compat google,pico-sku2 google,pico mediatek,mt8183
Config conf-20, kernel kernel-1, fdt fdt-20, compat google,pico-sku1 google,pico mediatek,mt8183
Config conf-19, kernel kernel-1, fdt fdt-19, compat google,makomo-rev4-sku1 google,makomo-rev5-sku1 google,makomo mediatek,mt8183
Config conf-18, kernel kernel-1, fdt fdt-18, compat google,makomo-rev4-sku0 google,makomo-rev5-sku0 google,makomo mediatek,mt8183
Config conf-17, kernel kernel-1, fdt fdt-17, compat google,makomo-rev3-sku0 google,makomo mediatek,mt8183
Config conf-16, kernel kernel-1, fdt fdt-16, compat google,makomo-rev0-sku0 google,makomo mediatek,mt8183
Config conf-15, kernel kernel-1, fdt fdt-15, compat google,juniper-sku17 (match) google,juniper mediatek,mt8183
Config conf-14, kernel kernel-1, fdt fdt-14, compat google,kappa mediatek,mt8183
Config conf-13, kernel kernel-1, fdt fdt-13, compat google,juniper-sku16 google,juniper (match) mediatek,mt8183
Config conf-12, kernel kernel-1, fdt fdt-12, compat google,fennel-sku0 google,fennel mediatek,mt8183
Config conf-11, kernel kernel-1, fdt fdt-11, compat google,fennel-sku2 google,fennel mediatek,mt8183
Config conf-10, kernel kernel-1, fdt fdt-10, compat google,fennel-sku7 google,fennel mediatek,mt8183
Config conf-9, kernel kernel-1, fdt fdt-9, compat google,fennel-sku6 google,fennel mediatek,mt8183
Config conf-8, kernel kernel-1, fdt fdt-8, compat google,fennel-sku1 google,fennel mediatek,mt8183
Config conf-7, kernel kernel-1, fdt fdt-7, compat google,damu mediatek,mt8183
Config conf-6, kernel kernel-1, fdt fdt-6, compat google,cozmo mediatek,mt8183
Config conf-5, kernel kernel-1, fdt fdt-5, compat google,cerise-sku0 google,cerise mediatek,mt8183
Config conf-4, kernel kernel-1, fdt fdt-4, compat google,cerise-rev3-sku0 google,cerise mediatek,mt8183
Config conf-3, kernel kernel-1, fdt fdt-3, compat google,burnet mediatek,mt8183
Config conf-2, kernel kernel-1, fdt fdt-2, compat google,bellis-rev0-sku1 google,bellis mediatek,mt8183
Config conf-1, kernel kernel-1, fdt fdt-1, compat google,bellis-rev0-sku0 google,bellis mediatek,mt8183
Choosing best match conf-15 for compat google,juniper-sku17.
LZ4 decompressing fdt-15 to 0x5f800000
tpm_get_response: command 0x17b, return code 0x0
tpm_cleanup: add release locality here.
Shutting down all USB controllers.
Exiting depthcharge with code 4 at timestamp: 6724249
LZ4 decompressing kernel-1 to 0x8017b418
LZ4 decompressing kernel-1 to 0x40000000
jumping to kernel
WARNING: Unimplemented Arm Architecture Service Call: 0x80000002 
INFO:    cpu0: "DYNAMIC_SPM_FW_VERSION", wakesrc = 0xe87dde7, pcm_con1 = 0x5849
INFO:    settle = 99, sec = 131041, sw_flag = 0x8809a 0x40, src_req = 0x0
INFO:    suspend: wake up by R12_EINT_EVENT_B, timer_out = 0
INFO:    r15 = 0xb79, r13 = 0x86040000, debug_flag = 0x1910ff 0x0
INFO:    sw_flag = 0x8809a 0x40, r12 = 0x40, r12_ext = 0x0
INFO:    idle_sta = 0x1ff, req_sta =  0x100000, event_reg = 0x90100000
INFO:    isr = 0x10, raw_sta = 0x40, raw_ext_sta = 0x400290aa
INFO:    wake_misc = 0x0
INFO:    PSCI Power Domain Map:
INFO:      Domain Node : Level 2, parent_node -1, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      CPU Node : MPID 0x0, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x1, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x2, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x3, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x100, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x101, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x102, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x103, parent_node 2, State ON (0x0)


coreboot-v1.9308_26_0.0.22-10544-g50eadf7c92 Mon Feb  8 05:04:19 UTC 2021 verstage starting (log level: 8)...
ARM64: Exception handlers installed.
WDT: Last reset was cold boot
SPI0(PAD0) initialized at 992727 Hz
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
Probing TPM: . done!
TPM ready after 0 ms
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
tlcl_send_startup: Startup return code is 0
TPM: setup succeeded
src/security/tpm/tss/tcg-2.0/tss.c:223 index 0x1007 return code 0
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
Phase 1
FMAP: area GBB found @ 3f5000 (12032 bytes)
VB2:vb2_check_recovery() Recovery reason from previous boot: 0x0 / 0x0
Phase 2
Phase 3
FMAP: area GBB found @ 3f5000 (12032 bytes)
read SPI 0x3f5180 0x1000: 1296 us, 3160 KB/s, 25.280 Mbps
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_keyblock() Checking key block signature...
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_fw_preamble() Verifying preamble.
Phase 4
FMAP: area FW_MAIN_B found @ 5a9000 (1367808 bytes)
VB2:vb2api_init_hash() HW crypto for hash_alg 2 not supported, using SW
Saving nvdata
tlcl_extend: response is 0
tlcl_extend: response is 0
tlcl_lock_nv_write: response is 0
Slot B is selected


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 romstage starting (log level: 8)...
ARM64: Exception handlers installed.
[RTC]rtc_enable_dcxo,41: con=0x482, osc32con=0x826f, sec=0x2008
[RTC]rtc_check_state,142: con=482, pwrkey1=a357, pwrkey2=67d2
[RTC]rtc_eosc_cali,157: PMIC_RG_FQMTR_CKSEL=0x4a
[RTC]rtc_get_frequency_meter,134: input=0xf, output=792
[RTC]rtc_osc_init,208: EOSC32 cali val = 0x826f
[RTC]rtc_boot_common,186: irqsta=0, bbpu=0, con=482
[RTC]rtc_bbpu_power_on,373: rtc_write_trigger=1
[RTC]rtc_bbpu_power_on,376: done BBPU=0x9
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_DDR_TRAINING found @ 556000 (8192 bytes)
read_calibration_data_from_flash: ret=0x8f0, length=0x8f0
DRAM-K: Fast Calibration
Calibration params loaded from flash
Run calibration (freq: 1600, first: 1)
Vendor id is 0x6
Run calibration (freq: 2400, first: 0)
Vendor id is 0x6
Run calibration (freq: 3200, first: 0)
Vendor id is 0x6
[MEM] complex R/W mem test pass : 0
[MEM] complex R/W mem test pass : 0
Mapping address range [0000000040000000:0000000140000000) as     cacheable | read-write | non-secure | normal
CBMEM:
IMD: root @ 00000000fffff000 254 entries.
IMD: root @ 00000000ffffec00 62 entries.
VBOOT: copying vboot_working_data (3840 bytes) to CBMEM...
out: cmd=0xa4: 03 6c a4 00 00 00 0c 00 00 01 00 00 50 7f 11 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Chrome EC: clear events_b mask to 0x0000000020004000
out: cmd=0xa4: 03 ea a4 00 00 00 0c 00 02 01 00 00 00 40 00 20 00 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/ramstage'
CBFS: Found @ offset 10b40 size d3a0
read SPI 0x5b9b94 0xd384: 16505 us, 3280 KB/s, 26.240 Mbps
Accumulated console time in romstage 0 ms


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 ramstage starting (log level: 8)...
ARM64: Exception handlers installed.
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_VPD found @ 550000 (16384 bytes)
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
read SPI 0x3f8600 0x7a00: 9522 us, 3279 KB/s, 26.232 Mbps
FMAP: area RW_VPD found @ 550000 (16384 bytes)
read SPI 0x550600 0x3a00: 4533 us, 3275 KB/s, 26.200 Mbps
BS: BS_PRE_DEVICE times (ms): entry 0 run 0 exit 0
BS: BS_DEV_INIT_CHIPS times (ms): entry 0 run 0 exit 0
Enumerating buses...
Show all devs... Before device enumeration.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
Compare with tree...
Root Device: enabled 1
 CPU_CLUSTER: 0: enabled 1
  CPU: 00: enabled 1
Root Device scanning...
root_dev_scan_bus for Root Device
CPU_CLUSTER: 0 enabled
root_dev_scan_bus for Root Device done
scan_bus: scanning of bus Root Device took 6 usecs
done
BS: BS_DEV_ENUMERATE times (ms): entry 0 run 0 exit 0
Allocating resources...
Reading resources...
Root Device read_resources bus 0 link: 0
CPU_CLUSTER: 0 read_resources bus 0 link: 0
CPU: 00 missing read_resources
CPU_CLUSTER: 0 read_resources bus 0 link: 0 done
Root Device read_resources bus 0 link: 0 done
Done reading resources.
Show resources in subtree (Root Device)...After reading.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Setting resources...
Root Device assign_resources, bus 0 link: 0
CPU_CLUSTER: 0 missing set_resources
Root Device assign_resources, bus 0 link: 0
Done setting resources.
Show resources in subtree (Root Device)...After assigning values.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Done allocating resources.
BS: BS_DEV_RESOURCES times (ms): entry 0 run 0 exit 0
Enabling resources...
done.
BS: BS_DEV_ENABLE times (ms): entry 0 run 0 exit 0
Initializing devices...
Root Device init ...
mainboard_init: Starting display init.
ADC[4]: Raw value=214746 ID=1
anx7625_power_on_init: Init interface.
anx7625_disable_pd_protocol: Disabled PD feature.
anx7625_power_on_init: Firmware: ver 0x0, rev 0x0.
anx7625_start_dp_work: Secure OCM version=00
anx7625_hpd_change_detect: HPD received 0x7e:0x45=0x91
sp_tx_get_edid_block: EDID Block = 1
Extracted contents:
header:          00 ff ff ff ff ff ff 00
serial number:   2c 82 30 11 00 00 00 00 31 1e
version:         01 04
basic params:    95 1a 0e 78 02
chroma info:     e1 c1 94 5b 59 94 29 22 50 54
established:     00 00 00
standard:        01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1:    3e 1c 56 a0 50 00 16 30 28 20 55 00 00 90 10 00 00 18
descriptor 2:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 3:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 4:    00 00 00 fe 00 4b 44 31 31 36 4e 32 39 33 30 41 30 32
extensions:      00
checksum:        f0

Manufacturer: KDB Model 1130 Serial Number 0
Made week 49 of 2020
EDID version: 1.4
Digital display
6 bits per primary color channel
DisplayPort interface
Maximum image size: 26 cm x 14 cm
Gamma: 220%
Check DPMS levels
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Established timings supported:
Standard timings supported:
Detailed timings
Hex of detail: 3e1c56a05000163028205500009010000018
Detailed mode (IN HEX): Clock 72300 KHz, 100 mm x 90 mm
               0556 057e 059e 05f6 hborder 0
               0300 0305 030a 0316 vborder 0
               -hsync -vsync 
Did detailed timing
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000fe004b443131364e32393330413032
ASCII string: KD116N2930A02
Checksum
Checksum: 0xf0 (valid)
get_active_panel: Found ID 1: 'KDB KD116N2930A02' 1366x768@0Hz
DSI data_rate: 433800000 bps
anx7625_parse_edid: set default k value to 0x3d for panel
anx7625_parse_edid: pixelclock(72300).
 hactive(1366), hsync(32), hfp(40), hbp(88)
 vactive(768), vsync(5), vfp(5), vbp(12)
anx7625_dsi_config: config dsi.
anx7625_dsi_video_config: compute M(15794176), N(737280), divider(8).
anx7625_dsi_config: success to config DSI
anx7625_dp_start: MIPI phy setup OK.
[SSUSB] Setting up USB HOST controller...
[SSUSB] u3phy_ports_enable u2p:1, u3p:0
[SSUSB] phy power-on done.
out: cmd=0xf: 03 d9 0f 00 00 00 04 00 11 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
SPM: pcm index = 1
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'pcm_allinone_lp4_3200.bin'
CBFS: Found @ offset 1e400 size 1026
read SPI 0x5c7448 0x1026: 1271 us, 3252 KB/s, 26.016 Mbps
SPM: binary array size = 2988
SPM: version = pcm_allinone_v1.17.2_20180829
SPM binary loaded in 2 msecs
spm_kick_im_to_fetch: ptr = 000000004021ee82
spm_kick_im_to_fetch: len = 2988
SPM: spm_kick_pcm_to_run
SPM: spm_kick_pcm_to_run done
SPM: spm_init done in 5 msecs
Root Device init finished in 246167 usecs
CPU_CLUSTER: 0 init ...
Mapping address range [0000000000200000:0000000000280000) as     cacheable | read-write |     secure | device
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'sspm.bin'
CBFS: Found @ offset 20500 size 41cb
read SPI 0x5c9538 0x41cb: 5142 us, 3275 KB/s, 26.200 Mbps
CPU_CLUSTER: 0 init finished in 8336 usecs
Devices initialized
Show all devs... After init.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
BS: BS_DEV_INIT times (ms): entry 0 run 254 exit 0
FMAP: area RW_ELOG found @ 558000 (4096 bytes)
ELOG: NV offset 0x558000 size 0x1000
read SPI 0x558000 0x1000: 1259 us, 3253 KB/s, 26.024 Mbps
ELOG: area is 4096 bytes, full threshold 3842, shrink size 1024
ELOG: Event(17) added with size 13 at 2025-02-28 19:10:31 UTC
out: cmd=0x121: 03 db 21 01 00 00 00 00 
in-header: 03 ea 00 00 2c 00 00 00 
in-data: 5c 04 00 00 00 00 00 00 02 08 00 00 08 00 00 00 5c 37 00 00 08 00 00 00 5b 4a e1 0e 08 00 00 00 e6 ec 05 00 08 00 00 00 2a 25 10 00 
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 54 a4 00 00 00 0c 00 00 01 00 00 f8 ff 01 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
ELOG: Event(A0) added with size 9 at 2025-02-28 19:10:31 UTC
elog_add_boot_reason: Logged dev mode boot
Finalize devices...
Devices finalized
BS: BS_POST_DEVICE times (ms): entry 3 run 0 exit 0
BS: BS_OS_RESUME_CHECK times (ms): entry 0 run 0 exit 0
Writing coreboot table at 0xffed9000
 0. 0000000000114000-000000000011efff: RAMSTAGE
 1. 0000000040000000-000000004023cfff: RAMSTAGE
 2. 000000004023d000-00000000545fffff: RAM
 3. 0000000054600000-000000005465ffff: BL31
 4. 0000000054660000-00000000ffed8fff: RAM
 5. 00000000ffed9000-00000000ffffffff: CONFIGURATION TABLES
 6. 0000000100000000-000000013fffffff: RAM
Passing 5 GPIOs to payload:
            NAME |       PORT | POLARITY |     VALUE
   write protect | 0x00000096 |      low |       low
        EC in RW | 0x000000b1 |     high | undefined
    EC interrupt | 0x00000097 |      low | undefined
   TPM interrupt | 0x00000099 |     high | undefined
  speaker enable | 0x000000af |     high | undefined
out: cmd=0x6: 03 f7 06 00 00 00 00 00 
in-header: 03 f2 00 00 02 00 00 00 
in-data: 09 00 
Board ID: 9
ADC[3]: Raw value=1252987 ID=10
RAM code: 10
SKU ID: 17
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
Wrote coreboot table at: 00000000ffed9000, 0x368 bytes, checksum a8c5
coreboot table: 896 bytes.
IMD ROOT    0. 00000000fffff000 00001000
IMD SMALL   1. 00000000ffffe000 00001000
CONSOLE     2. 00000000fffde000 00020000
FMAP        3. 00000000fffdd000 0000047c
TIME STAMP  4. 00000000fffdc000 00000910
VBOOT WORK  5. 00000000fffdb000 00000f00
RAMOOPS     6. 00000000ffedb000 00100000
COREBOOT    7. 00000000ffed9000 00002000
IMD small region:
  IMD ROOT    0. 00000000ffffec00 00000400
  EC HOSTEVENT 1. 00000000ffffebe0 00000008
  VPD         2. 00000000ffffe9a0 0000022d
BS: BS_WRITE_TABLES times (ms): entry 0 run 0 exit 0
out: cmd=0xa4: 03 e0 a4 00 00 00 0c 00 00 01 00 00 dc 2f 21 40 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Probing TPM:  done!
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
Checking cr50 for pending updates
Reading cr50 TPM mode
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/payload'
CBFS: Found @ offset 50180 size 16deb
read SPI 0x5f91b8 0x16deb: 28553 us, 3280 KB/s, 26.240 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000080000000 memsize 0x11809c0 srcaddr 0x000000004000b438 filesize 0x16db3
Loading Segment: addr: 0x0000000080000000 memsz: 0x00000000011809c0 filesz: 0x0000000000016db3
using LZMA
[ 0x80000000, 80033268, 0x811809c0) <- 4000b438
Clearing Segment: addr: 0x0000000080033268 memsz: 0x000000000114d758
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000080000000
Loaded segments
BS: BS_PAYLOAD_LOAD times (ms): entry 9 run 45 exit 0
Jumping to boot code at 0000000080000000(00000000ffed9000)
CPU0: stack: 0000000000114000 - 0000000000118000, lowest used address 00000000001176a0, stack used: 2400 bytes
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/bl31'
CBFS: Found @ offset 36a00 size 4b17
read SPI 0x5dfa28 0x4b17: 5866 us, 3277 KB/s, 26.216 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000054600000 memsize 0x27000 srcaddr 0x000000004000b438 filesize 0x4adf
Loading Segment: addr: 0x0000000054600000 memsz: 0x0000000000027000 filesz: 0x0000000000004adf
using LZMA
[ 0x54600000, 5460d408, 0x54627000) <- 4000b438
Clearing Segment: addr: 0x000000005460d408 memsz: 0x0000000000019bf8
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000054601000
Loaded segments
NOTICE:  MT8183 bl31_setup
NOTICE:  BL31: v2.1(release):v2.1-809-g62969c490
NOTICE:  BL31: Built : Mon May 30 03:26:46 UTC 2022
INFO:    [DEVAPC] dump DEVAPC registers:
INFO:    [DEVAPC] (INFRA)D0_APC_0 = 0x0, (INFRA)D1_APC_0 = 0xfcfffffc, (INFRA)D2_APC_0 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_1 = 0x0, (INFRA)D1_APC_1 = 0xffffffff, (INFRA)D2_APC_1 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_2 = 0x0, (INFRA)D1_APC_2 = 0xffffffff, (INFRA)D2_APC_2 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_3 = 0x0, (INFRA)D1_APC_3 = 0xffffffff, (INFRA)D2_APC_3 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_4 = 0x80000000, (INFRA)D1_APC_4 = 0xffffffff, (INFRA)D2_APC_4 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_5 = 0x2aaa, (INFRA)D1_APC_5 = 0xfcff3fff, (INFRA)D2_APC_5 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_6 = 0x0, (INFRA)D1_APC_6 = 0xffffffff, (INFRA)D2_APC_6 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_7 = 0x0, (INFRA)D1_APC_7 = 0xffffffff, (INFRA)D2_APC_7 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_8 = 0x0, (INFRA)D1_APC_8 = 0xffffffff, (INFRA)D2_APC_8 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_9 = 0x0, (INFRA)D1_APC_9 = 0xffffffff, (INFRA)D2_APC_9 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_10 = 0x0, (INFRA)D1_APC_10 = 0xffffffff, (INFRA)D2_APC_10 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_11 = 0x0, (INFRA)D1_APC_11 = 0xffffffff, (INFRA)D2_APC_11 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_12 = 0x0, (INFRA)D1_APC_12 = 0xff, (INFRA)D2_APC_12 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_0 = 0x0, (MM)D1_APC_0 = 0xffc000ff, (MM)D2_APC_0 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_1 = 0x0, (MM)D1_APC_1 = 0x3fffffff, (MM)D2_APC_1 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_2 = 0x0, (MM)D1_APC_2 = 0xcffff33c, (MM)D2_APC_2 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_3 = 0x0, (MM)D1_APC_3 = 0x3ccfc0ff, (MM)D2_APC_3 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_4 = 0x0, (MM)D1_APC_4 = 0xffff0000, (MM)D2_APC_4 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_5 = 0x0, (MM)D1_APC_5 = 0xffffffff, (MM)D2_APC_5 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_6 = 0x0, (MM)D1_APC_6 = 0xffffffff, (MM)D2_APC_6 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_7 = 0x0, (MM)D1_APC_7 = 0xffffffff, (MM)D2_APC_7 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_8 = 0x0, (MM)D1_APC_8 = 0x3ffffff, (MM)D2_APC_8 = 0x0
INFO:    [DEVAPC] MAS_DOM_0 = 0x1
INFO:    [DEVAPC] MAS_DOM_1 = 0x200
INFO:    [DEVAPC] MAS_DOM_2 = 0x0
INFO:    [DEVAPC] MAS_DOM_3 = 0x2000
INFO:    [DEVAPC] MAS_SEC_0 = 0x8000000
INFO:    [DEVAPC]  (INFRA)MAS_DOMAIN_REMAP_0 = 0x88, (INFRA)MAS_DOMAIN_REMAP_1 = 0x0
INFO:    [DEVAPC]  (MM)MAS_DOMAIN_REMAP_0 = 0x24
WARNING: region 0:
WARNING: 	apc:0x168, sa:0x0, ea:0xfff
WARNING: region 1:
WARNING: 	apc:0x140, sa:0x1000, ea:0x128f
WARNING: region 2:
WARNING: 	apc:0x168, sa:0x1290, ea:0x1fff
WARNING: region 3:
WARNING: 	apc:0x168, sa:0x2000, ea:0xbfff
WARNING: region 4:
WARNING: 	apc:0x168, sa:0xc000, ea:0x1ffff
WARNING: region 5:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 6:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 7:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
INFO:    GICv3 without legacy support detected. ARM GICv3 driver initialized in EL3
INFO:    SPM: enable SPMC mode
NOTICE:  spm_boot_init() start
NOTICE:  spm_boot_init() end
INFO:    BL31: Initializing runtime services
INFO:    BL31: Preparing for EL3 exit to normal world
INFO:    Entry point address = 0x80000000
INFO:    SPSR = 0x8


Starting depthcharge on Juniper...
vboot_handoff: creating legacy vboot_handoff structure
vboot_handoff: copying FW preamble
ec_init(0): CrosEC protocol v3 supported (544, 544)
Wipe memory regions:
	[0x00000040000000, 0x00000054600000)
	[0x00000054660000, 0x00000080000000)
	[0x000000811809c0, 0x000000ffed9000)
	[0x00000100000000, 0x00000140000000)
Initializing XHCI USB controller at 0x11200000.
Calling VbSelectAndLoadKernel().
Connected to device vid:did:rid of 1ae0:0028:00
tpm_get_response: command 0x14e, return code 0x0
ReadSpaceKernel: TPM: read secdata_kernel: 02 4c 57 52 47 01 00 01 00 00 00 00 55
RollbackKernelRead: TPM: RollbackKernelRead 0x10001
tpm_get_response: command 0x14e, return code 0x28b
RollbackFwmpRead: TPM: no FWMP space
VbSelectAndLoadKernel: GBB flags are 0x0
print_hash: RW(active) hash: fb5c0dfa6c2692bec07dda7f769b1ccaa90b944b36137e9ce9d22c3b38a385f7
Trying to locate 'ecrw.hash' in CBFS
sync_one_ec: devidx=0 select_rw=4
sync_one_ec: jumping to EC-RW
EC returned from reboot after 23137us
Waiting for EC to clear limit power flag.
vb2_developer_ui: Entering
vboot_draw_screen: screen=0x101 locale=1
CBGFX: cbgfx initialized: screen:width=1366, height=768, offset=0 canvas:width=768, height=768, offset=299
vboot_init_locale: Supported locales: en, es-419, pt-BR, fr, es, pt-PT, ca, it, de, el, nl, da, nb, sv, fi, et, lv, lt, ru, pl, cs, sk, hu, sl, sr, hr, bg, ro, uk, tr, he, ar, fa, hi, th, ms, vi, id, fil, zh-CN, zh-TW, ko, ja, bn, gu, kn, ml, mr, ta, te, (50 locales)
load_archive: loading vbgfx.bin
load_archive: loading font.bin
load_archive: loading locale_es-419.bin
vb2_developer_ui: VbBootDeveloper() - user pressed Ctrl+D; skip delay
vb2_developer_ui: VbBootDeveloper() - trying fixed disk
Man 000045 Snr 2556076829 Product DA4032 Revision 0.1
VbTryLoadKernel: trying disk 0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 4
LoadKernel: Found kernel entry at 65605 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
vb2_load_partition: read 13036 KB in 294 ms at 44208 KB/s.
vb2_load_partition: Partition is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 2
LoadKernel: Found kernel entry at 69 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry no more kernels
LoadKernel: Good partition 4
VbTryLoadKernel: LoadKernel() = 0x0
vboot_draw_screen: screen=0x0 locale=1
tpm_get_response: command 0x121, return code 0x0
RollbackKernelLock: TPM: lock secdata_kernel returned 0x0
VbSelectAndLoadKernel: Returning 0
Boot policy: Match for type 0 with cmdline 1
Modified kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
Loading FIT.
Image fdt-36 has 16926 bytes.
Image fdt-35 has 16925 bytes.
Image fdt-34 has 16908 bytes.
Image fdt-33 has 16949 bytes.
Image fdt-32 has 16948 bytes.
Image fdt-31 has 16906 bytes.
Image fdt-30 has 17326 bytes.
Image fdt-29 has 17015 bytes.
Image fdt-28 has 17370 bytes.
Image fdt-27 has 17045 bytes.
Image fdt-26 has 17379 bytes.
Image fdt-25 has 17262 bytes.
Image fdt-24 has 17520 bytes.
Image fdt-23 has 17472 bytes.
Image fdt-22 has 17222 bytes.
Image fdt-21 has 17239 bytes.
Image fdt-20 has 17182 bytes.
Image fdt-19 has 17230 bytes.
Image fdt-18 has 17489 bytes.
Image fdt-17 has 17485 bytes.
Image fdt-16 has 17224 bytes.
Image fdt-15 has 17269 bytes.
Image fdt-14 has 17105 bytes.
Image fdt-13 has 17202 bytes.
Image fdt-12 has 17476 bytes.
Image fdt-11 has 17217 bytes.
Image fdt-10 has 17236 bytes.
Image fdt-9 has 17492 bytes.
Image fdt-8 has 17550 bytes.
Image fdt-7 has 17462 bytes.
Image fdt-6 has 17196 bytes.
Image fdt-5 has 17430 bytes.
Image fdt-4 has 17178 bytes.
Image fdt-3 has 17199 bytes.
Image fdt-2 has 17151 bytes.
Image fdt-1 has 17405 bytes.
Image kernel-1 has 12637811 bytes.
Compat preference: google,juniper-rev9-sku17 google,juniper-sku17 google,juniper-rev9 google,juniper
Config conf-36, kernel kernel-1, fdt fdt-36, compat google,krane-sku176 google,krane mediatek,mt8183
Config conf-35, kernel kernel-1, fdt fdt-35, compat google,krane-sku0 google,krane mediatek,mt8183
Config conf-34, kernel kernel-1, fdt fdt-34, compat google,kodama-sku32 google,kodama mediatek,mt8183
Config conf-33, kernel kernel-1, fdt fdt-33, compat google,kodama-sku288 google,kodama mediatek,mt8183
Config conf-32, kernel kernel-1, fdt fdt-32, compat google,kodama-sku272 google,kodama mediatek,mt8183
Config conf-31, kernel kernel-1, fdt fdt-31, compat google,kodama-sku16 google,kodama mediatek,mt8183
Config conf-30, kernel kernel-1, fdt fdt-30, compat google,katsu mediatek,mt8183
Config conf-29, kernel kernel-1, fdt fdt-29, compat google,katsu-sku38 google,katsu mediatek,mt8183
Config conf-28, kernel kernel-1, fdt fdt-28, compat google,kakadu-rev3 google,kakadu-rev2 google,kakadu mediatek,mt8183
Config conf-27, kernel kernel-1, fdt fdt-27, compat google,kakadu-rev3-sku22 google,kakadu-rev2-sku22 google,kakadu mediatek,mt8183
Config conf-26, kernel kernel-1, fdt fdt-26, compat google,kakadu-rev1 google,kakadu-rev0 google,kakadu mediatek,mt8183
Config conf-25, kernel kernel-1, fdt fdt-25, compat google,willow-sku1 google,willow mediatek,mt8183
Config conf-24, kernel kernel-1, fdt fdt-24, compat google,willow-sku0 google,willow mediatek,mt8183
Config conf-23, kernel kernel-1, fdt fdt-23, compat google,cerise-sku1 google,cerise mediatek,mt8183
Config conf-22, kernel kernel-1, fdt fdt-22, compat google,cerise-rev3-sku1 google,cerise mediatek,mt8183
Config conf-21, kernel kernel-1, fdt fdt-21, compat google,pico-sku2 google,pico mediatek,mt8183
Config conf-20, kernel kernel-1, fdt fdt-20, compat google,pico-sku1 google,pico mediatek,mt8183
Config conf-19, kernel kernel-1, fdt fdt-19, compat google,makomo-rev4-sku1 google,makomo-rev5-sku1 google,makomo mediatek,mt8183
Config conf-18, kernel kernel-1, fdt fdt-18, compat google,makomo-rev4-sku0 google,makomo-rev5-sku0 google,makomo mediatek,mt8183
Config conf-17, kernel kernel-1, fdt fdt-17, compat google,makomo-rev3-sku0 google,makomo mediatek,mt8183
Config conf-16, kernel kernel-1, fdt fdt-16, compat google,makomo-rev0-sku0 google,makomo mediatek,mt8183
Config conf-15, kernel kernel-1, fdt fdt-15, compat google,juniper-sku17 (match) google,juniper mediatek,mt8183
Config conf-14, kernel kernel-1, fdt fdt-14, compat google,kappa mediatek,mt8183
Config conf-13, kernel kernel-1, fdt fdt-13, compat google,juniper-sku16 google,juniper (match) mediatek,mt8183
Config conf-12, kernel kernel-1, fdt fdt-12, compat google,fennel-sku0 google,fennel mediatek,mt8183
Config conf-11, kernel kernel-1, fdt fdt-11, compat google,fennel-sku2 google,fennel mediatek,mt8183
Config conf-10, kernel kernel-1, fdt fdt-10, compat google,fennel-sku7 google,fennel mediatek,mt8183
Config conf-9, kernel kernel-1, fdt fdt-9, compat google,fennel-sku6 google,fennel mediatek,mt8183
Config conf-8, kernel kernel-1, fdt fdt-8, compat google,fennel-sku1 google,fennel mediatek,mt8183
Config conf-7, kernel kernel-1, fdt fdt-7, compat google,damu mediatek,mt8183
Config conf-6, kernel kernel-1, fdt fdt-6, compat google,cozmo mediatek,mt8183
Config conf-5, kernel kernel-1, fdt fdt-5, compat google,cerise-sku0 google,cerise mediatek,mt8183
Config conf-4, kernel kernel-1, fdt fdt-4, compat google,cerise-rev3-sku0 google,cerise mediatek,mt8183
Config conf-3, kernel kernel-1, fdt fdt-3, compat google,burnet mediatek,mt8183
Config conf-2, kernel kernel-1, fdt fdt-2, compat google,bellis-rev0-sku1 google,bellis mediatek,mt8183
Config conf-1, kernel kernel-1, fdt fdt-1, compat google,bellis-rev0-sku0 google,bellis mediatek,mt8183
Choosing best match conf-15 for compat google,juniper-sku17.
LZ4 decompressing fdt-15 to 0x5f800000
tpm_get_response: command 0x17b, return code 0x0
tpm_cleanup: add release locality here.
Shutting down all USB controllers.
Exiting depthcharge with code 4 at timestamp: 4251934
LZ4 decompressing kernel-1 to 0x8017b418
LZ4 decompressing kernel-1 to 0x40000000
jumping to kernel
WARNING: Unimplemented Arm Architecture Service Call: 0x80000002 
INFO:    PSCI Power Domain Map:
INFO:      Domain Node : Level 2, parent_node -1, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 1, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      Domain Node : Level 0, parent_node 0, State ON (0x0)
INFO:      CPU Node : MPID 0x0, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x1, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x2, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x3, parent_node 1, State ON (0x0)
INFO:      CPU Node : MPID 0x100, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x101, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x102, parent_node 2, State ON (0x0)
INFO:      CPU Node : MPID 0x103, parent_node 2, State ON (0x0)


coreboot-v1.9308_26_0.0.22-10544-g50eadf7c92 Mon Feb  8 05:04:19 UTC 2021 verstage starting (log level: 8)...
ARM64: Exception handlers installed.
WDT: Last reset was cold boot
SPI0(PAD0) initialized at 992727 Hz
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
Probing TPM: . done!
TPM ready after 0 ms
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
tlcl_send_startup: Startup return code is 0
TPM: setup succeeded
src/security/tpm/tss/tcg-2.0/tss.c:223 index 0x1007 return code 0
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
Phase 1
FMAP: area GBB found @ 3f5000 (12032 bytes)
VB2:vb2_check_recovery() Recovery reason from previous boot: 0x0 / 0x0
Phase 2
Phase 3
FMAP: area GBB found @ 3f5000 (12032 bytes)
read SPI 0x3f5180 0x1000: 1293 us, 3167 KB/s, 25.336 Mbps
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_keyblock() Checking key block signature...
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
FMAP: area VBLOCK_B found @ 5a7000 (8192 bytes)
VB2:vb2_verify_fw_preamble() Verifying preamble.
Phase 4
FMAP: area FW_MAIN_B found @ 5a9000 (1367808 bytes)
VB2:vb2api_init_hash() HW crypto for hash_alg 2 not supported, using SW
Saving nvdata
tlcl_extend: response is 0
tlcl_extend: response is 0
tlcl_lock_nv_write: response is 0
Slot B is selected


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 romstage starting (log level: 8)...
ARM64: Exception handlers installed.
[RTC]rtc_enable_dcxo,41: con=0x482, osc32con=0x826f, sec=0x2008
[RTC]rtc_check_state,142: con=482, pwrkey1=a357, pwrkey2=67d2
[RTC]rtc_eosc_cali,157: PMIC_RG_FQMTR_CKSEL=0x4a
[RTC]rtc_get_frequency_meter,134: input=0xf, output=792
[RTC]rtc_osc_init,208: EOSC32 cali val = 0x826f
[RTC]rtc_boot_common,186: irqsta=0, bbpu=0, con=482
[RTC]rtc_bbpu_power_on,373: rtc_write_trigger=1
[RTC]rtc_bbpu_power_on,376: done BBPU=0x9
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 5d a4 00 00 00 0c 00 00 01 00 00 f4 fb 00 00 00 00 00 00 
in-header: 03 a5 00 00 08 00 00 00 
in-data: 00 20 20 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_DDR_TRAINING found @ 556000 (8192 bytes)
read_calibration_data_from_flash: ret=0x8f0, length=0x8f0
DRAM-K: Fast Calibration
Calibration params loaded from flash
Run calibration (freq: 1600, first: 1)
Vendor id is 0x6
Run calibration (freq: 2400, first: 0)
Vendor id is 0x6
Run calibration (freq: 3200, first: 0)
Vendor id is 0x6
[MEM] complex R/W mem test pass : 0
[MEM] complex R/W mem test pass : 0
Mapping address range [0000000040000000:0000000140000000) as     cacheable | read-write | non-secure | normal
CBMEM:
IMD: root @ 00000000fffff000 254 entries.
IMD: root @ 00000000ffffec00 62 entries.
VBOOT: copying vboot_working_data (3840 bytes) to CBMEM...
out: cmd=0xa4: 03 6c a4 00 00 00 0c 00 00 01 00 00 50 7f 11 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Chrome EC: clear events_b mask to 0x0000000020004000
out: cmd=0xa4: 03 ea a4 00 00 00 0c 00 02 01 00 00 00 40 00 20 00 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/ramstage'
CBFS: Found @ offset 10b40 size d3a0
read SPI 0x5b9b94 0xd384: 16506 us, 3280 KB/s, 26.240 Mbps
Accumulated console time in romstage 0 ms


coreboot-v1.9308_26_0.0.22-10566-g8417b00957 Mon May 30 03:26:46 UTC 2022 ramstage starting (log level: 8)...
ARM64: Exception handlers installed.
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
Manufacturer: ef
SF: Detected W25Q64JW with sector size 0x1000, total 0x800000
FMAP: area RW_VPD found @ 550000 (16384 bytes)
FMAP: area RO_VPD found @ 3f8000 (32768 bytes)
read SPI 0x3f8600 0x7a00: 9523 us, 3279 KB/s, 26.232 Mbps
FMAP: area RW_VPD found @ 550000 (16384 bytes)
read SPI 0x550600 0x3a00: 4533 us, 3275 KB/s, 26.200 Mbps
BS: BS_PRE_DEVICE times (ms): entry 0 run 0 exit 0
BS: BS_DEV_INIT_CHIPS times (ms): entry 0 run 0 exit 0
Enumerating buses...
Show all devs... Before device enumeration.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
Compare with tree...
Root Device: enabled 1
 CPU_CLUSTER: 0: enabled 1
  CPU: 00: enabled 1
Root Device scanning...
root_dev_scan_bus for Root Device
CPU_CLUSTER: 0 enabled
root_dev_scan_bus for Root Device done
scan_bus: scanning of bus Root Device took 7 usecs
done
BS: BS_DEV_ENUMERATE times (ms): entry 0 run 0 exit 0
Allocating resources...
Reading resources...
Root Device read_resources bus 0 link: 0
CPU_CLUSTER: 0 read_resources bus 0 link: 0
CPU: 00 missing read_resources
CPU_CLUSTER: 0 read_resources bus 0 link: 0 done
Root Device read_resources bus 0 link: 0 done
Done reading resources.
Show resources in subtree (Root Device)...After reading.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Setting resources...
Root Device assign_resources, bus 0 link: 0
CPU_CLUSTER: 0 missing set_resources
Root Device assign_resources, bus 0 link: 0
Done setting resources.
Show resources in subtree (Root Device)...After assigning values.
 Root Device child on link 0 CPU_CLUSTER: 0
  CPU_CLUSTER: 0 child on link 0 CPU: 00
  CPU_CLUSTER: 0 resource base 40000000 size 100000000 align 0 gran 0 limit 0 flags e0004200 index 0
   CPU: 00
Done allocating resources.
BS: BS_DEV_RESOURCES times (ms): entry 0 run 0 exit 0
Enabling resources...
done.
BS: BS_DEV_ENABLE times (ms): entry 0 run 0 exit 0
Initializing devices...
Root Device init ...
mainboard_init: Starting display init.
ADC[4]: Raw value=214746 ID=1
anx7625_power_on_init: Init interface.
anx7625_disable_pd_protocol: Disabled PD feature.
anx7625_power_on_init: Firmware: ver 0x0, rev 0x0.
anx7625_start_dp_work: Secure OCM version=00
anx7625_hpd_change_detect: HPD received 0x7e:0x45=0x91
sp_tx_get_edid_block: EDID Block = 1
Extracted contents:
header:          00 ff ff ff ff ff ff 00
serial number:   2c 82 30 11 00 00 00 00 31 1e
version:         01 04
basic params:    95 1a 0e 78 02
chroma info:     e1 c1 94 5b 59 94 29 22 50 54
established:     00 00 00
standard:        01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1:    3e 1c 56 a0 50 00 16 30 28 20 55 00 00 90 10 00 00 18
descriptor 2:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 3:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
descriptor 4:    00 00 00 fe 00 4b 44 31 31 36 4e 32 39 33 30 41 30 32
extensions:      00
checksum:        f0

Manufacturer: KDB Model 1130 Serial Number 0
Made week 49 of 2020
EDID version: 1.4
Digital display
6 bits per primary color channel
DisplayPort interface
Maximum image size: 26 cm x 14 cm
Gamma: 220%
Check DPMS levels
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Established timings supported:
Standard timings supported:
Detailed timings
Hex of detail: 3e1c56a05000163028205500009010000018
Detailed mode (IN HEX): Clock 72300 KHz, 100 mm x 90 mm
               0556 057e 059e 05f6 hborder 0
               0300 0305 030a 0316 vborder 0
               -hsync -vsync 
Did detailed timing
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000000000000000000000000000000000
Manufacturer-specified data, tag 0
Hex of detail: 000000fe004b443131364e32393330413032
ASCII string: KD116N2930A02
Checksum
Checksum: 0xf0 (valid)
get_active_panel: Found ID 1: 'KDB KD116N2930A02' 1366x768@0Hz
DSI data_rate: 433800000 bps
anx7625_parse_edid: set default k value to 0x3d for panel
anx7625_parse_edid: pixelclock(72300).
 hactive(1366), hsync(32), hfp(40), hbp(88)
 vactive(768), vsync(5), vfp(5), vbp(12)
anx7625_dsi_config: config dsi.
anx7625_dsi_video_config: compute M(15794176), N(737280), divider(8).
anx7625_dsi_config: success to config DSI
anx7625_dp_start: MIPI phy setup OK.
[SSUSB] Setting up USB HOST controller...
[SSUSB] u3phy_ports_enable u2p:1, u3p:0
[SSUSB] phy power-on done.
out: cmd=0xf: 03 d9 0f 00 00 00 04 00 11 00 00 00 
in-header: 03 fd 00 00 00 00 00 00 
in-data: 
SPM: pcm index = 1
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'pcm_allinone_lp4_3200.bin'
CBFS: Found @ offset 1e400 size 1026
read SPI 0x5c7448 0x1026: 1271 us, 3252 KB/s, 26.016 Mbps
SPM: binary array size = 2988
SPM: version = pcm_allinone_v1.17.2_20180829
SPM binary loaded in 2 msecs
spm_kick_im_to_fetch: ptr = 000000004021ee82
spm_kick_im_to_fetch: len = 2988
SPM: spm_kick_pcm_to_run
SPM: spm_kick_pcm_to_run done
SPM: spm_init done in 5 msecs
Root Device init finished in 246164 usecs
CPU_CLUSTER: 0 init ...
Mapping address range [0000000000200000:0000000000280000) as     cacheable | read-write |     secure | device
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'sspm.bin'
CBFS: Found @ offset 20500 size 41cb
read SPI 0x5c9538 0x41cb: 5142 us, 3275 KB/s, 26.200 Mbps
CPU_CLUSTER: 0 init finished in 8334 usecs
Devices initialized
Show all devs... After init.
Root Device: enabled 1
CPU_CLUSTER: 0: enabled 1
CPU: 00: enabled 1
BS: BS_DEV_INIT times (ms): entry 0 run 254 exit 0
FMAP: area RW_ELOG found @ 558000 (4096 bytes)
ELOG: NV offset 0x558000 size 0x1000
read SPI 0x558000 0x1000: 1259 us, 3253 KB/s, 26.024 Mbps
ELOG: area is 4096 bytes, full threshold 3842, shrink size 1024
ELOG: Event(17) added with size 13 at 2025-02-28 19:19:48 UTC
out: cmd=0x121: 03 db 21 01 00 00 00 00 
in-header: 03 1b 00 00 2c 00 00 00 
in-data: 5d 04 00 00 00 00 00 00 02 08 00 00 08 00 00 00 5b 4a e1 0e 08 00 00 00 e6 ec 05 00 08 00 00 00 2a 25 10 00 08 00 00 00 d8 81 08 00 
out: cmd=0xd: 03 f0 0d 00 00 00 00 00 
in-header: 03 19 00 00 08 00 00 00 
in-data: a2 e0 47 00 13 00 00 00 
Chrome EC: UHEPI supported
out: cmd=0xa4: 03 54 a4 00 00 00 0c 00 00 01 00 00 f8 ff 01 00 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
FMAP: area RW_NVRAM found @ 554000 (8192 bytes)
ELOG: Event(A0) added with size 9 at 2025-02-28 19:19:48 UTC
elog_add_boot_reason: Logged dev mode boot
Finalize devices...
Devices finalized
BS: BS_POST_DEVICE times (ms): entry 3 run 0 exit 0
BS: BS_OS_RESUME_CHECK times (ms): entry 0 run 0 exit 0
Writing coreboot table at 0xffed9000
 0. 0000000000114000-000000000011efff: RAMSTAGE
 1. 0000000040000000-000000004023cfff: RAMSTAGE
 2. 000000004023d000-00000000545fffff: RAM
 3. 0000000054600000-000000005465ffff: BL31
 4. 0000000054660000-00000000ffed8fff: RAM
 5. 00000000ffed9000-00000000ffffffff: CONFIGURATION TABLES
 6. 0000000100000000-000000013fffffff: RAM
Passing 5 GPIOs to payload:
            NAME |       PORT | POLARITY |     VALUE
   write protect | 0x00000096 |      low |       low
        EC in RW | 0x000000b1 |     high | undefined
    EC interrupt | 0x00000097 |      low | undefined
   TPM interrupt | 0x00000099 |     high | undefined
  speaker enable | 0x000000af |     high | undefined
out: cmd=0x6: 03 f7 06 00 00 00 00 00 
in-header: 03 f2 00 00 02 00 00 00 
in-data: 09 00 
Board ID: 9
ADC[3]: Raw value=1252987 ID=10
RAM code: 10
SKU ID: 17
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
Wrote coreboot table at: 00000000ffed9000, 0x368 bytes, checksum a8c5
coreboot table: 896 bytes.
IMD ROOT    0. 00000000fffff000 00001000
IMD SMALL   1. 00000000ffffe000 00001000
CONSOLE     2. 00000000fffde000 00020000
FMAP        3. 00000000fffdd000 0000047c
TIME STAMP  4. 00000000fffdc000 00000910
VBOOT WORK  5. 00000000fffdb000 00000f00
RAMOOPS     6. 00000000ffedb000 00100000
COREBOOT    7. 00000000ffed9000 00002000
IMD small region:
  IMD ROOT    0. 00000000ffffec00 00000400
  EC HOSTEVENT 1. 00000000ffffebe0 00000008
  VPD         2. 00000000ffffe9a0 0000022d
BS: BS_WRITE_TABLES times (ms): entry 0 run 0 exit 0
out: cmd=0xa4: 03 e0 a4 00 00 00 0c 00 00 01 00 00 dc 2f 21 40 00 00 00 00 
in-header: 03 e5 00 00 08 00 00 00 
in-data: 80 20 60 10 00 00 00 00 
Probing TPM:  done!
Connected to device vid:did:rid of 1ae0:0028:00
Firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d4903
Initialized TPM device CR50 revision 0
Checking cr50 for pending updates
Reading cr50 TPM mode
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/payload'
CBFS: Found @ offset 50180 size 16deb
read SPI 0x5f91b8 0x16deb: 28556 us, 3280 KB/s, 26.240 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000080000000 memsize 0x11809c0 srcaddr 0x000000004000b438 filesize 0x16db3
Loading Segment: addr: 0x0000000080000000 memsz: 0x00000000011809c0 filesz: 0x0000000000016db3
using LZMA
[ 0x80000000, 80033268, 0x811809c0) <- 4000b438
Clearing Segment: addr: 0x0000000080033268 memsz: 0x000000000114d758
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000080000000
Loaded segments
BS: BS_PAYLOAD_LOAD times (ms): entry 9 run 45 exit 0
Jumping to boot code at 0000000080000000(00000000ffed9000)
CPU0: stack: 0000000000114000 - 0000000000118000, lowest used address 00000000001176a0, stack used: 2400 bytes
CBFS: 'VBOOT' located CBFS at [5a9000:60ffc0)
CBFS: Locating 'fallback/bl31'
CBFS: Found @ offset 36a00 size 4b17
read SPI 0x5dfa28 0x4b17: 5865 us, 3277 KB/s, 26.216 Mbps
Checking segment from ROM address 0x000000004000b400
Checking segment from ROM address 0x000000004000b41c
Loading segment from ROM address 0x000000004000b400
  code (compression=1)
  New segment dstaddr 0x0000000054600000 memsize 0x27000 srcaddr 0x000000004000b438 filesize 0x4adf
Loading Segment: addr: 0x0000000054600000 memsz: 0x0000000000027000 filesz: 0x0000000000004adf
using LZMA
[ 0x54600000, 5460d408, 0x54627000) <- 4000b438
Clearing Segment: addr: 0x000000005460d408 memsz: 0x0000000000019bf8
Loading segment from ROM address 0x000000004000b41c
  Entry Point 0x0000000054601000
Loaded segments
NOTICE:  MT8183 bl31_setup
NOTICE:  BL31: v2.1(release):v2.1-809-g62969c490
NOTICE:  BL31: Built : Mon May 30 03:26:46 UTC 2022
INFO:    [DEVAPC] dump DEVAPC registers:
INFO:    [DEVAPC] (INFRA)D0_APC_0 = 0x0, (INFRA)D1_APC_0 = 0xfcfffffc, (INFRA)D2_APC_0 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_1 = 0x0, (INFRA)D1_APC_1 = 0xffffffff, (INFRA)D2_APC_1 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_2 = 0x0, (INFRA)D1_APC_2 = 0xffffffff, (INFRA)D2_APC_2 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_3 = 0x0, (INFRA)D1_APC_3 = 0xffffffff, (INFRA)D2_APC_3 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_4 = 0x80000000, (INFRA)D1_APC_4 = 0xffffffff, (INFRA)D2_APC_4 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_5 = 0x2aaa, (INFRA)D1_APC_5 = 0xfcff3fff, (INFRA)D2_APC_5 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_6 = 0x0, (INFRA)D1_APC_6 = 0xffffffff, (INFRA)D2_APC_6 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_7 = 0x0, (INFRA)D1_APC_7 = 0xffffffff, (INFRA)D2_APC_7 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_8 = 0x0, (INFRA)D1_APC_8 = 0xffffffff, (INFRA)D2_APC_8 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_9 = 0x0, (INFRA)D1_APC_9 = 0xffffffff, (INFRA)D2_APC_9 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_10 = 0x0, (INFRA)D1_APC_10 = 0xffffffff, (INFRA)D2_APC_10 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_11 = 0x0, (INFRA)D1_APC_11 = 0xffffffff, (INFRA)D2_APC_11 = 0x0
INFO:    [DEVAPC] (INFRA)D0_APC_12 = 0x0, (INFRA)D1_APC_12 = 0xff, (INFRA)D2_APC_12 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_0 = 0x0, (MM)D1_APC_0 = 0xffc000ff, (MM)D2_APC_0 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_1 = 0x0, (MM)D1_APC_1 = 0x3fffffff, (MM)D2_APC_1 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_2 = 0x0, (MM)D1_APC_2 = 0xcffff33c, (MM)D2_APC_2 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_3 = 0x0, (MM)D1_APC_3 = 0x3ccfc0ff, (MM)D2_APC_3 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_4 = 0x0, (MM)D1_APC_4 = 0xffff0000, (MM)D2_APC_4 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_5 = 0x0, (MM)D1_APC_5 = 0xffffffff, (MM)D2_APC_5 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_6 = 0x0, (MM)D1_APC_6 = 0xffffffff, (MM)D2_APC_6 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_7 = 0x0, (MM)D1_APC_7 = 0xffffffff, (MM)D2_APC_7 = 0x0
INFO:    [DEVAPC] (MM)D0_APC_8 = 0x0, (MM)D1_APC_8 = 0x3ffffff, (MM)D2_APC_8 = 0x0
INFO:    [DEVAPC] MAS_DOM_0 = 0x1
INFO:    [DEVAPC] MAS_DOM_1 = 0x200
INFO:    [DEVAPC] MAS_DOM_2 = 0x0
INFO:    [DEVAPC] MAS_DOM_3 = 0x2000
INFO:    [DEVAPC] MAS_SEC_0 = 0x8000000
INFO:    [DEVAPC]  (INFRA)MAS_DOMAIN_REMAP_0 = 0x88, (INFRA)MAS_DOMAIN_REMAP_1 = 0x0
INFO:    [DEVAPC]  (MM)MAS_DOMAIN_REMAP_0 = 0x24
WARNING: region 0:
WARNING: 	apc:0x168, sa:0x0, ea:0xfff
WARNING: region 1:
WARNING: 	apc:0x140, sa:0x1000, ea:0x128f
WARNING: region 2:
WARNING: 	apc:0x168, sa:0x1290, ea:0x1fff
WARNING: region 3:
WARNING: 	apc:0x168, sa:0x2000, ea:0xbfff
WARNING: region 4:
WARNING: 	apc:0x168, sa:0xc000, ea:0x1ffff
WARNING: region 5:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 6:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
WARNING: region 7:
WARNING: 	apc:0x0, sa:0x0, ea:0x0
INFO:    GICv3 without legacy support detected. ARM GICv3 driver initialized in EL3
INFO:    SPM: enable SPMC mode
NOTICE:  spm_boot_init() start
NOTICE:  spm_boot_init() end
INFO:    BL31: Initializing runtime services
INFO:    BL31: Preparing for EL3 exit to normal world
INFO:    Entry point address = 0x80000000
INFO:    SPSR = 0x8


Starting depthcharge on Juniper...
vboot_handoff: creating legacy vboot_handoff structure
vboot_handoff: copying FW preamble
ec_init(0): CrosEC protocol v3 supported (544, 544)
Wipe memory regions:
	[0x00000040000000, 0x00000054600000)
	[0x00000054660000, 0x00000080000000)
	[0x000000811809c0, 0x000000ffed9000)
	[0x00000100000000, 0x00000140000000)
Initializing XHCI USB controller at 0x11200000.
Calling VbSelectAndLoadKernel().
Connected to device vid:did:rid of 1ae0:0028:00
tpm_get_response: command 0x14e, return code 0x0
ReadSpaceKernel: TPM: read secdata_kernel: 02 4c 57 52 47 01 00 01 00 00 00 00 55
RollbackKernelRead: TPM: RollbackKernelRead 0x10001
tpm_get_response: command 0x14e, return code 0x28b
RollbackFwmpRead: TPM: no FWMP space
VbSelectAndLoadKernel: GBB flags are 0x0
print_hash: RW(active) hash: fb5c0dfa6c2692bec07dda7f769b1ccaa90b944b36137e9ce9d22c3b38a385f7
Trying to locate 'ecrw.hash' in CBFS
sync_one_ec: devidx=0 select_rw=4
sync_one_ec: jumping to EC-RW
EC returned from reboot after 22911us
Waiting for EC to clear limit power flag.
vb2_developer_ui: Entering
vboot_draw_screen: screen=0x101 locale=1
CBGFX: cbgfx initialized: screen:width=1366, height=768, offset=0 canvas:width=768, height=768, offset=299
vboot_init_locale: Supported locales: en, es-419, pt-BR, fr, es, pt-PT, ca, it, de, el, nl, da, nb, sv, fi, et, lv, lt, ru, pl, cs, sk, hu, sl, sr, hr, bg, ro, uk, tr, he, ar, fa, hi, th, ms, vi, id, fil, zh-CN, zh-TW, ko, ja, bn, gu, kn, ml, mr, ta, te, (50 locales)
load_archive: loading vbgfx.bin
load_archive: loading font.bin
load_archive: loading locale_es-419.bin
vb2_developer_ui: VbBootDeveloper() - user pressed Ctrl+D; skip delay
vb2_developer_ui: VbBootDeveloper() - trying fixed disk
Man 000045 Snr 2556076829 Product DA4032 Revision 0.1
VbTryLoadKernel: trying disk 0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 4
LoadKernel: Found kernel entry at 65605 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
vb2_load_partition: read 13036 KB in 294 ms at 44207 KB/s.
vb2_load_partition: Partition is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry likes partition 2
LoadKernel: Found kernel entry at 69 size 65536
vb2_verify_keyblock: Checking key block signature...
vb2_verify_kernel_preamble: Verifying kernel preamble.
vb2_verify_kernel_vblock: Kernel preamble is good.
LoadKernel: Key block valid: 1
LoadKernel: Combined version: 65541
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at same prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 2
GptNextKernelEntry: GptNextKernelEntry s1 t0 p1
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 4
GptNextKernelEntry: GptNextKernelEntry s1 t0 p2
GptNextKernelEntry: GptNextKernelEntry looking at new prio partition 6
GptNextKernelEntry: GptNextKernelEntry s0 t15 p0
GptNextKernelEntry: GptNextKernelEntry no more kernels
LoadKernel: Good partition 4
VbTryLoadKernel: LoadKernel() = 0x0
vboot_draw_screen: screen=0x0 locale=1
tpm_get_response: command 0x121, return code 0x0
RollbackKernelLock: TPM: lock secdata_kernel returned 0x0
VbSelectAndLoadKernel: Returning 0
Boot policy: Match for type 0 with cmdline 1
Modified kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
Loading FIT.
Image fdt-36 has 16926 bytes.
Image fdt-35 has 16925 bytes.
Image fdt-34 has 16908 bytes.
Image fdt-33 has 16949 bytes.
Image fdt-32 has 16948 bytes.
Image fdt-31 has 16906 bytes.
Image fdt-30 has 17326 bytes.
Image fdt-29 has 17015 bytes.
Image fdt-28 has 17370 bytes.
Image fdt-27 has 17045 bytes.
Image fdt-26 has 17379 bytes.
Image fdt-25 has 17262 bytes.
Image fdt-24 has 17520 bytes.
Image fdt-23 has 17472 bytes.
Image fdt-22 has 17222 bytes.
Image fdt-21 has 17239 bytes.
Image fdt-20 has 17182 bytes.
Image fdt-19 has 17230 bytes.
Image fdt-18 has 17489 bytes.
Image fdt-17 has 17485 bytes.
Image fdt-16 has 17224 bytes.
Image fdt-15 has 17269 bytes.
Image fdt-14 has 17105 bytes.
Image fdt-13 has 17202 bytes.
Image fdt-12 has 17476 bytes.
Image fdt-11 has 17217 bytes.
Image fdt-10 has 17236 bytes.
Image fdt-9 has 17492 bytes.
Image fdt-8 has 17550 bytes.
Image fdt-7 has 17462 bytes.
Image fdt-6 has 17196 bytes.
Image fdt-5 has 17430 bytes.
Image fdt-4 has 17178 bytes.
Image fdt-3 has 17199 bytes.
Image fdt-2 has 17151 bytes.
Image fdt-1 has 17405 bytes.
Image kernel-1 has 12637811 bytes.
Compat preference: google,juniper-rev9-sku17 google,juniper-sku17 google,juniper-rev9 google,juniper
Config conf-36, kernel kernel-1, fdt fdt-36, compat google,krane-sku176 google,krane mediatek,mt8183
Config conf-35, kernel kernel-1, fdt fdt-35, compat google,krane-sku0 google,krane mediatek,mt8183
Config conf-34, kernel kernel-1, fdt fdt-34, compat google,kodama-sku32 google,kodama mediatek,mt8183
Config conf-33, kernel kernel-1, fdt fdt-33, compat google,kodama-sku288 google,kodama mediatek,mt8183
Config conf-32, kernel kernel-1, fdt fdt-32, compat google,kodama-sku272 google,kodama mediatek,mt8183
Config conf-31, kernel kernel-1, fdt fdt-31, compat google,kodama-sku16 google,kodama mediatek,mt8183
Config conf-30, kernel kernel-1, fdt fdt-30, compat google,katsu mediatek,mt8183
Config conf-29, kernel kernel-1, fdt fdt-29, compat google,katsu-sku38 google,katsu mediatek,mt8183
Config conf-28, kernel kernel-1, fdt fdt-28, compat google,kakadu-rev3 google,kakadu-rev2 google,kakadu mediatek,mt8183
Config conf-27, kernel kernel-1, fdt fdt-27, compat google,kakadu-rev3-sku22 google,kakadu-rev2-sku22 google,kakadu mediatek,mt8183
Config conf-26, kernel kernel-1, fdt fdt-26, compat google,kakadu-rev1 google,kakadu-rev0 google,kakadu mediatek,mt8183
Config conf-25, kernel kernel-1, fdt fdt-25, compat google,willow-sku1 google,willow mediatek,mt8183
Config conf-24, kernel kernel-1, fdt fdt-24, compat google,willow-sku0 google,willow mediatek,mt8183
Config conf-23, kernel kernel-1, fdt fdt-23, compat google,cerise-sku1 google,cerise mediatek,mt8183
Config conf-22, kernel kernel-1, fdt fdt-22, compat google,cerise-rev3-sku1 google,cerise mediatek,mt8183
Config conf-21, kernel kernel-1, fdt fdt-21, compat google,pico-sku2 google,pico mediatek,mt8183
Config conf-20, kernel kernel-1, fdt fdt-20, compat google,pico-sku1 google,pico mediatek,mt8183
Config conf-19, kernel kernel-1, fdt fdt-19, compat google,makomo-rev4-sku1 google,makomo-rev5-sku1 google,makomo mediatek,mt8183
Config conf-18, kernel kernel-1, fdt fdt-18, compat google,makomo-rev4-sku0 google,makomo-rev5-sku0 google,makomo mediatek,mt8183
Config conf-17, kernel kernel-1, fdt fdt-17, compat google,makomo-rev3-sku0 google,makomo mediatek,mt8183
Config conf-16, kernel kernel-1, fdt fdt-16, compat google,makomo-rev0-sku0 google,makomo mediatek,mt8183
Config conf-15, kernel kernel-1, fdt fdt-15, compat google,juniper-sku17 (match) google,juniper mediatek,mt8183
Config conf-14, kernel kernel-1, fdt fdt-14, compat google,kappa mediatek,mt8183
Config conf-13, kernel kernel-1, fdt fdt-13, compat google,juniper-sku16 google,juniper (match) mediatek,mt8183
Config conf-12, kernel kernel-1, fdt fdt-12, compat google,fennel-sku0 google,fennel mediatek,mt8183
Config conf-11, kernel kernel-1, fdt fdt-11, compat google,fennel-sku2 google,fennel mediatek,mt8183
Config conf-10, kernel kernel-1, fdt fdt-10, compat google,fennel-sku7 google,fennel mediatek,mt8183
Config conf-9, kernel kernel-1, fdt fdt-9, compat google,fennel-sku6 google,fennel mediatek,mt8183
Config conf-8, kernel kernel-1, fdt fdt-8, compat google,fennel-sku1 google,fennel mediatek,mt8183
Config conf-7, kernel kernel-1, fdt fdt-7, compat google,damu mediatek,mt8183
Config conf-6, kernel kernel-1, fdt fdt-6, compat google,cozmo mediatek,mt8183
Config conf-5, kernel kernel-1, fdt fdt-5, compat google,cerise-sku0 google,cerise mediatek,mt8183
Config conf-4, kernel kernel-1, fdt fdt-4, compat google,cerise-rev3-sku0 google,cerise mediatek,mt8183
Config conf-3, kernel kernel-1, fdt fdt-3, compat google,burnet mediatek,mt8183
Config conf-2, kernel kernel-1, fdt fdt-2, compat google,bellis-rev0-sku1 google,bellis mediatek,mt8183
Config conf-1, kernel kernel-1, fdt fdt-1, compat google,bellis-rev0-sku0 google,bellis mediatek,mt8183
Choosing best match conf-15 for compat google,juniper-sku17.
LZ4 decompressing fdt-15 to 0x5f800000
tpm_get_response: command 0x17b, return code 0x0
tpm_cleanup: add release locality here.
Shutting down all USB controllers.
Exiting depthcharge with code 4 at timestamp: 22414502
LZ4 decompressing kernel-1 to 0x8017b418
LZ4 decompressing kernel-1 to 0x40000000
jumping to kernel
WARNING: Unimplemented Arm Architecture Service Call: 0x80000002 
