-----------
Port C0: enabled, disconnected  State:
Role:SNK UFP, Polarity:CC1
CC State:None
Cable type:Passive
TBT Adapter type:Gen3
Optical Cable:False
Link LSRX Communication:Bi-directional
TBT Cable Speed:UNKNOWN
Rounded support: 3rd Gen rounded support
Port C0 SOP Discovery
-----------
