<6>[    0.000000] Booting Linux on physical CPU 0x0000000000 [0x410fd034]
<5>[    0.000000] Linux version 5.10.230-25844-gdc65f732bf53 (cros-kernel@chromium.org) (Chromium OS 19.0_pre530567 clang version 19.0.0git (/mnt/host/source/src/third_party/llvm-project 3b5e7c83a6e226d5bd7ed2e9b67449b64812074c), LLD 19.0.0) #1 SMP PREEMPT Thu, 2 Jan 2025 01:16:47 -0800
<5>[    0.000000] random: crng init done
<6>[    0.000000] Machine model: Google kenzo sku17 board
<6>[    0.000000] Reserved memory: created DMA memory pool at 0x0000000050000000, size 41 MiB
<6>[    0.000000] OF: reserved mem: initialized node memory@50000000, compatible id shared-dma-pool
<6>[    0.000000] Zone ranges:
<6>[    0.000000]   DMA      [mem 0x0000000040000000-0x00000000ffffffff]
<6>[    0.000000]   DMA32    empty
<6>[    0.000000]   Normal   [mem 0x0000000100000000-0x000000013fffffff]
<6>[    0.000000] Movable zone start for each node
<6>[    0.000000] Early memory node ranges
<6>[    0.000000]   node   0: [mem 0x0000000040000000-0x000000004fffffff]
<6>[    0.000000]   node   0: [mem 0x0000000050000000-0x00000000528fffff]
<6>[    0.000000]   node   0: [mem 0x0000000052900000-0x00000000545fffff]
<6>[    0.000000]   node   0: [mem 0x0000000054700000-0x00000000ffdfffff]
<6>[    0.000000]   node   0: [mem 0x0000000100000000-0x000000013fffffff]
<6>[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000013fffffff]
<7>[    0.000000] On node 0 totalpages: 1047808
<7>[    0.000000]   DMA zone: 12288 pages used for memmap
<7>[    0.000000]   DMA zone: 0 pages reserved
<7>[    0.000000]   DMA zone: 785664 pages, LIFO batch:63
<7>[    0.000000]   Normal zone: 4096 pages used for memmap
<7>[    0.000000]   Normal zone: 262144 pages, LIFO batch:63
<6>[    0.000000] On node 0, zone DMA: 256 pages in unavailable ranges
<6>[    0.000000] On node 0, zone Normal: 512 pages in unavailable ranges
<6>[    0.000000] psci: probing for conduit method from DT.
<6>[    0.000000] psci: PSCIv1.1 detected in firmware.
<6>[    0.000000] psci: Using standard PSCI v0.2 function IDs
<6>[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
<6>[    0.000000] psci: SMC Calling Convention v1.2
<6>[    0.000000] percpu: Embedded 32 pages/cpu s93592 r8192 d29288 u131072
<7>[    0.000000] pcpu-alloc: s93592 r8192 d29288 u131072 alloc=32*4096
<7>[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 [0] 4 [0] 5 [0] 6 [0] 7 
<6>[    0.000000] Detected VIPT I-cache on CPU0
<6>[    0.000000] CPU features: detected: ARM erratum 845719
<6>[    0.000000] CPU features: detected: GIC system register CPU interface
<6>[    0.000000] CPU features: kernel page table isolation forced ON by KASLR
<6>[    0.000000] CPU features: detected: Kernel page table isolation (KPTI)
<6>[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1031424
<5>[    0.000000] Kernel command line: cros_secure console= loglevel=7 init=/sbin/init cros_secure drm.trace=0x106 root=/dev/dm-0 rootwait ro dm_verity.error_behavior=3 dm_verity.max_bios=-1 dm_verity.dev_wait=1 dm="1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583" noinitrd vt.global_cursor_default=0 kern_guid=873d93f3-0066-4720-87c3-b0fe6a96eb51 cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4= cpuidle.governor=teo irqchip.gicv3_pseudo_nmi=1
<6>[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes, linear)
<6>[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes, linear)
<6>[    0.000000] mem auto-init: stack:all(zero), heap alloc:on, heap free:off
<6>[    0.000000] software IO TLB: mapped [mem 0x00000000fbe00000-0x00000000ffe00000] (64MB)
<6>[    0.000000] Memory: 3971572K/4191232K available (13758K kernel code, 2436K rwdata, 9280K rodata, 1408K init, 1075K bss, 219660K reserved, 0K cma-reserved)
<6>[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=8, Nodes=1
<6>[    0.000000] ftrace: allocating 40629 entries in 159 pages
<6>[    0.000000] ftrace: allocated 159 pages with 6 groups
<6>[    0.000000] rcu: Preemptible hierarchical RCU implementation.
<6>[    0.000000] 	Trampoline variant of Tasks RCU enabled.
<6>[    0.000000] 	Rude variant of Tasks RCU enabled.
<6>[    0.000000] 	Tracing variant of Tasks RCU enabled.
<6>[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 100 jiffies.
<6>[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
<6>[    0.000000] GIC: enabling workaround for GICv3: Mediatek Chromebook GICR save problem
<6>[    0.000000] GICv3: GIC: Using split EOI/Deactivate mode
<6>[    0.000000] GICv3: 640 SPIs implemented
<6>[    0.000000] GICv3: 0 Extended SPIs implemented
<6>[    0.000000] GICv3: Distributor has no Range Selector support
<6>[    0.000000] GICv3: 16 PPIs implemented
<6>[    0.000000] GICv3: CPU0: found redistributor 0 region 0:0x000000000c100000
<6>[    0.000000] GICv3: GIC: PPI partition interrupt-partition-0[0] { /cpus/cpu@0[0] /cpus/cpu@1[1] /cpus/cpu@2[2] /cpus/cpu@3[3] }
<6>[    0.000000] GICv3: GIC: PPI partition interrupt-partition-1[1] { /cpus/cpu@100[4] /cpus/cpu@101[5] /cpus/cpu@102[6] /cpus/cpu@103[7] }
<6>[    0.000000] rcu: 	Offload RCU callbacks from CPUs: 0-7.
<6>[    0.000000] kfence: initialized - using 2097152 bytes for 255 objects at 0x(____ptrval____)-0x(____ptrval____)
<6>[    0.000000] arch_timer: cp15 timer(s) running at 13.00MHz (phys).
<6>[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x2ff89eacb, max_idle_ns: 440795202429 ns
<6>[    0.000002] sched_clock: 56 bits at 13MHz, resolution 76ns, wraps every 4398046511101ns
<6>[    0.000351] Calibrating delay loop (skipped), value calculated using timer frequency.. 26.00 BogoMIPS (lpj=13000)
<6>[    0.000359] pid_max: default: 32768 minimum: 301
<6>[    0.000438] LSM: Security Framework initializing
<6>[    0.000470] landlock: Up and running.
<6>[    0.000473] Yama: becoming mindful.
<6>[    0.000484] LoadPin: ready to pin (currently enforcing)
<6>[    0.000501] Chromium OS LSM: enabled
<6>[    0.000503] SELinux:  Initializing.
<6>[    0.000547] LSM support for eBPF active
<6>[    0.000583] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
<6>[    0.000596] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes, linear)
<6>[    0.001976] rcu: Hierarchical SRCU implementation.
<6>[    0.002644] smp: Bringing up secondary CPUs ...
<6>[    0.003280] Detected VIPT I-cache on CPU1
<6>[    0.003303] GICv3: CPU1: found redistributor 1 region 0:0x000000000c120000
<6>[    0.003333] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
<6>[    0.003955] Detected VIPT I-cache on CPU2
<6>[    0.003966] GICv3: CPU2: found redistributor 2 region 0:0x000000000c140000
<6>[    0.003978] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
<6>[    0.004553] Detected VIPT I-cache on CPU3
<6>[    0.004562] GICv3: CPU3: found redistributor 3 region 0:0x000000000c160000
<6>[    0.004574] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
<6>[    0.005261] CPU features: detected: ARM erratum 858921
<6>[    0.005267] CPU features: detected: Spectre-v2
<6>[    0.005274] CPU features: detected: Spectre-BHB
<6>[    0.005277] Detected VIPT I-cache on CPU4
<6>[    0.005293] GICv3: CPU4: found redistributor 100 region 0:0x000000000c180000
<6>[    0.005299] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.005307] arch_timer: CPU4: Trapping CNTVCT access
<6>[    0.005317] CPU4: Booted secondary processor 0x0000000100 [0x410fd092]
<6>[    0.005860] Detected VIPT I-cache on CPU5
<6>[    0.005872] GICv3: CPU5: found redistributor 101 region 0:0x000000000c1a0000
<6>[    0.005877] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.005882] arch_timer: CPU5: Trapping CNTVCT access
<6>[    0.005889] CPU5: Booted secondary processor 0x0000000101 [0x410fd092]
<6>[    0.006460] Detected VIPT I-cache on CPU6
<6>[    0.006472] GICv3: CPU6: found redistributor 102 region 0:0x000000000c1c0000
<6>[    0.006478] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.006483] arch_timer: CPU6: Trapping CNTVCT access
<6>[    0.006489] CPU6: Booted secondary processor 0x0000000102 [0x410fd092]
<6>[    0.007060] Detected VIPT I-cache on CPU7
<6>[    0.007073] GICv3: CPU7: found redistributor 103 region 0:0x000000000c1e0000
<6>[    0.007078] arch_timer: Enabling local workaround for ARM erratum 858921
<6>[    0.007083] arch_timer: CPU7: Trapping CNTVCT access
<6>[    0.007090] CPU7: Booted secondary processor 0x0000000103 [0x410fd092]
<6>[    0.007161] smp: Brought up 1 node, 8 CPUs
<6>[    0.007200] SMP: Total of 8 processors activated.
<6>[    0.007204] CPU features: detected: 32-bit EL0 Support
<6>[    0.007208] CPU features: detected: CRC32 instructions
<6>[    0.007212] CPU features: detected: 32-bit EL1 Support
<6>[    0.007365] CPU features: emulated: Privileged Access Never (PAN) using TTBR0_EL1 switching
<6>[    0.020736] CPU: All CPU(s) started at EL2
<6>[    0.020766] alternatives: patching kernel code
<6>[    0.021967] devtmpfs: initialized
<6>[    0.029724] KASLR enabled
<6>[    0.029850] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
<6>[    0.029877] futex hash table entries: 2048 (order: 5, 131072 bytes, linear)
<6>[    0.030089] pinctrl core: initialized pinctrl subsystem
<6>[    0.030547] NET: Registered protocol family 16
<6>[    0.031267] DMA: preallocated 512 KiB GFP_KERNEL pool for atomic allocations
<6>[    0.031476] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
<6>[    0.031679] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
<6>[    0.031726] audit: initializing netlink subsys (disabled)
<5>[    0.031897] audit: type=2000 audit(0.031:1): state=initialized audit_enabled=0 res=1
<6>[    0.032100] thermal_sys: Registered thermal governor 'step_wise'
<6>[    0.032103] thermal_sys: Registered thermal governor 'user_space'
<6>[    0.032108] thermal_sys: Registered thermal governor 'power_allocator'
<4>[    0.032572] thermal thermal_zone7: power_allocator: sustainable_power will be estimated
<4>[    0.032610] thermal thermal_zone8: power_allocator: sustainable_power will be estimated
<6>[    0.032705] cpuidle: using governor ladder
<6>[    0.032815] cpuidle: using governor menu
<6>[    0.032829] cpuidle: using governor teo
<6>[    0.033004] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
<6>[    0.033106] ASID allocator initialised with 32768 entries
<6>[    0.034499] printk: console [ramoops-1] enabled
<6>[    0.034617] pstore: Registered ramoops as persistent store backend
<6>[    0.034623] ramoops: using 0x100000@0xffedb000, ecc: 0
<7>[    0.091995] gpiochip_find_base: found new base at 320
<7>[    0.092029] gpio gpiochip0: (pinctrl_paris): created GPIO range 0->191 ==> 10005000.pinctrl PIN 0->191
<7>[    0.092277] gpio gpiochip0: (pinctrl_paris): added GPIO chardev (254:0)
<7>[    0.092323] gpio gpiochip0: registered GPIOs 320 to 511 on pinctrl_paris
<6>[    0.101243] cryptd: max_cpu_qlen set to 1000
<7>[    0.102802] reg-fixed-voltage regulator0: GPIO lookup for consumer (null)
<7>[    0.102806] reg-fixed-voltage regulator0: using device tree for GPIO lookup
<7>[    0.102821] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator0[0]'
<7>[    0.102835] of_get_named_gpiod_flags: parsed 'gpio' property of node '/regulator0[0]' - status (0)
<7>[    0.102854] gpio gpiochip0: Persistence not supported for GPIO 178
<7>[    0.102980] reg-fixed-voltage regulator1: GPIO lookup for consumer (null)
<7>[    0.102983] reg-fixed-voltage regulator1: using device tree for GPIO lookup
<7>[    0.102991] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator1[0]'
<7>[    0.102999] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator1[0]'
<7>[    0.103003] reg-fixed-voltage regulator1: using lookup tables for GPIO lookup
<7>[    0.103007] reg-fixed-voltage regulator1: No GPIO consumer (null) found
<7>[    0.103104] reg-fixed-voltage regulator2: GPIO lookup for consumer (null)
<7>[    0.103107] reg-fixed-voltage regulator2: using device tree for GPIO lookup
<7>[    0.103114] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator2[0]'
<7>[    0.103121] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator2[0]'
<7>[    0.103125] reg-fixed-voltage regulator2: using lookup tables for GPIO lookup
<7>[    0.103129] reg-fixed-voltage regulator2: No GPIO consumer (null) found
<7>[    0.103217] reg-fixed-voltage regulator3: GPIO lookup for consumer (null)
<7>[    0.103220] reg-fixed-voltage regulator3: using device tree for GPIO lookup
<7>[    0.103231] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator3[0]'
<7>[    0.103237] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator3[0]'
<7>[    0.103242] reg-fixed-voltage regulator3: using lookup tables for GPIO lookup
<7>[    0.103245] reg-fixed-voltage regulator3: No GPIO consumer (null) found
<7>[    0.103336] reg-fixed-voltage regulator4: GPIO lookup for consumer (null)
<7>[    0.103339] reg-fixed-voltage regulator4: using device tree for GPIO lookup
<7>[    0.103346] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator4[0]'
<7>[    0.103352] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator4[0]'
<7>[    0.103357] reg-fixed-voltage regulator4: using lookup tables for GPIO lookup
<7>[    0.103360] reg-fixed-voltage regulator4: No GPIO consumer (null) found
<7>[    0.103461] reg-fixed-voltage regulator5: GPIO lookup for consumer (null)
<7>[    0.103464] reg-fixed-voltage regulator5: using device tree for GPIO lookup
<7>[    0.103471] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator5[0]'
<7>[    0.103478] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator5[0]'
<7>[    0.103482] reg-fixed-voltage regulator5: using lookup tables for GPIO lookup
<7>[    0.103485] reg-fixed-voltage regulator5: No GPIO consumer (null) found
<7>[    0.103576] reg-fixed-voltage regulator6: GPIO lookup for consumer (null)
<7>[    0.103579] reg-fixed-voltage regulator6: using device tree for GPIO lookup
<7>[    0.103586] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/regulator6[0]'
<7>[    0.103593] of_get_named_gpiod_flags: can't parse 'gpio' property of node '/regulator6[0]'
<7>[    0.103597] reg-fixed-voltage regulator6: using lookup tables for GPIO lookup
<7>[    0.103600] reg-fixed-voltage regulator6: No GPIO consumer (null) found
<7>[    0.103761] reg-fixed-voltage pp1200-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.103764] reg-fixed-voltage pp1200-mipibrdg: using device tree for GPIO lookup
<7>[    0.103773] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp1200-mipibrdg[0]'
<7>[    0.103784] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp1200-mipibrdg[0]' - status (0)
<7>[    0.103793] gpio gpiochip0: Persistence not supported for GPIO 54
<6>[    0.103808] pp1200_mipibrdg: supplied by pp1800_alw
<7>[    0.104091] reg-fixed-voltage pp1800-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.104094] reg-fixed-voltage pp1800-mipibrdg: using device tree for GPIO lookup
<7>[    0.104103] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp1800-mipibrdg[0]'
<7>[    0.104114] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp1800-mipibrdg[0]' - status (0)
<7>[    0.104122] gpio gpiochip0: Persistence not supported for GPIO 36
<6>[    0.104136] pp1800_mipibrdg: supplied by pp1800_alw
<7>[    0.104331] reg-fixed-voltage pp3300-panel: GPIO lookup for consumer (null)
<7>[    0.104334] reg-fixed-voltage pp3300-panel: using device tree for GPIO lookup
<7>[    0.104343] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/pp3300-panel[0]'
<7>[    0.104353] of_get_named_gpiod_flags: parsed 'gpio' property of node '/pp3300-panel[0]' - status (0)
<7>[    0.104361] gpio gpiochip0: Persistence not supported for GPIO 35
<6>[    0.104373] pp3300_panel: supplied by pp3300_alw
<7>[    0.104577] reg-fixed-voltage vddio-mipibrdg: GPIO lookup for consumer (null)
<7>[    0.104580] reg-fixed-voltage vddio-mipibrdg: using device tree for GPIO lookup
<7>[    0.104590] of_get_named_gpiod_flags: can't parse 'gpios' property of node '/vddio-mipibrdg[0]'
<7>[    0.104601] of_get_named_gpiod_flags: parsed 'gpio' property of node '/vddio-mipibrdg[0]' - status (0)
<7>[    0.104609] gpio gpiochip0: Persistence not supported for GPIO 37
<6>[    0.104621] vddio_mipibrdg: supplied by pp3300_alw
<6>[    0.105007] iommu: Default domain type: Translated 
<6>[    0.105116] vgaarb: loaded
<5>[    0.105374] SCSI subsystem initialized
<6>[    0.105457] usbcore: registered new interface driver usbfs
<6>[    0.105488] usbcore: registered new interface driver hub
<6>[    0.105507] usbcore: registered new device driver usb
<6>[    0.105536] mc: Linux media interface: v0.10
<6>[    0.105550] videodev: Linux video capture interface: v2.00
<7>[    0.106584] mediatek,efuse 8000000.soc_data: GPIO lookup for consumer wp
<7>[    0.106588] mediatek,efuse 8000000.soc_data: using device tree for GPIO lookup
<7>[    0.106601] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/soc_data@8000000[0]'
<7>[    0.106609] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/soc_data@8000000[0]'
<7>[    0.106616] mediatek,efuse 8000000.soc_data: using lookup tables for GPIO lookup
<7>[    0.106620] mediatek,efuse 8000000.soc_data: No GPIO consumer wp found
<7>[    0.106784] mediatek,efuse 11f10000.efuse: GPIO lookup for consumer wp
<7>[    0.106787] mediatek,efuse 11f10000.efuse: using device tree for GPIO lookup
<7>[    0.106795] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/efuse@11f10000[0]'
<7>[    0.106803] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/efuse@11f10000[0]'
<7>[    0.106808] mediatek,efuse 11f10000.efuse: using lookup tables for GPIO lookup
<7>[    0.106811] mediatek,efuse 11f10000.efuse: No GPIO consumer wp found
<6>[    0.106986] Advanced Linux Sound Architecture Driver Initialized.
<6>[    0.107633] clocksource: Switched to clocksource arch_sys_counter
<5>[    0.126779] VFS: Disk quotas dquot_6.6.0
<6>[    0.126829] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
<6>[    0.127461] NET: Registered protocol family 2
<6>[    0.127584] IP idents hash table entries: 65536 (order: 7, 524288 bytes, linear)
<6>[    0.129420] tcp_listen_portaddr_hash hash table entries: 2048 (order: 3, 32768 bytes, linear)
<6>[    0.129523] TCP established hash table entries: 32768 (order: 6, 262144 bytes, linear)
<6>[    0.129716] TCP bind hash table entries: 32768 (order: 7, 524288 bytes, linear)
<6>[    0.129969] TCP: Hash tables configured (established 32768 bind 32768)
<6>[    0.130065] UDP hash table entries: 2048 (order: 4, 65536 bytes, linear)
<6>[    0.130137] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes, linear)
<6>[    0.130289] NET: Registered protocol family 1
<6>[    0.130310] PCI: CLS 0 bytes, default 64
<6>[    0.131093] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counters available
<6>[    0.131282] hw perfevents: enabled with armv8_cortex_a73 PMU driver, 7 counters available
<6>[    0.131707] kvm [1]: IPA Size Limit: 40 bits
<6>[    0.132395] kvm [1]: vgic-v2@c420000
<6>[    0.132415] kvm [1]: GIC system register CPU interface enabled
<6>[    0.132529] kvm [1]: vgic interrupt IRQ18
<6>[    0.132667] kvm [1]: Hyp mode initialized successfully
<5>[    0.136141] Initialise system trusted keyrings
<6>[    0.136238] workingset: timestamp_bits=62 max_order=20 bucket_order=0
<6>[    0.139177] squashfs: version 4.0 (2009/01/31) Phillip Lougher
<6>[    0.139378] Registering esdfs 0.2
<6>[    0.139521] alt_syscall: table 'read_write_test' available.
<6>[    0.139544] alt_syscall: table 'android' available.
<6>[    0.139567] alt_syscall: table 'android_permissive' available.
<6>[    0.139592] alt_syscall: table 'third_party' available.
<6>[    0.139610] alt_syscall: table 'third_party_permissive' available.
<6>[    0.139638] alt_syscall: table 'complete' available.
<6>[    0.139655] alt_syscall: table 'complete_permissive' available.
<5>[    0.166396] Key type asymmetric registered
<5>[    0.166404] Asymmetric key parser 'x509' registered
<6>[    0.166431] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 246)
<6>[    0.166507] io scheduler mq-deadline registered
<6>[    0.166514] io scheduler kyber registered
<6>[    0.166570] io scheduler bfq registered
<7>[    0.168646] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.168650] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.168668] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.168683] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.168686] gpio-496 (enable): no flags found for enable
<4>[    0.168907] of_fixed_factor_clk: probe of fixed-factor-clock-13m failed with error -17
<3>[    0.179647] mtk-socinfo mtk-socinfo.0.auto: error -ENOENT: Failed to get socinfo data
<4>[    0.179663] mtk-socinfo: probe of mtk-socinfo.0.auto failed with error -2
<6>[    0.179725] mtk-socinfo mtk-socinfo.1.auto: SoC detected, family: MediaTek, soc_id: MT8183, machine: Kompanio 500
<6>[    0.180429] Serial: 8250/16550 driver, 4 ports, IRQ sharing disabled
<7>[    0.181456] mt6577-uart 11002000.serial: GPIO lookup for consumer rs485-term
<7>[    0.181460] mt6577-uart 11002000.serial: using device tree for GPIO lookup
<7>[    0.181474] of_get_named_gpiod_flags: can't parse 'rs485-term-gpios' property of node '/soc/serial@11002000[0]'
<7>[    0.181483] of_get_named_gpiod_flags: can't parse 'rs485-term-gpio' property of node '/soc/serial@11002000[0]'
<7>[    0.181490] mt6577-uart 11002000.serial: using lookup tables for GPIO lookup
<7>[    0.181494] mt6577-uart 11002000.serial: No GPIO consumer rs485-term found
<6>[    0.201615] 11002000.serial: ttyS0 at MMIO 0x11002000 (irq = 33, base_baud = 1625000) is a ST16650V2
<7>[    0.202200] mt6577-uart 11003000.serial: GPIO lookup for consumer rs485-term
<7>[    0.202204] mt6577-uart 11003000.serial: using device tree for GPIO lookup
<7>[    0.202214] of_get_named_gpiod_flags: can't parse 'rs485-term-gpios' property of node '/soc/serial@11003000[0]'
<7>[    0.202222] of_get_named_gpiod_flags: can't parse 'rs485-term-gpio' property of node '/soc/serial@11003000[0]'
<7>[    0.202227] mt6577-uart 11003000.serial: using lookup tables for GPIO lookup
<7>[    0.202230] mt6577-uart 11003000.serial: No GPIO consumer rs485-term found
<6>[    0.222342] 11003000.serial: ttyS1 at MMIO 0x11003000 (irq = 34, base_baud = 1625000) is a ST16650V2
<6>[    0.222444] serial serial0: tty port ttyS1 registered
<6>[    0.226941] usbcore: registered new interface driver udl
<6>[    0.229583] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14008000
<6>[    0.229617] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@14009000
<6>[    0.229650] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ovl@1400a000
<6>[    0.229678] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400b000
<6>[    0.229704] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/rdma@1400c000
<6>[    0.229738] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/color@1400e000
<6>[    0.229765] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/ccorr@1400f000
<6>[    0.229792] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/aal@14010000
<6>[    0.229819] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/gamma@14011000
<6>[    0.229896] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dsi@14014000
<6>[    0.229925] mediatek-drm mediatek-drm.3.auto: Adding component match for /soc/dpi@14015000
<7>[    0.233054] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.233058] panel-edp panel: using device tree for GPIO lookup
<7>[    0.233069] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.233077] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.233083] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.233087] panel-edp panel: No GPIO consumer hpd found
<7>[    0.233164] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.233167] panel-edp panel: using device tree for GPIO lookup
<7>[    0.233175] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.233182] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.233186] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.233189] panel-edp panel: No GPIO consumer enable found
<6>[    0.233702] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.233716] mali 13040000.mali: IRQ JOB not found
<3>[    0.233765] mali 13040000.mali: IRQ MMU not found
<3>[    0.233776] mali 13040000.mali: IRQ GPU not found
<6>[    0.233800] mali 13040000.mali: GPU metrics tracepoint support enabled
<4>[    0.233916] cacheinfo: Unable to detect cache hierarchy for CPU 0
<6>[    0.236171] loop: module loaded
<6>[    0.236333] lkdtm: No crash points registered, enable through debugfs
<6>[    0.245110] vsim1: Bringing 1800000uV into 2700000-2700000uV
<7>[    0.255403] of_get_named_gpiod_flags: parsed 'cs-gpios' property of node '/soc/spi@1100a000[0]' - status (0)
<4>[    0.256768] spi-nor spi1.0: found w25q64jwm, expected w25q64dw
<6>[    0.257319] spi-nor spi1.0: w25q64jwm (8192 Kbytes)
<7>[    0.257451] mtd mtd0: GPIO lookup for consumer wp
<7>[    0.257455] mtd mtd0: using device tree for GPIO lookup
<7>[    0.257467] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/spi@11010000/spi-flash@0[0]'
<7>[    0.257476] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/spi@11010000/spi-flash@0[0]'
<7>[    0.257482] mtd mtd0: using lookup tables for GPIO lookup
<7>[    0.257486] mtd mtd0: No GPIO consumer wp found
<7>[    0.259222] mdio_bus fixed-0: GPIO lookup for consumer reset
<7>[    0.259226] mdio_bus fixed-0: using lookup tables for GPIO lookup
<7>[    0.259230] mdio_bus fixed-0: No GPIO consumer reset found
<6>[    0.259243] PPP generic driver version 2.4.2
<6>[    0.259334] PPP MPPE Compression module registered
<6>[    0.260036] mtu3 11201000.usb: uwk - reg:0x420, version:101
<4>[    0.260082] mtu3 11201000.usb: supply vbus not found, using dummy regulator
<6>[    0.260147] mtu3 11201000.usb: dr_mode: 1, is_u3_dr: 0, u3p_dis_msk: 0, drd: auto
<6>[    0.260859] mtu3 11201000.usb: xHCI platform device register success...
<6>[    0.261057] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
<6>[    0.261063] ehci-pci: EHCI PCI platform driver
<6>[    0.261098] ehci-platform: EHCI generic platform driver
<6>[    0.261246] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
<6>[    0.261268] ohci-pci: OHCI PCI platform driver
<6>[    0.261288] ohci-platform: OHCI generic platform driver
<4>[    0.261884] xhci-mtk 11200000.xhci: supply vbus not found, using dummy regulator
<6>[    0.262062] tpm_tis_spi spi0.0: TPM ready IRQ confirmed on attempt 2
<6>[    0.262170] xhci-mtk 11200000.xhci: xHCI Host Controller
<6>[    0.262269] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 1
<6>[    0.262345] xhci-mtk 11200000.xhci: hcc params 0x01400f99 hci version 0x110 quirks 0x0000000000210010
<6>[    0.262383] xhci-mtk 11200000.xhci: irq 290, io mem 0x11200000
<6>[    0.262462] xhci-mtk 11200000.xhci: xHCI Host Controller
<6>[    0.262531] xhci-mtk 11200000.xhci: new USB bus registered, assigned bus number 2
<6>[    0.262543] xhci-mtk 11200000.xhci: Host supports USB 3.0 SuperSpeed
<6>[    0.262623] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.10
<6>[    0.262638] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    0.262645] usb usb1: Product: xHCI Host Controller
<6>[    0.262650] usb usb1: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
<6>[    0.262656] usb usb1: SerialNumber: 11200000.xhci
<6>[    0.262902] hub 1-0:1.0: USB hub found
<6>[    0.262923] hub 1-0:1.0: 1 port detected
<6>[    0.263098] usb usb2: We don't know the algorithms for LPM for this host, disabling LPM.
<6>[    0.263144] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.10
<6>[    0.263151] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    0.263156] usb usb2: Product: xHCI Host Controller
<6>[    0.263162] usb usb2: Manufacturer: Linux 5.10.230-25844-gdc65f732bf53 xhci-hcd
<6>[    0.263167] usb usb2: SerialNumber: 11200000.xhci
<6>[    0.263352] hub 2-0:1.0: USB hub found
<3>[    0.263369] hub 2-0:1.0: config failed, hub doesn't have any ports! (err -19)
<6>[    0.263561] usbcore: registered new interface driver cdc_acm
<6>[    0.263567] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
<6>[    0.263599] usbcore: registered new interface driver usb-storage
<6>[    0.264777] mt6397-rtc mt6358-rtc: registered as rtc0
<6>[    0.264950] mt6397-rtc mt6358-rtc: setting system clock to 2025-02-28T19:20:10 UTC (1740770410)
<6>[    0.264982] i2c /dev entries driver
<4>[    0.268257] elan_i2c 2-0015: supply vcc not found, using dummy regulator
<6>[    0.271338] tpm_tis_spi spi0.0: 2.0 TPM (device-id 0x28, rev-id 0)
<6>[    0.271934] mtk-wdt 10007000.watchdog: Watchdog enabled (timeout=31 sec, nowayout=0)
<6>[    0.272280] device-mapper: ioctl: 4.43.0-ioctl (2020-10-01) initialised: dm-devel@redhat.com
<6>[    0.272420] device-mapper: verity-chromeos: dm-verity-chromeos registered
<4>[    0.272788] cpu cpu0: dummy supplies not allowed for exclusive requests
<4>[    0.273573] cpu cpu4: dummy supplies not allowed for exclusive requests
<6>[    0.274413] cpu cpu0: EM: created perf domain
<6>[    0.274757] cpu cpu4: EM: created perf domain
<6>[    0.275107] cpufreq: cpufreq_online: CPU4: Running at unlisted initial frequency: 1199999 KHz, changing to: 1248000 KHz
<7>[    0.276311] pwrseq_simple wifi-pwrseq: GPIO lookup for consumer reset
<7>[    0.276314] pwrseq_simple wifi-pwrseq: using device tree for GPIO lookup
<7>[    0.276327] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/wifi-pwrseq[0]' - status (0)
<7>[    0.276339] gpio gpiochip0: Persistence not supported for GPIO 119
<6>[    0.276501] sdhci: Secure Digital Host Controller Interface driver
<6>[    0.276505] sdhci: Copyright(c) Pierre Ossman
<6>[    0.276691] sdhci-pltfm: SDHCI platform and OF driver helper
<3>[    0.277464] SMCCC: SOC_ID: ARCH_SOC_ID(0) returned error: ffffffffffffffff
<6>[    0.277489] hid: raw HID events driver (C) Jiri Kosina
<7>[    0.277529] mtk-msdc 11230000.mmc: GPIO lookup for consumer wp
<7>[    0.277531] mtk-msdc 11240000.mmc: GPIO lookup for consumer wp
<7>[    0.277534] mtk-msdc 11240000.mmc: using device tree for GPIO lookup
<7>[    0.277536] mtk-msdc 11230000.mmc: using device tree for GPIO lookup
<7>[    0.277546] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/mmc@11230000[0]'
<7>[    0.277550] of_get_named_gpiod_flags: can't parse 'wp-gpios' property of node '/soc/mmc@11240000[0]'
<7>[    0.277557] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/mmc@11240000[0]'
<7>[    0.277560] of_get_named_gpiod_flags: can't parse 'wp-gpio' property of node '/soc/mmc@11230000[0]'
<7>[    0.277566] mtk-msdc 11240000.mmc: using lookup tables for GPIO lookup
<7>[    0.277567] mtk-msdc 11230000.mmc: using lookup tables for GPIO lookup
<7>[    0.277570] mtk-msdc 11230000.mmc: No GPIO consumer wp found
<7>[    0.277572] mtk-msdc 11240000.mmc: No GPIO consumer wp found
<6>[    0.277690] mtk-msdc 11240000.mmc: allocated mmc-pwrseq
<6>[    0.277837] usbcore: registered new interface driver usbhid
<6>[    0.277842] usbhid: USB HID core driver
<4>[    0.278152] i2c_hid_of 0-0040: supply vdd not found, using dummy regulator
<6>[    0.278155] ashmem: initialized
<4>[    0.278170] i2c_hid_of 2-002c: supply vdd not found, using dummy regulator
<4>[    0.278217] i2c_hid_of 0-0040: supply vddl not found, using dummy regulator
<4>[    0.278241] i2c_hid_of 2-002c: supply vddl not found, using dummy regulator
<6>[    0.278375] spi_master spi2: will run message pump with realtime priority
<6>[    0.282512] GACT probability NOT on
<6>[    0.282697] xt_time: kernel timezone is -0000
<6>[    0.282895] Initializing XFRM netlink socket
<6>[    0.283071] NET: Registered protocol family 10
<6>[    0.283493] Segment Routing with IPv6
<6>[    0.283614] NET: Registered protocol family 17
<6>[    0.283686] NET: Registered protocol family 15
<6>[    0.283768] NET: Registered protocol family 40
<6>[    0.284022] registered taskstats version 1
<5>[    0.284029] Loading compiled-in X.509 certificates
<5>[    0.284113] Key type .fscrypt registered
<5>[    0.284118] Key type fscrypt-provisioning registered
<6>[    0.284311] pstore: Using crash dump compression: deflate
<5>[    0.284946] Key type encrypted registered
<7>[    0.294333] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.294339] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.294357] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.294369] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.294371] gpio-496 (enable): no flags found for enable
<7>[    0.297764] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.297770] panel-edp panel: using device tree for GPIO lookup
<7>[    0.297778] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.297783] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.297788] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.297791] panel-edp panel: No GPIO consumer hpd found
<7>[    0.297894] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.297896] panel-edp panel: using device tree for GPIO lookup
<7>[    0.297901] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.297906] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.297909] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.297910] panel-edp panel: No GPIO consumer enable found
<6>[    0.298215] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.298227] mali 13040000.mali: IRQ JOB not found
<3>[    0.298241] mali 13040000.mali: IRQ MMU not found
<3>[    0.298250] mali 13040000.mali: IRQ GPU not found
<6>[    0.298268] mali 13040000.mali: GPU metrics tracepoint support enabled
<7>[    0.300960] pwm-backlight backlight_lcd0: GPIO lookup for consumer enable
<7>[    0.300967] pwm-backlight backlight_lcd0: using device tree for GPIO lookup
<7>[    0.300980] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/backlight_lcd0[0]' - status (0)
<7>[    0.300992] gpio gpiochip0: Persistence not supported for GPIO 176
<7>[    0.300994] gpio-496 (enable): no flags found for enable
<6>[    0.302150] mtk-iommu 10205000.iommu: bound 14017000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302162] mtk-iommu 10205000.iommu: bound 16010000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302167] mtk-iommu 10205000.iommu: bound 1502f000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302172] mtk-iommu 10205000.iommu: bound 1a002000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302177] mtk-iommu 10205000.iommu: bound 17010000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302182] mtk-iommu 10205000.iommu: bound 15021000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302187] mtk-iommu 10205000.iommu: bound 1a001000.larb (ops 0xffffffdb8cac6448)
<6>[    0.302297] mediatek-disp-ovl 14008000.ovl: Adding to iommu group 0
<6>[    0.302808] mediatek-disp-ovl 14009000.ovl: Adding to iommu group 0
<6>[    0.302996] mediatek-disp-ovl 1400a000.ovl: Adding to iommu group 0
<6>[    0.303176] mediatek-disp-rdma 1400b000.rdma: Adding to iommu group 0
<6>[    0.303465] mediatek-disp-rdma 1400c000.rdma: Adding to iommu group 0
<7>[    0.304218] panel-edp panel: GPIO lookup for consumer hpd
<7>[    0.304221] panel-edp panel: using device tree for GPIO lookup
<7>[    0.304230] of_get_named_gpiod_flags: can't parse 'hpd-gpios' property of node '/panel[0]'
<7>[    0.304235] of_get_named_gpiod_flags: can't parse 'hpd-gpio' property of node '/panel[0]'
<7>[    0.304240] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.304243] panel-edp panel: No GPIO consumer hpd found
<7>[    0.304301] panel-edp panel: GPIO lookup for consumer enable
<7>[    0.304303] panel-edp panel: using device tree for GPIO lookup
<7>[    0.304308] of_get_named_gpiod_flags: can't parse 'enable-gpios' property of node '/panel[0]'
<7>[    0.304312] of_get_named_gpiod_flags: can't parse 'enable-gpio' property of node '/panel[0]'
<7>[    0.304315] panel-edp panel: using lookup tables for GPIO lookup
<7>[    0.304317] panel-edp panel: No GPIO consumer enable found
<7>[    0.304575] anx7625 4-0058: GPIO lookup for consumer enable
<7>[    0.304577] anx7625 4-0058: using device tree for GPIO lookup
<7>[    0.304588] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/soc/i2c@11008000/anx7625@58[0]' - status (0)
<7>[    0.304599] gpio gpiochip0: Persistence not supported for GPIO 45
<7>[    0.304606] anx7625 4-0058: GPIO lookup for consumer reset
<7>[    0.304608] anx7625 4-0058: using device tree for GPIO lookup
<7>[    0.304615] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@11008000/anx7625@58[0]' - status (0)
<7>[    0.304620] gpio gpiochip0: Persistence not supported for GPIO 73
<6>[    0.305579] mali 13040000.mali: Kernel DDK version r44p1-01eac0
<3>[    0.305597] mali 13040000.mali: IRQ JOB not found
<3>[    0.305643] mali 13040000.mali: IRQ MMU not found
<3>[    0.305662] mali 13040000.mali: IRQ GPU not found
<6>[    0.305697] mali 13040000.mali: GPU metrics tracepoint support enabled
<6>[    0.308545] mali 13040000.mali: GPU identified as 0x1 arch 6.2.2 r0p3 status 0
<6>[    0.309089] mali 13040000.mali: No priority control manager is configured
<7>[    0.309200] of_get_named_gpiod_flags: parsed 'gpios' property of node '/wifi-wakeup/wowlan[0]' - status (0)
<7>[    0.309213] gpio gpiochip0: Persistence not supported for GPIO 113
<6>[    0.309267] mali 13040000.mali: No memory group manager is configured
<6>[    0.309308] input: wifi-wakeup as /devices/platform/wifi-wakeup/input/input0
<4>[    0.309735] cros-ec-pchg cros-ec-pchg.15.auto: Unable to get number or ports (err:-95)
<6>[    0.309742] cros-ec-pchg cros-ec-pchg.15.auto: No peripheral charge ports (err:-95)
<6>[    0.310565] mali 13040000.mali: Using configured power model mali-g72-power-model, and fallback mali-simple-power-model
<6>[    0.310590] mali 13040000.mali: No volt-bin detected, using default OPP table
<7>[    0.310609] of_get_named_gpiod_flags: parsed 'gpios' property of node '/volume-buttons/volume_down[0]' - status (0)
<6>[    0.310614] mali 13040000.mali: OPP 0 : opp_freq=300000000 core_mask=f
<6>[    0.310637] mali 13040000.mali: OPP 1 : opp_freq=320000000 core_mask=f
<7>[    0.310639] gpio gpiochip0: Persistence not supported for GPIO 6
<6>[    0.310649] mali 13040000.mali: OPP 2 : opp_freq=340000000 core_mask=f
<6>[    0.310659] mali 13040000.mali: OPP 3 : opp_freq=360000000 core_mask=f
<6>[    0.310668] mali 13040000.mali: OPP 4 : opp_freq=380000000 core_mask=f
<6>[    0.310675] mali 13040000.mali: OPP 5 : opp_freq=400000000 core_mask=f
<6>[    0.310683] mali 13040000.mali: OPP 6 : opp_freq=420000000 core_mask=f
<7>[    0.310687] of_get_named_gpiod_flags: parsed 'gpios' property of node '/volume-buttons/volume_up[0]' - status (0)
<7>[    0.310692] gpio gpiochip0: Persistence not supported for GPIO 5
<6>[    0.310695] mali 13040000.mali: OPP 7 : opp_freq=460000000 core_mask=f
<6>[    0.310700] mali 13040000.mali: OPP 8 : opp_freq=500000000 core_mask=f
<6>[    0.310705] mali 13040000.mali: OPP 9 : opp_freq=540000000 core_mask=f
<6>[    0.310713] mali 13040000.mali: OPP 10 : opp_freq=580000000 core_mask=f
<6>[    0.310720] mali 13040000.mali: OPP 11 : opp_freq=620000000 core_mask=f
<6>[    0.310727] mali 13040000.mali: OPP 12 : opp_freq=653000000 core_mask=f
<6>[    0.310735] mali 13040000.mali: OPP 13 : opp_freq=698000000 core_mask=f
<6>[    0.310741] mali 13040000.mali: OPP 14 : opp_freq=743000000 core_mask=f
<6>[    0.310748] mali 13040000.mali: OPP 15 : opp_freq=800000000 core_mask=f
<6>[    0.310815] input: volume-buttons as /devices/platform/volume-buttons/input/input1
<6>[    0.311036] device-mapper: init: waiting for all devices to be available before creating mapped devices
<7>[    0.311196] sbs-battery 12-000b: GPIO lookup for consumer sbs,battery-detect
<7>[    0.311200] sbs-battery 12-000b: using device tree for GPIO lookup
<7>[    0.311212] of_get_named_gpiod_flags: can't parse 'sbs,battery-detect-gpios' property of node '/soc/spi@11012000/cros-ec@0/i2c-tunnel/sbs-battery@b[0]'
<7>[    0.311222] of_get_named_gpiod_flags: can't parse 'sbs,battery-detect-gpio' property of node '/soc/spi@11012000/cros-ec@0/i2c-tunnel/sbs-battery@b[0]'
<7>[    0.311228] sbs-battery 12-000b: using lookup tables for GPIO lookup
<7>[    0.311232] sbs-battery 12-000b: No GPIO consumer sbs,battery-detect found
<6>[    0.311403] mali 13040000.mali: Probed as mali0
<6>[    0.311890] mtk-svs 1100b000.svs: M_HW_RES0: 0x00120090
<6>[    0.311896] mtk-svs 1100b000.svs: M_HW_RES1: 0xe7fcbb1b
<6>[    0.311900] mtk-svs 1100b000.svs: M_HW_RES2: 0x478b47c7
<6>[    0.311904] mtk-svs 1100b000.svs: M_HW_RES3: 0xabfbf757
<6>[    0.311907] mtk-svs 1100b000.svs: M_HW_RES4: 0xe6fca5ed
<6>[    0.311910] mtk-svs 1100b000.svs: M_HW_RES5: 0x47bb4bc0
<6>[    0.311914] mtk-svs 1100b000.svs: M_HW_RES6: 0xe6fcc7e6
<6>[    0.311917] mtk-svs 1100b000.svs: M_HW_RES7: 0xe7fc980f
<6>[    0.311921] mtk-svs 1100b000.svs: M_HW_RES8: 0x4bbb4bef
<6>[    0.311924] mtk-svs 1100b000.svs: M_HW_RES9: 0xabfb366c
<6>[    0.311927] mtk-svs 1100b000.svs: M_HW_RES14: 0x9e862dbb
<6>[    0.311931] mtk-svs 1100b000.svs: M_HW_RES15: 0x015a0010
<6>[    0.311934] mtk-svs 1100b000.svs: M_HW_RES16: 0xe7fc8e1c
<6>[    0.311937] mtk-svs 1100b000.svs: M_HW_RES17: 0x47bb47ef
<6>[    0.311941] mtk-svs 1100b000.svs: M_HW_RES18: 0xabfbc84d
<4>[    0.313432] thermal thermal_zone9: power_allocator: sustainable_power will be estimated
<6>[    0.313635] sbs-battery 12-000b: sbs-battery: battery gas gauge device registered
<4>[    0.314099] devfreq 13040000.mali: Couldn't update frequency transition information.
<6>[    0.314829]  SVSB_CPU_LITTLE: svs_init01_isr_handler: VDN74~30:0x141c242b~0x2f33373d, DC:0x031701cf
<6>[    0.315095]  SVSB_CPU_BIG: svs_init01_isr_handler: VDN74~30:0x151e262d~0x32373c41, DC:0x031a016a
<6>[    0.315355]  SVSB_CCI: svs_init01_isr_handler: VDN74~30:0x13192229~0x2d32383d, DC:0x031afed0
<6>[    0.315615]  SVSB_GPU: svs_init01_isr_handler: VDN74~30:0x1416181a~0x1d202428, DC:0x0320ff00
<6>[    0.318089]  SVSB_CPU_LITTLE: svs_init02_isr_handler: VOP74~30:0x1b232b32~0x363a3e44, DC:0x03170000
<6>[    0.318286]  SVSB_CPU_BIG: svs_init02_isr_handler: VOP74~30:0x1c252d34~0x393e4348, DC:0x031a0000
<6>[    0.318355]  SVSB_CCI: svs_init02_isr_handler: VOP74~30:0x1d232b32~0x373b4246, DC:0x031a0130
<6>[    0.318486]  SVSB_GPU: svs_init02_isr_handler: VOP74~30:0x181a1c1e~0x2124282c, DC:0x03200100
<7>[    0.320019] it6505 3-005c: GPIO lookup for consumer reset
<7>[    0.320024] it6505 3-005c: using device tree for GPIO lookup
<7>[    0.320045] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@1100f000/it6505dptx@5c[0]' - status (0)
<7>[    0.320061] gpio gpiochip0: Persistence not supported for GPIO 179
<6>[    0.321174] mediatek-dpi 14015000.dpi: Found bridge node: /soc/i2c@1100f000/it6505dptx@5c
<6>[    0.321767] mediatek-drm mediatek-drm.3.auto: bound 14008000.ovl (ops 0xffffffdb8ca58738)
<6>[    0.321777] mediatek-drm mediatek-drm.3.auto: bound 14009000.ovl (ops 0xffffffdb8ca58738)
<6>[    0.321785] mediatek-drm mediatek-drm.3.auto: bound 1400a000.ovl (ops 0xffffffdb8ca58738)
<6>[    0.321793] mediatek-drm mediatek-drm.3.auto: bound 1400b000.rdma (ops 0xffffffdb8ca590f8)
<6>[    0.321801] mediatek-drm mediatek-drm.3.auto: bound 1400c000.rdma (ops 0xffffffdb8ca590f8)
<6>[    0.321808] mediatek-drm mediatek-drm.3.auto: bound 1400e000.color (ops 0xffffffdb8ca57bf0)
<6>[    0.321816] mediatek-drm mediatek-drm.3.auto: bound 1400f000.ccorr (ops 0xffffffdb8ca578b8)
<6>[    0.321823] mediatek-drm mediatek-drm.3.auto: bound 14010000.aal (ops 0xffffffdb8ca57648)
<6>[    0.321831] mediatek-drm mediatek-drm.3.auto: bound 14011000.gamma (ops 0xffffffdb8ca57f30)
<6>[    0.321849] input: cros_ec as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input2
<6>[    0.323068] mediatek-drm mediatek-drm.3.auto: bound 14014000.dsi (ops 0xffffffdb8ca5e8c0)
<6>[    0.323277] mediatek-drm mediatek-drm.3.auto: bound 14015000.dpi (ops 0xffffffdb8ca5e2f0)
<6>[    0.324023] [drm] Initialized mediatek 1.0.0 20150513 for mediatek-drm.3.auto on minor 0
<6>[    0.326877] tpm_tis_spi spi0.0: Cr50 firmware version: B2-C:0 RO_A:0.0.13/b9f09fb5 RW_A:0.5.271/cr50_v4.11_mp.81-08ba0d
<6>[    0.327235] input: cros_ec_buttons as /devices/platform/soc/11012000.spi/spi_master/spi2/spi2.0/11012000.spi:cros-ec@0:keyboard-controller/input/input3
<6>[    0.337683] cros-ec-spi spi2.0: Chrome EC device registered
<4>[    0.343546] sbs-battery 12-000b: I2C adapter does not support I2C_FUNC_SMBUS_READ_BLOCK_DATA.
                  Fallback method does not support PEC.
<4>[    0.343959] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
<4>[    0.351262] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
<4>[    0.354436] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
<4>[    0.355072] mmc1: queuing unknown CIS tuple 0x14 (0 bytes)
<6>[    0.357740] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
<6>[    0.358779] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
<4>[    0.359613] mmc1: queuing unknown CIS tuple 0x80 (1 bytes)
<4>[    0.359669] mmc1: queuing unknown CIS tuple 0x81 (1 bytes)
<4>[    0.359717] mmc1: queuing unknown CIS tuple 0x82 (1 bytes)
<6>[    0.359746] mmc1: new ultra high speed SDR104 SDIO card at address 0001
<6>[    0.371119] mtk-msdc 11230000.mmc: phase: [map:ffffff3f] [maxlen:24] [final:20]
<6>[    0.373512] mmc0: new HS400 MMC card at address 0001
<6>[    0.375139] mmcblk0: mmc0:0001 DA4032 29.1 GiB 
<6>[    0.376405] mmcblk0boot0: mmc0:0001 DA4032 partition 1 4.00 MiB
<6>[    0.377668] mmcblk0boot1: mmc0:0001 DA4032 partition 2 4.00 MiB
<6>[    0.377836] mmcblk0rpmb: mmc0:0001 DA4032 partition 3 16.0 MiB, chardev (241:0)
<6>[    0.383338]  mmcblk0: p1 p2 p3 p4 p5 p6 p7 p8 p9 p10 p11 p12
<6>[    0.408699] input: hid-over-i2c 06CB:CDB5 Mouse as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input4
<6>[    0.409167] hid-generic 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
<6>[    0.410184] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    0.410545] device-mapper: ioctl: dm-0 (vroot) is ready
<6>[    0.410791] clk: Disabling unused clocks
<6>[    0.411230] ALSA device list:
<6>[    0.411238]   No soundcards found.
<3>[    0.411286] Warning: unable to open an initial console. Fallback to ttynull.
<6>[    0.411300] printk: console [ttynull0] enabled
<6>[    0.421786] EXT4-fs (dm-0): mounting ext2 file system using the ext4 subsystem
<6>[    0.429065] EXT4-fs (dm-0): mounted filesystem without journal. Opts: (null)
<6>[    0.429127] VFS: Mounted root (ext2 filesystem) readonly on device 254:0.
<6>[    0.437399] devtmpfs: mounted
<6>[    0.440210] Freeing unused kernel memory: 1408K
<6>[    0.440297] Run /sbin/init as init process
<7>[    0.440303]   with arguments:
<7>[    0.440306]     /sbin/init
<7>[    0.440309]     cros_secure
<7>[    0.440312]   with environment:
<7>[    0.440315]     HOME=/
<7>[    0.440317]     TERM=linux
<7>[    0.440322]     dm=1 vroot none ro 1,0 5324800 verity payload=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashtree=PARTUUID=873d93f3-0066-4720-87c3-b0fe6a96eb51/PARTNROFF=1 hashstart=5324800 alg=sha256 root_hexdigest=43f07fb59275b335def5ac5b86c6a4689536c493c956e5f815a7e48ac59b123e salt=f3c76eeb034d7b17b9e53bb155d407f4b29e30be1a454a7d9b090465ea770583
<7>[    0.440325]     cros_lsb_release_hash=GBY2Gkxw5ezHBA6Lqkv65ZuwTBQC0kBWObNli64/5o4=
<5>[    0.538864] audit: type=1404 audit(1740770410.773:2): enforcing=1 old_enforcing=0 auid=4294967295 ses=4294967295 enabled=1 old-enabled=1 lsm=selinux res=1
<6>[    0.608728] SELinux:  Permission bpf in class capability2 not defined in policy.
<6>[    0.608752] SELinux:  Permission checkpoint_restore in class capability2 not defined in policy.
<6>[    0.608783] SELinux:  Permission bpf in class cap2_userns not defined in policy.
<6>[    0.608790] SELinux:  Permission checkpoint_restore in class cap2_userns not defined in policy.
<6>[    0.608951] SELinux: the above unknown classes and permissions will be denied
<6>[    0.617869] SELinux:  policy capability network_peer_controls=1
<6>[    0.617890] SELinux:  policy capability open_perms=1
<6>[    0.617897] SELinux:  policy capability extended_socket_class=1
<6>[    0.617903] SELinux:  policy capability always_check_network=0
<6>[    0.617910] SELinux:  policy capability cgroup_seclabel=0
<6>[    0.617916] SELinux:  policy capability nnp_nosuid_transition=1
<6>[    0.617922] SELinux:  policy capability genfs_seclabel_symlinks=0
<6>[    0.617928] SELinux:  policy capability ioctl_skip_cloexec=0
<6>[    0.657671] usb 1-1: new high-speed USB device number 2 using xhci-mtk
<5>[    0.670814] audit: type=1403 audit(1740770410.904:3): auid=4294967295 ses=4294967295 lsm=selinux res=1
<6>[    0.785772] usb 1-1: New USB device found, idVendor=05e3, idProduct=0608, bcdDevice=60.90
<6>[    0.785790] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
<6>[    0.785798] usb 1-1: Product: USB2.0 Hub
<6>[    0.787282] hub 1-1:1.0: USB hub found
<6>[    0.787672] hub 1-1:1.0: 3 ports detected
<5>[    0.974941] audit: type=1400 audit(1740770411.209:4): avc:  granted  { execute } for  pid=342 comm="sh" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:cros_init_scripts:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
<6>[    1.064655] usb 1-1.3: new high-speed USB device number 3 using xhci-mtk
<6>[    1.151668] usb 1-1.3: New USB device found, idVendor=0408, idProduct=a064, bcdDevice= 0.04
<6>[    1.151687] usb 1-1.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
<6>[    1.151694] usb 1-1.3: Product: HD User Facing
<6>[    1.151700] usb 1-1.3: Manufacturer: Quanta
<7>[    1.198022] udevd[357]: Starting version 249
<6>[    1.359099] EXT4-fs (mmcblk0p1): mounted filesystem with ordered data mode. Opts: commit=600,discard
<6>[    1.362778] EXT4-fs (mmcblk0p8): mounted filesystem with ordered data mode. Opts: 
<6>[    1.403385] LoadPin: dm-0 (254:0): read-only
<6>[    1.403407] LoadPin: load pinning engaged.
<5>[    1.403440] LoadPin: kernel-module pinned obj="/lib/modules/5.10.230-25844-gdc65f732bf53/kernel/drivers/input/serio/serio.ko.gz" pid=380 cmdline="udevd --daemon"
<6>[    1.487250] rmi4_f01 rmi4-00.fn01: found RMI device, manufacturer: Synaptics, product: TM3509-001, fw id: 3010219
<6>[    1.496213] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
<5>[    1.511718] INFO chromeos_startup: [tpm.cc(323)] TPM ready
<5>[    1.511890] INFO chromeos_startup: [tpm2.cc(121)] Getting key from TPM2 NVRAM index 8388613
<5>[    1.524010] INFO chromeos_startup: [tpm.cc(440)] Found encstateful NVRAM area.
<5>[    1.540738] INFO chromeos_startup: [encryption_key.cc(181)] Using NVRAM as system key; already populated.
<6>[    1.569055] input: Synaptics TM3509-001 as /devices/platform/soc/11009000.i2c/i2c-2/2-002c/0018:06CB:CDB5.0001/input/input6
<6>[    1.569657] hid-rmi 0018:06CB:CDB5.0001: input,hidraw0: I2C HID v1.00 Mouse [hid-over-i2c 06CB:CDB5] on 2-002c
<5>[    1.631144] INFO chromeos_startup: [tpm_setup.cc(98)] There is no bio_crypto_init binary, so skip sending TPM seed.
<5>[    1.662662] INFO chromeos_startup: [tpm.cc(421)] Version 2 Lockbox NVRAM area found.
<5>[    1.662719] INFO chromeos_startup: [tpm_setup.cc(245)] Lockbox is valid, exporting.
<5>[    1.665343] INFO chromeos_startup: [dmcrypt_container.cc(112)] Setting up backing device
<5>[    1.778435] INFO chromeos_startup: [dmcrypt_container.cc(177)] Waiting for dm-crypt device to appear
<5>[    1.785766] INFO chromeos_startup: [dmcrypt_container.cc(143)] Removing provisioned dmcrypt key from kernel keyring.
<5>[    1.806322] INFO chromeos_startup: [encrypted_fs.cc(275)] Mounting /dev/mapper/encstateful onto /mnt/stateful_partition/encrypted
<5>[    1.807108] INFO chromeos_startup: [encrypted_fs.cc(89)] Using vm.dirty_expire_centisecs/100 as the commit interval
<6>[    1.813967] EXT4-fs (dm-1): mounted filesystem with ordered data mode. Opts: discard,commit=600
<5>[    1.814146] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/var onto /var
<5>[    1.820135] INFO chromeos_startup: [encrypted_fs.cc(300)] Bind mounting /mnt/stateful_partition/encrypted/chronos onto /home/chronos
<6>[    1.912056] fscrypt: AES-256-CTS-CBC using implementation "cts-cbc-aes-ce"
<5>[    1.927037] audit: type=1400 audit(1740770412.161:5): avc:  granted  { execute } for  pid=598 comm="chromeos_startu" name="crash_reporter" dev="dm-0" ino=14092 scontext=u:r:chromeos_startup:s0 tcontext=u:object_r:cros_crash_reporter_exec:s0 tclass=file
<5>[    1.933614] WARNING chromeos_startup: [stateful_mount.cc(470)] Failed to read from /mnt/stateful_partition/.update_available: No such file or directory (2)
<6>[    1.933882] EXT4-fs (mmcblk0p1): re-mounted. Opts: 
<7>[    2.042548] frecon[588]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<5>[    2.234762] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/var)
<5>[    2.434231] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/user)
<5>[    2.435267] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/root)
<5>[    2.436299] INFO chromeos_startup: [utils.cc(41)] restorecon: Skipping restorecon on directory(/home/chronos)
<5>[    2.518511] audit: type=1400 audit(1740770412.752:6): avc:  denied  { search } for  pid=630 comm="rsyslogd" name="hosts.d" dev="dm-0" ino=23817 scontext=u:r:cros_rsyslogd:s0 tcontext=u:object_r:cros_run_crosdns:s0 tclass=dir permissive=0
<7>[    2.670274] frecon[588]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<7>[    2.701481] frecon[588]: Frecon using drm driver mediatek, version 1.0, date(20150513), desc(Mediatek SoC DRM)
<5>[    3.148455] init: bluetoothd pre-start process (756) terminated with status 1
<7>[    3.166682] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    3.166698] gpio gpiochip0: registered chardev handle for line 150
<7>[    3.166732] gpio gpiochip0: registered chardev handle for 1 lines
<3>[    3.213501] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213537] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213550] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213824] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213837] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213848] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213862] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213875] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213886] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213962] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<3>[    3.213975] OF: graph: no port node found in /soc/spi@11012000/cros-ec@0/typec/connector@0
<6>[    3.783826] ath10k_sdio mmc1:0001:1: qca6174 hw3.2 sdio target 0x05030000 chip_id 0x00000000 sub 0000:0000
<6>[    3.783848] ath10k_sdio mmc1:0001:1: kconfig debug 1 debugfs 1 tracing 1 dfs 0 testmode 1
<6>[    3.784052] ath10k_sdio mmc1:0001:1: firmware ver WLAN.RMH.4.4.1-00189 api 6 features wowlan,ignore-otp,mfp crc32 595e0108
<6>[    3.826792] Bluetooth: bt_init() Core ver 2.22
<6>[    3.827025] NET: Registered protocol family 31
<6>[    3.827035] Bluetooth: bt_init() HCI device and connection manager initialized
<6>[    3.827056] Bluetooth: hci_sock_init() HCI socket layer initialized
<6>[    3.827068] Bluetooth: l2cap_init_sockets() L2CAP socket layer initialized
<6>[    3.827103] Bluetooth: sco_init() SCO socket layer initialized
<6>[    3.940283] ath10k_sdio mmc1:0001:1: board_file api 2 bmi_id 0:4 crc32 e57aadc7
<6>[    4.275106] ath10k_sdio mmc1:0001:1: htt-ver 3.87 wmi-op 4 htt-op 3 cal otp max-sta 32 raw 0 hwcrypto 1
<4>[    4.344066] mmc1: queuing unknown CIS tuple 0x01 (3 bytes)
<4>[    4.351482] mmc1: queuing unknown CIS tuple 0x1a (5 bytes)
<4>[    4.355318] mmc1: queuing unknown CIS tuple 0x1b (8 bytes)
<6>[    4.358867] mtk-msdc 11240000.mmc: phase: [map:ff00003f] [maxlen:8] [final:28]
<6>[    4.360103] mtk-msdc 11240000.mmc: phase: [map:ffffffff] [maxlen:32] [final:10]
<7>[    4.360270] ath: EEPROM regdomain: 0x6c
<7>[    4.360273] ath: EEPROM indicates we should expect a direct regpair map
<7>[    4.360282] ath: Country alpha2 being used: 00
<7>[    4.360284] ath: Regpair used: 0x6c
<7>[    4.374757] udevd[391]: Using default interface naming scheme 'v249'.
<7>[    4.642725] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    4.642742] gpio gpiochip0: registered chardev handle for line 150
<7>[    4.642757] gpio gpiochip0: registered chardev handle for 1 lines
<7>[    4.904861] ath: EEPROM regdomain: 0x8348
<7>[    4.904872] ath: EEPROM indicates we should expect a country code
<7>[    4.904877] ath: doing EEPROM country->regdmn map search
<7>[    4.904881] ath: country maps to regdmn code: 0x3a
<7>[    4.904885] ath: Country alpha2 being used: US
<7>[    4.904888] ath: Regpair used: 0x3a
<7>[    4.904901] ath: regdomain 0x8348 dynamically updated by user
<5>[    5.638097] init: failsafe-delay main process (740) killed by TERM signal
<5>[    5.678790] init: secagentd post-start process (1651) terminated with status 2
<7>[    6.252569] max98357a max98357a: GPIO lookup for consumer sdmode
<7>[    6.252584] max98357a max98357a: using device tree for GPIO lookup
<7>[    6.252620] of_get_named_gpiod_flags: parsed 'sdmode-gpios' property of node '/max98357a[0]' - status (0)
<7>[    6.252692] gpio gpiochip0: Persistence not supported for GPIO 175
<6>[    6.257466] mt6358-sound mt6358-sound: mt6358_platform_driver_probe(), dev name mt6358-sound
<6>[    6.437488] fuse: init (API version 7.32)
<4>[    6.478563] elants_i2c 0-0010: supply vcc33 not found, using dummy regulator
<4>[    6.478930] elants_i2c 0-0010: supply vccio not found, using dummy regulator
<7>[    6.479017] elants_i2c 0-0010: GPIO lookup for consumer reset
<7>[    6.479020] elants_i2c 0-0010: using device tree for GPIO lookup
<7>[    6.479050] of_get_named_gpiod_flags: parsed 'reset-gpios' property of node '/soc/i2c@11007000/touchscreen@10[0]' - status (0)
<7>[    6.479073] gpio gpiochip0: Persistence not supported for GPIO 156
<3>[    6.500841] elants_i2c 0-0010: nothing at this address
<6>[    6.532367] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<4>[    6.545320] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: No cache defaults, reading back from HW
<6>[    6.546383] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mtk_afe_combine_sub_dai(), num of dai 20
<6>[    6.548967] mt8183_mt6358_ts3a227 mt8183-sound: mt8183_mt6358_ts3a227_max98357_dev_probe Can't find pin state wov -19
<3>[    6.550568] debugfs: Directory '11220000.audio-controller:mt8183-afe-pcm' with parent 'mt8183_mt6358_ts3a227_max98357' already present!
<4>[    6.577360] hdmi-audio-codec hdmi-audio-codec.17.auto: ASoC: sink widget TX overwritten
<6>[    6.577404] Bluetooth: hci_uart_init() HCI UART driver ver 2.3
<6>[    6.577420] Bluetooth: hci_uart_register_proto() HCI UART protocol H4 registered
<6>[    6.577495] Bluetooth: hci_uart_register_proto() HCI UART protocol Three-wire (H5) registered
<6>[    6.577538] Bluetooth: hci_uart_register_proto() HCI UART protocol QCA registered
<7>[    6.582512] hci_uart_qca serial0-0: GPIO lookup for consumer enable
<7>[    6.582526] hci_uart_qca serial0-0: using device tree for GPIO lookup
<7>[    6.582568] of_get_named_gpiod_flags: parsed 'enable-gpios' property of node '/soc/serial@11003000/bluetooth[0]' - status (0)
<7>[    6.582592] gpio gpiochip0: Persistence not supported for GPIO 120
<6>[    6.583461] Bluetooth: qca_setup() hci0: setting up ROME/QCA6390
<3>[    6.615856] mtk-scp 10500000.scp: invalid resource
<6>[    6.615944] mtk-scp 10500000.scp: assigned reserved memory node memory@50000000
<3>[    6.619679] debugfs: File 'Playback' in directory 'dapm' already present!
<3>[    6.619715] debugfs: File 'Capture' in directory 'dapm' already present!
<6>[    6.627441] input: mt8183_mt6358_ts3a227_max98357 Headset Jack as /devices/platform/mt8183-sound/sound/card0/input7
<6>[    6.628490] input: mt8183_mt6358_ts3a227_max98357 HDMI Jack as /devices/platform/mt8183-sound/sound/card0/input8
<6>[    6.637163] remoteproc remoteproc0: scp is available
<6>[    6.775085] remoteproc remoteproc0: powering up scp
<6>[    6.775121] remoteproc remoteproc0: Booting fw image mediatek/mt8183/scp_legacy.img, size 1032064
<6>[    6.775147] mtk-scp 10500000.scp: IPI buf addr 0x0007bdb0
<3>[    6.797259] Bluetooth: qca_recv() hci0: Frame reassembly failed (-84)
<6>[    6.808206] mtk-mdp3 14001000.mdp3_rdma0: Adding to iommu group 0
<3>[    6.808289] mtk-mdp3 14001000.mdp3_rdma0: can't get node mediatek,mmsys2
<3>[    6.808296] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mmsys2
<3>[    6.808329] mtk-mdp3 14001000.mdp3_rdma0: Failed to get mdp mm-mutex2
<6>[    6.808736] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:3 alias:0 id:11 base:0x14001000 regs:00000000679216e2
<6>[    6.808793] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:23 alias:0 id:9 base:0x14000000 regs:0000000019fe76a6
<6>[    6.808838] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:24 alias:1 id:10 base:0x14000000 regs:0000000024246d4a
<6>[    6.808876] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:7 alias:0 id:18 base:0x14005000 regs:00000000dbd222ac
<6>[    6.808909] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:8 alias:1 id:19 base:0x14006000 regs:0000000074387a53
<6>[    6.808942] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:1 alias:0 id:4 base:0x15020000 regs:0000000062697b80
<6>[    6.808985] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:22 alias:1 id:6 base:0x15020000 regs:000000004509d63b
<6>[    6.809037] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:0 id:14 base:0x14003000 regs:0000000053331eaa
<6>[    6.809082] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:4 alias:1 id:15 base:0x14004000 regs:00000000938d46f4
<6>[    6.809125] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:5 alias:0 id:20 base:0x14005000 regs:000000007ffd1497
<6>[    6.809171] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:6 alias:0 id:21 base:0x14006000 regs:000000008fa0654c
<6>[    6.809293] mtk-mdp3 14001000.mdp3_rdma0: mdp3_rdma0 type:18 alias:0 id:13 base:0x1401c000 regs:000000006d4317de
<3>[    6.809430] mdp_debug_init:start
<3>[    6.809607] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-tdshp0
<3>[    6.809616] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-color0
<3>[    6.809622] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mdp3-aal0
<3>[    6.809723] [MTK-MDP3][ERR] mdp_alloc_reference_VA_by_name:80: DEV: cannot parse node name:mediatek,larb
<3>[    6.809738] mdp_debug_init:end
<7>[    6.813907] udevd[415]: Using default interface naming scheme 'v249'.
<6>[    6.816609] mtk-mdp3 14001000.mdp3_rdma0: Driver registered as /dev/video2
<6>[    6.889508] mtk-jpeg 17030000.venc_jpg: Adding to iommu group 0
<6>[    6.890334] mtk-jpeg 17030000.venc_jpg: mtk-jpeg-enc device registered as /dev/video0 (81,1)
<6>[    6.908353] mtk-cam-p1 1a000000.camisp: Adding to iommu group 0
<6>[    6.910189] mtk-cam-p1 1a000000.camisp: Registered media0
<6>[    6.910215] mtk-cam-p1 1a000000.camisp: Registered mtk-cam-p1 1a000000.camisp
<6>[    6.917966] mtk-vcodec-enc 17020000.vcodec: Adding to iommu group 0
<6>[    6.944752] mtk-fd-4.0 1502b000.fd: Adding to iommu group 0
<6>[    6.945657] mtk-fd-4.0 1502b000.fd: scp addr:0x0000000050a00000 va:ffffffc018a00000
<6>[    6.945731] mtk-fd-4.0 1502b000.fd: scp iova addr:0x00000000fdb00000
<6>[    6.958467] mtk-cam-dip 15022000.dip: Adding to iommu group 0
<6>[    6.963761] mtk-scp 10500000.scp: creating channel cros-ec-rpmsg addr 0xd
<6>[    6.963768] mtk-scp 10500000.scp: SCP is ready. FW version kukui_scp_v2.0.2796-7246101293
<6>[    6.963779] remoteproc remoteproc0: remote processor scp is now up
<6>[    7.073563] mtk-vcodec-dec 16000000.vcodec: Adding to iommu group 0
<6>[    7.097703] Bluetooth: qca_read_soc_version() hci0: QCA Product ID   :0x00000008
<6>[    7.097724] Bluetooth: qca_read_soc_version() hci0: QCA SOC Version  :0x00000044
<6>[    7.097730] Bluetooth: qca_read_soc_version() hci0: QCA ROM Version  :0x00000302
<6>[    7.097736] Bluetooth: qca_read_soc_version() hci0: QCA Patch Version:0x00000111
<6>[    7.097745] Bluetooth: qca_uart_setup() hci0: QCA controller version 0x00440302
<6>[    7.097754] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/rampatch_00440302.bin
<6>[    7.433694] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[    7.433717] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[    7.433724] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[    7.433730] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<4>[    7.444211] memfd_create() without MFD_EXEC nor MFD_NOEXEC_SEAL, pid=2604 'patchpaneld'
<6>[    7.647083] cros-ec-dev cros-ec-dev.18.auto: CrOS System Control Processor MCU detected
<4>[    7.673793] cros-ec-pchg cros-ec-pchg.25.auto: Unable to get number or ports (err:-95)
<6>[    7.673820] cros-ec-pchg cros-ec-pchg.25.auto: No peripheral charge ports (err:-95)
<6>[    7.690346] cros-ec-rpmsg 10500000.scp.cros-ec-rpmsg.13.-1: Chrome EC device registered
<6>[    7.728690] Bluetooth: qca_download_firmware() hci0: QCA Downloading qca/nvm_00440302_i2s.bin
<6>[    7.818440] Bluetooth: qca_uart_setup() hci0: QCA setup on UART is completed
<7>[    8.027098] usb 1-1.3: GPIO lookup for consumer privacy
<7>[    8.027115] usb 1-1.3: using lookup tables for GPIO lookup
<7>[    8.027122] usb 1-1.3: No GPIO consumer privacy found
<6>[    8.027130] usb 1-1.3: Found UVC 1.00 device HD User Facing (0408:a064)
<6>[    8.051499] usbcore: registered new interface driver uvcvideo
<6>[    8.112872] mt8183-audio 11220000.audio-controller:mt8183-afe-pcm: mt8183_adda_dmic_set(), kcontrol name MTKAIF_DMIC, mtkaif_dmic 1
<6>[    8.185567] IPv6: ADDRCONF(NETDEV_CHANGE): arc_ns0: link becomes ready
<6>[    8.185861] IPv6: ADDRCONF(NETDEV_CHANGE): veth0: link becomes ready
<6>[    8.207517] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    8.315210] IPv6: ADDRCONF(NETDEV_CHANGE): veth1: link becomes ready
<7>[    8.569195] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.569207] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.569216] gpio gpiochip0: registered chardev handle for 1 lines
<5>[    8.575296] init: send-boot-elog-metrics main process (3104) terminated with status 1
<6>[    8.613452] wlan0: authenticate with 84:17:ef:e4:dc:b6
<6>[    8.669177] wlan0: send auth to 84:17:ef:e4:dc:b6 (try 1/3)
<6>[    8.671300] wlan0: authenticated
<6>[    8.672917] wlan0: associate with 84:17:ef:e4:dc:b6 (try 1/3)
<6>[    8.676654] wlan0: RX AssocResp from 84:17:ef:e4:dc:b6 (capab=0x1511 status=0 aid=7)
<6>[    8.687157] wlan0: associated
<7>[    8.715495] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.715508] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.715517] gpio gpiochip0: registered chardev handle for 1 lines
<7>[    8.722947] wlan0: Limiting TX power to 30 (30 - 0) dBm as advertised by 84:17:ef:e4:dc:b6
<6>[    8.751500] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[    8.753753] wlan0: dropped frame to 84:17:ef:e4:dc:b6 (unauthorized port)
<6>[    8.760751] wlan0: dropped frame to 84:17:ef:e4:dc:b6 (unauthorized port)
<7>[    8.900065] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[    8.900077] gpio gpiochip0: registered chardev handle for line 150
<7>[    8.900087] gpio gpiochip0: registered chardev handle for 1 lines
<6>[    8.920226] 8021q: 802.1Q VLAN Support v1.8
<6>[    8.923565] device-mapper: verity: sha256 using implementation "sha256-ce"
<6>[    9.047268] zram: Added device: zram0
<6>[    9.131942] zram0: detected capacity change from 0 to 8136663040
<6>[    9.158818] Adding 7945956k swap on /dev/zram0.  Priority:-2 extents:1 across:7945956k SS
<6>[    9.260854] async_tx: api initialized (async)
<6>[    9.266453] xor: measuring software checksum speed
<6>[    9.269790]    8regs           :  3345 MB/sec
<6>[    9.271900]    32regs          :  4784 MB/sec
<6>[    9.274427]    arm64_neon      :  4248 MB/sec
<6>[    9.274443] xor: using function: 32regs (4784 MB/sec)
<6>[    9.508327] zram: setup backing device /dev/mapper/zram-writeback
<3>[    9.552248] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.553091] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.553843] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.554679] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.555525] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.556365] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.557196] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.558027] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.558861] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.559701] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.560546] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.561437] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.562299] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.563150] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.564050] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.564864] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.565700] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.566523] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.567394] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.568228] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.569069] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.569853] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.570673] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.571517] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.572345] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.573172] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.574005] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.574820] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.575634] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.576448] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.577261] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[    9.578096] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.008671] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.009572] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.010619] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.011733] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.012682] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.013534] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.014387] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.015238] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.016100] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.016969] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.017823] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.018678] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.019533] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.020388] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.021241] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.022120] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.023052] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.023990] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.024901] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.025787] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.026675] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.027559] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.028444] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.029327] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.030211] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.031231] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.032184] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.033177] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.034141] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.035091] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.035946] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   15.036835] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<6>[   30.688477] vaux18: disabling
<6>[   30.688611] vio28: disabling
<6>[   38.450680] fscrypt: AES-256-XTS using implementation "xts-aes-ce"
<6>[   59.035986] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.036010] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.036015] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.036019] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.114429] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.114446] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.114450] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.114454] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.166065] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.166087] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.166093] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.166099] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   59.220655] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10
<6>[   59.220672] mtk-mdp3 14001000.mdp3_rdma0: [0] type:10, frame:32x32
<6>[   59.220676] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9
<6>[   59.220681] mtk-mdp3 14001000.mdp3_rdma0: [0] type:9, frame:32x32
<6>[   62.432935] PDLOG 2025/02/28 19:19:50.659 P0 Disconnected
<3>[   67.010218] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.011544] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.012625] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.013709] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.014649] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.015757] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.016965] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.017994] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.019049] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.020061] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.021061] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.022106] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.023108] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.024104] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.025091] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.026094] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.027093] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.028121] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.029168] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.030117] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.031222] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.032343] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.033340] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.034283] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.035210] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.036204] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.037193] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.038183] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.039171] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.040136] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.041117] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   67.042160] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<7>[   68.193346] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[   68.193358] gpio gpiochip0: registered chardev handle for line 150
<7>[   68.193367] gpio gpiochip0: registered chardev handle for 1 lines
<7>[   68.457957] gpio gpiochip0: Persistence not supported for GPIO 150
<7>[   68.457980] gpio gpiochip0: registered chardev handle for line 150
<7>[   68.458000] gpio gpiochip0: registered chardev handle for 1 lines
<3>[   73.011380] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.012310] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.013202] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.014087] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.014915] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.015818] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.016735] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.017622] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.018520] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.019402] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.020285] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.021170] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.022065] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.022931] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.023844] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.025021] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.025990] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.026942] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.027828] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.028743] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.029642] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.030547] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.031431] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.032314] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.033205] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.034089] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.034918] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.035804] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.036688] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.037595] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.038533] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<3>[   73.039427] it6505 3-005c: [drm:it6505_aux_do_transfer] *ERROR* read failed reg[0xd] err: -6
<6>[  111.316035] tun: Universal TUN/TAP device driver, 1.6
<7>[  111.326235] udevd[5027]: Using default interface naming scheme 'v249'.
<7>[  111.332414] udevd[5025]: Using default interface naming scheme 'v249'.
<7>[  111.336510] udevd[5024]: Using default interface naming scheme 'v249'.
<7>[  111.341758] udevd[5035]: Using default interface naming scheme 'v249'.
<7>[  111.343165] udevd[5036]: Using default interface naming scheme 'v249'.
<7>[  111.347613] udevd[5029]: Using default interface naming scheme 'v249'.
<6>[  111.379078] arcbr0: port 1(vmtap0) entered blocking state
<6>[  111.379094] arcbr0: port 1(vmtap0) entered disabled state
<6>[  111.379293] device vmtap0 entered promiscuous mode
<6>[  111.389894] arc_wlan0: port 1(vmtap5) entered blocking state
<6>[  111.389910] arc_wlan0: port 1(vmtap5) entered disabled state
<6>[  111.390163] device vmtap5 entered promiscuous mode
<6>[  111.390277] arc_wlan0: port 1(vmtap5) entered blocking state
<6>[  111.390285] arc_wlan0: port 1(vmtap5) entered forwarding state
<6>[  111.513568] arcbr0: port 1(vmtap0) entered blocking state
<6>[  111.513588] arcbr0: port 1(vmtap0) entered forwarding state
<6>[  111.535099] IPv6: ADDRCONF(NETDEV_CHANGE): veth2: link becomes ready
<6>[  111.587513] EXT4-fs (loop9): Using encoding defined by superblock: utf8-12.1.0 with flags 0x0
<6>[  111.590757] EXT4-fs (loop9): mounted filesystem without journal. Opts: noload
