Wiphy phy0
	wiphy index: 0
	max # scan SSIDs: 16
	max scan IEs length: 195 bytes
	max # sched scan SSIDs: 16
	max # match sets: 16
	Retry short limit: 7
	Retry long limit: 4
	Coverage class: 0 (up to 0m)
	Device supports RSN-IBSS.
	Device supports AP-side u-APSD.
	Supported Ciphers:
		* WEP40 (00-0f-ac:1)
		* WEP104 (00-0f-ac:5)
		* TKIP (00-0f-ac:2)
		* CCMP-128 (00-0f-ac:4)
		* CMAC (00-0f-ac:6)
		* CMAC-256 (00-0f-ac:13)
		* GMAC-128 (00-0f-ac:11)
		* GMAC-256 (00-0f-ac:12)
	Available Antennas: TX 0x3 RX 0x3
	Configured Antennas: TX 0x3 RX 0x3
	Supported interface modes:
		 * IBSS
		 * managed
		 * AP
		 * monitor
		 * P2P-client
		 * P2P-GO
		 * P2P-device
	Band 1:
		Capabilities: 0x19ef
			RX LDPC
			HT20/HT40
			SM Power Save disabled
			RX HT20 SGI
			RX HT40 SGI
			TX STBC
			RX STBC 1-stream
			Max AMSDU length: 7935 bytes
			DSSS/CCK HT40
		Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
		Minimum RX AMPDU time spacing: 8 usec (0x06)
		HT TX/RX MCS rate indexes supported: 0-15
		Bitrates (non-HT):
			* 1.0 Mbps
			* 2.0 Mbps (short preamble supported)
			* 5.5 Mbps (short preamble supported)
			* 11.0 Mbps (short preamble supported)
			* 6.0 Mbps
			* 9.0 Mbps
			* 12.0 Mbps
			* 18.0 Mbps
			* 24.0 Mbps
			* 36.0 Mbps
			* 48.0 Mbps
			* 54.0 Mbps
		Frequencies:
			* 2412.0 MHz [1] (30.0 dBm)
			* 2417.0 MHz [2] (30.0 dBm)
			* 2422.0 MHz [3] (30.0 dBm)
			* 2427.0 MHz [4] (30.0 dBm)
			* 2432.0 MHz [5] (30.0 dBm)
			* 2437.0 MHz [6] (30.0 dBm)
			* 2442.0 MHz [7] (30.0 dBm)
			* 2447.0 MHz [8] (30.0 dBm)
			* 2452.0 MHz [9] (30.0 dBm)
			* 2457.0 MHz [10] (30.0 dBm)
			* 2462.0 MHz [11] (30.0 dBm)
			* 2467.0 MHz [12] (disabled)
			* 2472.0 MHz [13] (disabled)
			* 2484.0 MHz [14] (disabled)
	Band 2:
		Capabilities: 0x19ef
			RX LDPC
			HT20/HT40
			SM Power Save disabled
			RX HT20 SGI
			RX HT40 SGI
			TX STBC
			RX STBC 1-stream
			Max AMSDU length: 7935 bytes
			DSSS/CCK HT40
		Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
		Minimum RX AMPDU time spacing: 8 usec (0x06)
		HT TX/RX MCS rate indexes supported: 0-15
		VHT Capabilities (0x339071b2):
			Max MPDU length: 11454
			Supported Channel Width: neither 160 nor 80+80
			RX LDPC
			short GI (80 MHz)
			TX STBC
			SU Beamformee
			MU Beamformee
			RX antenna pattern consistency
			TX antenna pattern consistency
		VHT RX MCS set:
			1 streams: MCS 0-9
			2 streams: MCS 0-9
			3 streams: not supported
			4 streams: not supported
			5 streams: not supported
			6 streams: not supported
			7 streams: not supported
			8 streams: not supported
		VHT RX highest supported: 0 Mbps
		VHT TX MCS set:
			1 streams: MCS 0-9
			2 streams: MCS 0-9
			3 streams: not supported
			4 streams: not supported
			5 streams: not supported
			6 streams: not supported
			7 streams: not supported
			8 streams: not supported
		VHT TX highest supported: 0 Mbps
		VHT extended NSS: not supported
		Bitrates (non-HT):
			* 6.0 Mbps
			* 9.0 Mbps
			* 12.0 Mbps
			* 18.0 Mbps
			* 24.0 Mbps
			* 36.0 Mbps
			* 48.0 Mbps
			* 54.0 Mbps
		Frequencies:
			* 5180.0 MHz [36] (23.0 dBm) (no IR)
			* 5200.0 MHz [40] (23.0 dBm) (no IR)
			* 5220.0 MHz [44] (23.0 dBm) (no IR)
			* 5240.0 MHz [48] (23.0 dBm) (no IR)
			* 5260.0 MHz [52] (24.0 dBm) (no IR, radar detection)
			* 5280.0 MHz [56] (24.0 dBm) (no IR, radar detection)
			* 5300.0 MHz [60] (24.0 dBm) (no IR, radar detection)
			* 5320.0 MHz [64] (24.0 dBm) (no IR, radar detection)
			* 5500.0 MHz [100] (24.0 dBm) (no IR, radar detection)
			* 5520.0 MHz [104] (24.0 dBm) (no IR, radar detection)
			* 5540.0 MHz [108] (24.0 dBm) (no IR, radar detection)
			* 5560.0 MHz [112] (24.0 dBm) (no IR, radar detection)
			* 5580.0 MHz [116] (24.0 dBm) (no IR, radar detection)
			* 5600.0 MHz [120] (24.0 dBm) (no IR, radar detection)
			* 5620.0 MHz [124] (24.0 dBm) (no IR, radar detection)
			* 5640.0 MHz [128] (24.0 dBm) (no IR, radar detection)
			* 5660.0 MHz [132] (24.0 dBm) (no IR, radar detection)
			* 5680.0 MHz [136] (24.0 dBm) (no IR, radar detection)
			* 5700.0 MHz [140] (24.0 dBm) (no IR, radar detection)
			* 5720.0 MHz [144] (24.0 dBm) (no IR, radar detection)
			* 5745.0 MHz [149] (30.0 dBm) (no IR)
			* 5765.0 MHz [153] (30.0 dBm) (no IR)
			* 5785.0 MHz [157] (30.0 dBm) (no IR)
			* 5805.0 MHz [161] (30.0 dBm) (no IR)
			* 5825.0 MHz [165] (30.0 dBm) (no IR)
			* 5845.0 MHz [169] (27.0 dBm) (no IR)
			* 5865.0 MHz [173] (disabled)
	Supported commands:
		 * new_interface
		 * set_interface
		 * new_key
		 * start_ap
		 * new_station
		 * set_bss
		 * authenticate
		 * associate
		 * deauthenticate
		 * disassociate
		 * join_ibss
		 * remain_on_channel
		 * set_tx_bitrate_mask
		 * frame
		 * frame_wait_cancel
		 * set_wiphy_netns
		 * set_channel
		 * set_wds_peer
		 * probe_client
		 * set_noack_map
		 * register_beacons
		 * start_p2p_device
		 * set_mcast_rate
		 * testmode
		 * connect
		 * disconnect
		 * channel_switch
		 * set_qos_map
		 * set_multicast_to_unicast
	WoWLAN support:
		 * wake up on disconnect
		 * wake up on magic packet
		 * wake up on pattern match, up to 22 patterns of 1-134 bytes,
		   maximum packet offset 114 bytes
		 * wake up on network detection, up to 16 match sets
	software interface modes (can always be added):
		 * monitor
	valid interface combinations:
		 * #{ managed } <= 2, #{ AP, P2P-client, P2P-GO } <= 2, #{ P2P-device } <= 1,
		   total <= 4, #channels <= 1
		 * #{ managed } <= 2, #{ P2P-client } <= 2, #{ AP, P2P-GO } <= 1, #{ P2P-device } <= 1,
		   total <= 4, #channels <= 2
		 * #{ managed } <= 1, #{ IBSS } <= 1,
		   total <= 2, #channels <= 1
	HT Capability overrides:
		 * MCS: ff ff ff ff ff ff ff ff ff ff
		 * maximum A-MSDU length
		 * supported channel width
		 * short GI for 40 MHz
		 * max A-MPDU length exponent
		 * min MPDU start spacing
	Device supports TX status socket option.
	Device supports HT-IBSS.
	Device supports SAE with AUTHENTICATE command
	Device supports scan flush.
	Device supports AP scan.
	Device supports per-vif TX power setting
	Driver supports full state transitions for AP/GO clients
	Driver supports a userspace MPM
	Driver/device bandwidth changes during BSS lifetime (AP/GO mode)
	Device supports static SMPS
	Device supports configuring vdev MAC-addr on create.
	Device supports randomizing MAC-addr in scans.
	Device supports randomizing MAC-addr in net-detect scans.
	max # scan plans: 2
	max scan plan interval: 7200
	max scan plan iterations: 100
	Supported TX frame types:
		 * IBSS: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * managed: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * AP: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * AP/VLAN: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * mesh point: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * P2P-client: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * P2P-GO: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
		 * P2P-device: 0x00 0x10 0x20 0x30 0x40 0x50 0x60 0x70 0x80 0x90 0xa0 0xb0 0xc0 0xd0 0xe0 0xf0
	Supported RX frame types:
		 * IBSS: 0x40 0xb0 0xc0 0xd0
		 * managed: 0x40 0xb0 0xd0
		 * AP: 0x00 0x20 0x40 0xa0 0xb0 0xc0 0xd0
		 * AP/VLAN: 0x00 0x20 0x40 0xa0 0xb0 0xc0 0xd0
		 * mesh point: 0xb0 0xc0 0xd0
		 * P2P-client: 0x40 0xd0
		 * P2P-GO: 0x00 0x20 0x40 0xa0 0xb0 0xc0 0xd0
		 * P2P-device: 0x40 0xd0
	Maximum associated stations in AP mode: 32
	Supported extended features:
		* [ VHT_IBSS ]: VHT-IBSS
		* [ RRM ]: RRM
		* [ SET_SCAN_DWELL ]: scan dwell setting
		* [ FILS_STA ]: STA FILS (Fast Initial Link Setup)
		* [ CQM_RSSI_LIST ]: multiple CQM_RSSI_THOLD records
		* [ CONTROL_PORT_OVER_NL80211 ]: control port over nl80211
		* [ TXQS ]: FQ-CoDel-enabled intermediate TXQs
		* [ AIRTIME_FAIRNESS ]: airtime fairness scheduling
		* [ AQL ]: Airtime Queue Limits (AQL)
		* [ CONTROL_PORT_NO_PREAUTH ]: disable pre-auth over nl80211 control port support
		* [ DEL_IBSS_STA ]: deletion of IBSS station support
		* [ SCAN_FREQ_KHZ ]: scan on kHz frequency support
		* [ CONTROL_PORT_OVER_NL80211_TX_STATUS ]: tx status for nl80211 control port support
